smartctl 7.2 2020-12-30 r5155 [FreeBSD 12.2-RELEASE-p7 amd64] (local build)
Copyright (C) 2002-20, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Device Model:     ADATA SU700
Serial Number:    --
LU WWN Device Id: 5 707c18 ...
Firmware Version: B170428a
User Capacity:    240,057,409,536 bytes [240 GB]
Sector Size:      512 bytes logical/physical
Rotation Rate:    Solid State Device
Form Factor:      2.5 inches
TRIM Command:     Available, deterministic, zeroed
Device is:        Not in smartctl database [for details use: -P showall]
ATA Version is:   ACS-2 (minor revision not indicated)
SATA Version is:  SATA 3.2, 6.0 Gb/s (current: 6.0 Gb/s)
Local Time is:    Wed Jun 30 19:45:08 2021 EEST
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Unavailable
APM feature is:   Unavailable
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, frozen [SEC2]
Wt Cache Reorder: Enabled

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x04)	Offline data collection activity
					was suspended by an interrupting command from host.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(   33) seconds.
Offline data collection
capabilities: 			 (0x7b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   1) minutes.
Extended self-test routine
recommended polling time: 	 (   1) minutes.
Conveyance self-test routine
recommended polling time: 	 (   1) minutes.
SCT capabilities: 	       (0x0039)	SCT Status supported.
					SCT Error Recovery Control supported.
					SCT Feature Control supported.
					SCT Data Table supported.

SMART Attributes Data Structure revision number: 0
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  9 Power_On_Hours          -O--C-   100   100   000    -    2736
 12 Power_Cycle_Count       -O--C-   100   100   000    -    573
167 Unknown_Attribute       -O---K   100   100   000    -    0
168 Unknown_Attribute       -O--C-   100   100   000    -    20
169 Unknown_Attribute       PO--C-   100   100   010    -    135
173 Unknown_Attribute       -O--C-   200   200   000    -    64434143271
175 Program_Fail_Count_Chip PO--C-   042   100   010    -    0
180 Unused_Rsvd_Blk_Cnt_Tot PO--CK   100   100   020    -    912
192 Power-Off_Retract_Count -O--C-   100   100   000    -    54
194 Temperature_Celsius     -O---K   062   062   030    -    38 (Min/Max 37/40)
231 Unknown_SSD_Attribute   PO--CK   099   099   005    -    1
233 Media_Wearout_Indicator -O--CK   100   100   000    -    10313334016
234 Unknown_Attribute       -O--CK   100   100   000    -    2596600381440
241 Total_LBAs_Written      -O--CK   100   100   000    -    9284228765
242 Total_LBAs_Read         -O--CK   100   100   000    -    8001451141
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory Version 1
SMART           Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00       GPL,SL  R/O      1  Log Directory
0x01           SL  R/O      1  Summary SMART error log
0x02           SL  R/O     51  Comprehensive SMART error log
0x03       GPL     R/O     64  Ext. Comprehensive SMART error log
0x06           SL  R/O      1  SMART self-test log
0x07       GPL     R/O      1  Extended self-test log
0x09           SL  R/W      1  Selective self-test log
0x10       GPL     R/O      1  NCQ Command Error log
0x11       GPL     R/O      1  SATA Phy Event Counters log
0x30       GPL,SL  R/O      9  IDENTIFY DEVICE data log
0x80-0x9f  GPL,SL  R/W     16  Host vendor specific log
0xe0       GPL,SL  R/W      1  SCT Command/Status
0xe1       GPL,SL  R/W      1  SCT Data Transfer

SMART Extended Comprehensive Error Log Version: 1 (64 sectors)
Device Error Count: 9113 (device log contains only the most recent 256 errors)
	CR     = Command Register
	FEATR  = Features Register
	COUNT  = Count (was: Sector Count) Register
	LBA_48 = Upper bytes of LBA High/Mid/Low Registers ]  ATA-8
	LH     = LBA High (was: Cylinder High) Register    ]   LBA
	LM     = LBA Mid (was: Cylinder Low) Register      ] Register
	LL     = LBA Low (was: Sector Number) Register     ]
	DV     = Device (was: Device/Head) Register
	DC     = Device Control Register
	ER     = Error register
	ST     = Status register
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 9113 [152] occurred at disk power-on lifetime: 251 hours (10 days + 11 hours)
  When the command that caused the error occurred, the device was in a reserved state.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  00 -- 02 00 00 00 5a ef fb e0 40 08 00

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  00 00 00 00 00 00 00 00 00 00 00 00 00 33d+00:24:13.123  NOP [Abort queued commands]
  00 fb f2 00 00 41 76 00 1f e6 40 51 d4     00:00:00.000  NOP [Reserved subcommand] [OBS-ACS-2]
  00 78 d8 41 1f 08 fb 34 00 ca c8 00 00 38d+21:15:11.094  NOP [Reserved subcommand] [OBS-ACS-2]
  e0 fb 5a 08 00 40 00 00 00 00 02 ef e0     00:08:44.539  STANDBY IMMEDIATE
  00 00 00 40 00 08 fb e0 00 5a c6 aa 10 46d+10:59:08.928  NOP [Abort queued commands]

Error 9112 [151] occurred at disk power-on lifetime: 0 hours (0 days + 0 hours)
  When the command that caused the error occurred, the device was in an unknown state.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  00 -- 00 00 00 00 00 00 00 00 00 00 00

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  00 43 03 00 08 00 00 00 00 00 00 00 00     00:00:00.000  NOP [Reserved subcommand] [OBS-ACS-2]
  00 74 e0 46 41 00 f6 2c 00 e1 c8 40 00 15d+18:45:58.773  NOP [Reserved subcommand] [OBS-ACS-2]
  c8 f6 e0 08 00 46 74 00 41 e0 00 c8 00     00:08:44.534  READ DMA
  00 74 e0 46 41 08 f6 9c 00 df c8 00 00 38d+21:20:47.476  NOP [Reserved subcommand] [OBS-ACS-2]

Error 9111 [150] occurred at disk power-on lifetime: 8 hours (0 days + 8 hours)
  When the command that caused the error occurred, the device was in an unknown state.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  00 -- 00 00 00 00 00 00 00 00 00 00 00

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  75 46 41 c8 c8 00 00 f6 40 00 e0 ce 74     00:00:20.806  SEEK [RET-4]
  f6 08 00 00 00 00 46 74 c8 41 e0 e0 f6 43d+11:54:56.392  SECURITY DISABLE PASSWORD
  74 46 41 38 c8 00 08 f6 00 00 df e0 74 43d+10:06:34.054  SEEK [RET-4]
  f6 08 08 00 02 c0 40 00 ef 00 00 d9 43 43d+11:54:56.392  SECURITY DISABLE PASSWORD
  00 00 00 00 00 00 00 00 00 00 00 00 00     13:58:51.648  NOP [Abort queued commands]

Error 9110 [149] occurred at disk power-on lifetime: 0 hours (0 days + 0 hours)
  When the command that caused the error occurred, the device was sleeping.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  00 -- 00 e0 00 df c8 41 9c 46 74 f6 08

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  46 c0 ef f6 d9 74 00 08 e0 00 00 41 40     04:29:39.000  [RESERVED]
  08 00 aa 00 00 f6 c0 40 d9 ef 00 00 08     00:00:00.000  DEVICE RESET
  00 00 00 00 00 00 00 00 00 00 00 00 00  1d+14:30:09.408  NOP [Abort queued commands]
  46 9c c8 f6 df 75 00 00 ce 40 00 41 46     00:00:00.000  [RESERVED]
  08 00 00 74 e0 f6 38 46 df c8 41 00 08 12d+17:02:58.560  DEVICE RESET

Error 9109 [148] occurred at disk power-on lifetime: 246 hours (10 days + 6 hours)
  When the command that caused the error occurred, the device was in a reserved state.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  00 -- aa 00 00 00 d9 ec f6 c0 40 08 01  Device Fault

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  00 00 00 00 00 00 00 00 00 00 00 00 00     00:08:46.403  NOP [Abort queued commands]
  00 f6 df 00 00 46 75 00 41 ce 40 51 38     00:00:00.000  NOP [Reserved subcommand] [OBS-ACS-2]
  00 00 00 40 00 08 f6 c0 00 d9 ef 00 00 38d+21:20:47.476  NOP [Abort queued commands]
  c0 f6 d9 08 00 40 00 00 00 00 aa ef c0     09:27:58.966  CFA ERASE SECTORS [VS IF NO CFA]
  01 00 00 40 00 08 f6 c0 00 d9 c6 00 10 45d+21:00:17.280  [RESERVED]

Error 9108 [147] occurred at disk power-on lifetime: 0 hours (0 days + 0 hours)
  When the command that caused the error occurred, the device was in an unknown state.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  00 -- 00 00 00 00 00 00 00 00 00 00 00

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  00 43 03 00 08 00 00 00 00 00 00 00 00     00:00:00.000  NOP [Reserved subcommand] [OBS-ACS-2]
  00 76 d8 41 1f 00 fb 2c 00 f5 c8 40 00 15d+18:40:22.390  NOP [Reserved subcommand] [OBS-ACS-2]
  64 fb f4 08 00 41 76 00 1f d8 00 c8 00     00:08:44.539  SEND FPDMA QUEUED
  00 76 d8 41 1f 08 fb 9c 00 f3 c8 00 00 38d+21:15:11.094  NOP [Reserved subcommand] [OBS-ACS-2]

Error 9107 [146] occurred at disk power-on lifetime: 8 hours (0 days + 8 hours)
  When the command that caused the error occurred, the device was in an unknown state.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  00 -- 00 00 00 00 00 00 00 00 00 00 00

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  76 41 1f 64 c8 00 00 fb 40 00 f4 e6 76     00:00:20.801  SEEK [RET-4]
  fb 08 00 00 00 00 41 76 c8 1f d8 f4 fb 41d+22:37:58.664  [VENDOR SPECIFIC]
  76 41 1f d4 c8 00 08 fb 00 00 f2 d8 76 47d+07:18:58.369  SEEK [RET-4]
  fb 08 08 00 00 34 41 78 c8 1f d8 ca 43 41d+22:37:58.664  [VENDOR SPECIFIC]
  00 00 00 00 00 00 00 00 00 00 00 00 00     13:58:51.648  NOP [Abort queued commands]

Error 9106 [145] occurred at disk power-on lifetime: 0 hours (0 days + 0 hours)
  When the command that caused the error occurred, the device was sleeping.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  00 -- 00 d8 00 f3 c8 1f 9c 41 76 fb 08   at LBA = 0xf3c81f9c4176 = 268040849342838

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  41 34 c8 fb ca 76 00 08 d8 00 00 1f 41     04:35:11.700  READ VERIFY SECTOR(S) (w/o retry) [OBS-5]
  08 00 02 00 00 fb e0 40 5a ef 00 00 08  6d+02:40:13.312  DEVICE RESET
  00 00 00 00 00 00 00 00 00 00 00 00 00  1d+14:30:09.408  NOP [Abort queued commands]
  41 9c c8 fb f3 76 00 00 e6 40 00 1f 41     00:00:00.000  READ VERIFY SECTOR(S) (w/o retry) [OBS-5]
  08 00 00 76 d8 fb d4 41 f2 c8 1f 00 08  6d+02:38:02.240  DEVICE RESET

SMART Extended Self-test Log Version: 1 (1 sectors)
No self-tests have been logged.  [To run self-tests, use: smartctl -t]

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Status Version:                  3
SCT Version (vendor specific):       1 (0x0001)
Device State:                        Active (0)
Current Temperature:                     ? Celsius
Power Cycle Min/Max Temperature:      ?/ ? Celsius
Lifetime    Min/Max Temperature:      ?/ ? Celsius
Under/Over Temperature Limit Count:   0/0

SCT Temperature History Version:     2
Temperature Sampling Period:         1 minute
Temperature Logging Interval:        1 minute
Min/Max recommended Temperature:     -127/127 Celsius
Min/Max Temperature Limit:           -127/127 Celsius
Temperature History Size (Index):    478 (103)

SCT Error Recovery Control:
           Read:     80 (8.0 seconds)
          Write:     80 (8.0 seconds)

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11)
ID      Size     Value  Description
0x0001  2           20  Command failed due to ICRC error
0x0003  2            0  R_ERR response for device-to-host data FIS
0x0004  2            0  R_ERR response for host-to-device data FIS
0x0006  2            0  R_ERR response for device-to-host non-data FIS
0x0007  2            0  R_ERR response for host-to-device non-data FIS
0x0008  2            0  Device-to-host non-data FIS retries
0x0009  4            0  Transition from drive PhyRdy to drive PhyNRdy
0x000a  4           12  Device-to-host register FISes sent due to a COMRESET
0x000f  2            0  R_ERR response for host-to-device data FIS, CRC
0x0010  2            0  R_ERR response for host-to-device data FIS, non-CRC
0x0012  2            0  R_ERR response for host-to-device non-data FIS, CRC
0x0013  2            0  R_ERR response for host-to-device non-data FIS, non-CRC



