smartctl 7.1 2019-12-30 r5022 [FreeBSD 12.1-RELEASE amd64] (local build)
Copyright (C) 2002-19, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Seagate Momentus 5400.6
Device Model:     ST9320325AS
Serial Number:    --
LU WWN Device Id: 5 000c50 ...
Firmware Version: 0002SDM1
User Capacity:    320,072,933,376 bytes [320 GB]
Sector Size:      512 bytes logical/physical
Rotation Rate:    5400 rpm
Device is:        In smartctl database [for details use: -P show]
ATA Version is:   ATA8-ACS T13/1699-D revision 4
SATA Version is:  SATA 2.6, 3.0 Gb/s
Local Time is:    Wed Jan 27 11:38:36 2021 EST
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Unavailable
APM level is:     128 (minimum power consumption without standby)
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, NOT FROZEN [SEC1]
Wt Cache Reorder: Unknown

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x00)	Offline data collection activity
					was never started.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(    0) seconds.
Offline data collection
capabilities: 			 (0x73) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					No Offline surface scan supported.
					Self-test supported.
					Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   1) minutes.
Extended self-test routine
recommended polling time: 	 (  99) minutes.
Conveyance self-test routine
recommended polling time: 	 (   2) minutes.
SCT capabilities: 	       (0x103b)	SCT Status supported.
					SCT Error Recovery Control supported.
					SCT Feature Control supported.
					SCT Data Table supported.

SMART Attributes Data Structure revision number: 10
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     POSR--   114   099   006    -    76620297
  3 Spin_Up_Time            PO----   099   099   000    -    0
  4 Start_Stop_Count        -O--CK   090   090   020    -    10372
  5 Reallocated_Sector_Ct   PO--CK   100   100   036    -    1
  7 Seek_Error_Rate         POSR--   084   060   030    -    4576855739
  9 Power_On_Hours          -O--CK   089   088   000    -    9994
 10 Spin_Retry_Count        PO--C-   100   100   097    -    0
 12 Power_Cycle_Count       -O--CK   090   037   020    -    10312
184 End-to-End_Error        -O--CK   100   100   099    -    0
187 Reported_Uncorrect      -O--CK   090   090   000    -    10
188 Command_Timeout         -O--CK   100   083   000    -    17180133379
189 High_Fly_Writes         -O-RCK   100   100   000    -    0
190 Airflow_Temperature_Cel -O---K   070   052   045    -    30 (Min/Max 14/30)
191 G-Sense_Error_Rate      -O--CK   100   100   000    -    316
192 Power-Off_Retract_Count -O--CK   100   100   000    -    999
193 Load_Cycle_Count        -O--CK   001   001   000    -    230500
194 Temperature_Celsius     -O---K   030   048   000    -    30 (0 4 0 0 0)
195 Hardware_ECC_Recovered  -O-RC-   057   043   000    -    76620297
197 Current_Pending_Sector  -O--C-   100   100   000    -    0
198 Offline_Uncorrectable   ----C-   100   100   000    -    0
199 UDMA_CRC_Error_Count    -OSRCK   200   200   000    -    0
254 Free_Fall_Sensor        -O--CK   100   100   000    -    0
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory Version 1
SMART           Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00       GPL,SL  R/O      1  Log Directory
0x01       GPL,SL  R/O      1  Summary SMART error log
0x02       GPL,SL  R/O      5  Comprehensive SMART error log
0x03       GPL,SL  R/O      5  Ext. Comprehensive SMART error log
0x06       GPL,SL  R/O      1  SMART self-test log
0x07       GPL,SL  R/O      1  Extended self-test log
0x09       GPL,SL  R/W      1  Selective self-test log
0x10       GPL,SL  R/O      1  NCQ Command Error log
0x11       GPL,SL  R/O      1  SATA Phy Event Counters log
0x21       GPL,SL  R/O      1  Write stream error log
0x22       GPL,SL  R/O      1  Read stream error log
0x80-0x9f  GPL,SL  R/W     16  Host vendor specific log
0xa1       GPL,SL  VS      20  Device vendor specific log
0xa2       GPL     VS    2248  Device vendor specific log
0xa8       GPL,SL  VS      65  Device vendor specific log
0xa9       GPL,SL  VS       1  Device vendor specific log
0xb0       GPL     VS    2864  Device vendor specific log
0xbe-0xbf  GPL     VS   65535  Device vendor specific log
0xe0       GPL,SL  R/W      1  SCT Command/Status
0xe1       GPL,SL  R/W      1  SCT Data Transfer

SMART Extended Comprehensive Error Log Version: 1 (5 sectors)
Device Error Count: 10
	CR     = Command Register
	FEATR  = Features Register
	COUNT  = Count (was: Sector Count) Register
	LBA_48 = Upper bytes of LBA High/Mid/Low Registers ]  ATA-8
	LH     = LBA High (was: Cylinder High) Register    ]   LBA
	LM     = LBA Mid (was: Cylinder Low) Register      ] Register
	LL     = LBA Low (was: Sector Number) Register     ]
	DV     = Device (was: Device/Head) Register
	DC     = Device Control Register
	ER     = Error register
	ST     = Status register
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 10 [9] occurred at disk power-on lifetime: 8952 hours (373 days + 0 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 03 27 3f 8b 00 00  Error: UNC at LBA = 0x03273f8b = 52903819

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 00 20 00 00 00 c9 c5 25 40 00     00:02:03.242  READ FPDMA QUEUED
  60 00 00 00 20 00 00 00 c9 c5 05 40 00     00:02:03.240  READ FPDMA QUEUED
  60 00 00 00 08 00 00 00 47 91 f8 40 00     00:02:03.234  READ FPDMA QUEUED
  60 00 00 00 08 00 00 01 b8 e8 30 40 00     00:02:03.229  READ FPDMA QUEUED
  60 00 00 00 20 00 00 00 c9 c4 e5 40 00     00:02:03.222  READ FPDMA QUEUED

Error 9 [8] occurred at disk power-on lifetime: 8952 hours (373 days + 0 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 03 27 3f 8b 00 00  Error: UNC at LBA = 0x03273f8b = 52903819

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 00 08 00 00 00 6e 4b f8 40 00     00:02:00.655  READ FPDMA QUEUED
  60 00 00 00 40 00 00 00 2f e0 78 40 00     00:02:00.648  READ FPDMA QUEUED
  60 00 00 00 20 00 00 00 c9 c3 c5 40 00     00:02:00.645  READ FPDMA QUEUED
  60 00 00 00 20 00 00 00 c9 c3 a5 40 00     00:02:00.644  READ FPDMA QUEUED
  60 00 00 00 20 00 00 00 c9 c3 85 40 00     00:02:00.644  READ FPDMA QUEUED

Error 8 [7] occurred at disk power-on lifetime: 8952 hours (373 days + 0 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 03 27 3f 8b 00 00  Error: UNC at LBA = 0x03273f8b = 52903819

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 00 38 00 00 00 43 34 5c 40 00     00:01:57.627  READ FPDMA QUEUED
  60 00 00 00 08 00 00 01 b8 51 00 40 00     00:01:57.624  READ FPDMA QUEUED
  60 00 00 00 08 00 00 00 04 8c b0 40 00     00:01:57.599  READ FPDMA QUEUED
  61 00 00 00 08 00 00 06 76 49 a0 40 00     00:01:57.584  WRITE FPDMA QUEUED
  61 00 00 00 08 00 00 06 76 49 a8 40 00     00:01:57.583  WRITE FPDMA QUEUED

Error 7 [6] occurred at disk power-on lifetime: 8952 hours (373 days + 0 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 03 27 3f 8b 00 00  Error: UNC at LBA = 0x03273f8b = 52903819

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 00 28 00 00 00 0b 6e 3a 40 00     00:01:55.135  READ FPDMA QUEUED
  60 00 00 00 40 00 00 00 0b 6e 62 40 00     00:01:55.134  READ FPDMA QUEUED
  61 00 00 00 28 00 00 00 64 0a d8 40 00     00:01:55.074  WRITE FPDMA QUEUED
  61 00 00 00 08 00 00 00 64 0a b0 40 00     00:01:55.074  WRITE FPDMA QUEUED
  61 00 00 00 08 00 00 00 63 d6 38 40 00     00:01:55.073  WRITE FPDMA QUEUED

Error 6 [5] occurred at disk power-on lifetime: 8952 hours (373 days + 0 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 03 27 3f 8b 00 00  Error: WP at LBA = 0x03273f8b = 52903819

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 00 00 00 08 00 00 00 63 d1 18 40 00     00:01:52.526  WRITE FPDMA QUEUED
  61 00 00 00 08 00 00 00 63 b9 60 40 00     00:01:52.525  WRITE FPDMA QUEUED
  61 00 00 00 10 00 00 00 63 b9 40 40 00     00:01:52.525  WRITE FPDMA QUEUED
  61 00 00 00 08 00 00 00 63 b9 28 40 00     00:01:52.524  WRITE FPDMA QUEUED
  61 00 00 00 08 00 00 00 63 b4 c0 40 00     00:01:52.524  WRITE FPDMA QUEUED

Error 5 [4] occurred at disk power-on lifetime: 8952 hours (373 days + 0 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 03 27 3f 8b 00 00  Error: UNC at LBA = 0x03273f8b = 52903819

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 00 40 00 00 00 0b 6d fa 40 00     00:01:49.959  READ FPDMA QUEUED
  60 00 00 00 28 00 00 00 22 88 42 40 00     00:01:49.950  READ FPDMA QUEUED
  60 00 00 00 40 00 00 00 22 88 6a 40 00     00:01:49.933  READ FPDMA QUEUED
  60 00 00 00 40 00 00 00 0e 11 da 40 00     00:01:49.926  READ FPDMA QUEUED
  60 00 00 00 1e 00 00 00 03 36 f8 40 00     00:01:49.912  READ FPDMA QUEUED

Error 4 [3] occurred at disk power-on lifetime: 8952 hours (373 days + 0 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 03 27 3f 8b 00 00  Error: UNC at LBA = 0x03273f8b = 52903819

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 00 40 00 00 00 43 3d 44 40 00     00:01:47.339  READ FPDMA QUEUED
  60 00 00 00 40 00 00 00 0e 12 72 40 00     00:01:47.295  READ FPDMA QUEUED
  61 00 00 00 08 00 00 00 63 aa b0 40 00     00:01:47.288  WRITE FPDMA QUEUED
  61 00 00 00 08 00 00 00 63 aa 78 40 00     00:01:47.287  WRITE FPDMA QUEUED
  61 00 00 00 08 00 00 00 63 aa 50 40 00     00:01:47.287  WRITE FPDMA QUEUED

Error 3 [2] occurred at disk power-on lifetime: 8952 hours (373 days + 0 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 03 27 3f 8b 00 00  Error: WP at LBA = 0x03273f8b = 52903819

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 00 00 00 0c 00 00 00 0a 4c 78 40 00     00:01:44.701  WRITE FPDMA QUEUED
  61 00 00 00 20 00 00 03 67 5b 60 40 00     00:01:44.701  WRITE FPDMA QUEUED
  61 00 00 00 20 00 00 03 6d c0 a0 40 00     00:01:44.700  WRITE FPDMA QUEUED
  61 00 00 00 10 00 00 00 63 a7 e8 40 00     00:01:44.691  WRITE FPDMA QUEUED
  61 00 00 00 08 00 00 00 63 8b e0 40 00     00:01:44.690  WRITE FPDMA QUEUED

SMART Extended Self-test Log Version: 1 (1 sectors)
Num  Test_Description    Status                  Remaining  LifeTime(hours)  LBA_of_first_error
# 1  Short offline       Completed without error       00%      9967         -
# 2  Short offline       Completed without error       00%      9955         -
# 3  Short offline       Completed without error       00%      9639         -
# 4  Short offline       Aborted by host               90%      3692         -
# 5  Short offline       Completed without error       00%      9527         -
# 6  Short offline       Completed without error       00%      7778         -
# 7  Extended offline    Aborted by host               90%      7778         -
# 8  Short offline       Completed without error       00%        15         -

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Status Version:                  3
SCT Version (vendor specific):       522 (0x020a)
Device State:                        Active (0)
Current Temperature:                    30 Celsius
Power Cycle Min/Max Temperature:     14/30 Celsius
Lifetime    Min/Max Temperature:      4/48 Celsius
Under/Over Temperature Limit Count:   0/22

SCT Temperature History Version:     2
Temperature Sampling Period:         1 minute
Temperature Logging Interval:        1 minute
Min/Max recommended Temperature:      0/ 0 Celsius
Min/Max Temperature Limit:            0/ 0 Celsius
Temperature History Size (Index):    128 (19)

SCT Error Recovery Control:
           Read: Disabled
          Write: Disabled

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11)
ID      Size     Value  Description
0x000a  2            5  Device-to-host register FISes sent due to a COMRESET
0x0001  2            0  Command failed due to ICRC error
0x0003  2            0  R_ERR response for device-to-host data FIS
0x0004  2            0  R_ERR response for host-to-device data FIS
0x0006  2            0  R_ERR response for device-to-host non-data FIS
0x0007  2            0  R_ERR response for host-to-device non-data FIS

