smartctl 7.2 2020-12-30 r5155 [FreeBSD 12.1-RELEASE-p16-HBSD amd64] (local build)
Copyright (C) 2002-20, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Number:                       SAMSUNG MZVPW256HEGL-00000
Serial Number:                      --
Firmware Version:                   CXZ7500Q
PCI Vendor/Subsystem ID:            0x144d
IEEE OUI Identifier:                0x002538
Total NVM Capacity:                 256,060,514,304 [256 GB]
Unallocated NVM Capacity:           0
Controller ID:                      2
NVMe Version:                       1.2
Number of Namespaces:               1
Namespace 1 Size/Capacity:          256,060,514,304 [256 GB]
Namespace 1 Formatted LBA Size:     512
Namespace 1 IEEE EUI-64:            002538 ...
Local Time is:                      Sun May  2 20:42:38 2021 CEST
Firmware Updates (0x16):            3 Slots, no Reset required
Optional Admin Commands (0x0017):   Security Format Frmw_DL Self_Test
Optional NVM Commands (0x001f):     Comp Wr_Unc DS_Mngmt Wr_Zero Sav/Sel_Feat
Log Page Attributes (0x03):         S/H_per_NS Cmd_Eff_Lg
Warning  Comp. Temp. Threshold:     70 Celsius
Critical Comp. Temp. Threshold:     73 Celsius

Supported Power States
St Op     Max   Active     Idle   RL RT WL WT  Ent_Lat  Ex_Lat
 0 +     6.80W       -        -    0  0  0  0        0       0
 1 +     5.60W       -        -    1  1  1  1        0       0
 2 +     4.40W       -        -    2  2  2  2        0       0
 3 -   0.0400W       -        -    3  3  3  3      210    1500
 4 -   0.0050W       -        -    4  4  4  4     2200    6000

Supported LBA Sizes (NSID 0x1)
Id Fmt  Data  Metadt  Rel_Perf
 0 +     512       0         0

=== START OF SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

SMART/Health Information (NVMe Log 0x02)
Critical Warning:                   0x00
Temperature:                        40 Celsius
Available Spare:                    100%
Available Spare Threshold:          10%
Percentage Used:                    1%
Data Units Read:                    8,320,778 [4.26 TB]
Data Units Written:                 11,464,852 [5.87 TB]
Host Read Commands:                 93,932,765
Host Write Commands:                165,975,218
Controller Busy Time:               1,093
Power Cycles:                       754
Power On Hours:                     725
Unsafe Shutdowns:                   76
Media and Data Integrity Errors:    0
Error Information Log Entries:      442
Warning  Comp. Temperature Time:    0
Critical Comp. Temperature Time:    0
Temperature Sensor 1:               40 Celsius
Temperature Sensor 2:               65 Celsius

Error Information (NVMe Log 0x01, 16 of 64 entries)
Num   ErrCount  SQId   CmdId  Status  PELoc          LBA  NSID    VS
  0        442     0  0x0029  0x4202  0x028            0     0     -
  1        441     0  0x0028  0x4202  0x028            0     0     -
  2        440     0  0x001f  0x4004  0x02c            0     0     -
  3        439     0  0x001e  0x4004  0x02c            0     0     -
  4        438     0  0x001d  0x4202  0x028            0     0     -
  5        437     0  0x0002  0x4004  0x028            0     0     -
  6        436     0  0x0029  0x4202  0x028            0     0     -
  7        435     0  0x0028  0x4202  0x028            0     0     -
  8        434     0  0x001f  0x4004  0x02c            0     0     -
  9        433     0  0x001e  0x4004  0x02c            0     0     -
 10        432     0  0x001d  0x4202  0x028            0     0     -
 11        431     0  0x0002  0x4004  0x028            0     0     -
 12        430     0  0x0029  0x4202  0x028            0     0     -
 13        429     0  0x0028  0x4202  0x028            0     0     -
 14        428     0  0x001f  0x4004  0x02c            0     0     -
 15        427     0  0x001e  0x4004  0x02c            0     0     -
... (48 entries not read)

