smartctl 7.1 2019-12-30 r5022 [FreeBSD 12.1-RELEASE amd64] (local build)
Copyright (C) 2002-19, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     SAMSUNG SpinPoint F1 DT
Device Model:     SAMSUNG HD252HJ
Serial Number:    --
LU WWN Device Id: 5 0000f0 ...
Firmware Version: 1AC01113
User Capacity:    250,059,350,016 bytes [250 GB]
Sector Size:      512 bytes logical/physical
Device is:        In smartctl database [for details use: -P show]
ATA Version is:   ATA/ATAPI-7, ATA8-ACS T13/1699-D revision 3b
Local Time is:    Wed Feb 10 19:06:47 2021 EST
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Disabled
APM level is:     254 (maximum performance)
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, frozen [SEC2]
Wt Cache Reorder: Enabled

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED
See vendor-specific Attribute list for marginal Attributes.

General SMART Values:
Offline data collection status:  (0x00)	Offline data collection activity
					was never started.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		( 3832) seconds.
Offline data collection
capabilities: 			 (0x7b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   2) minutes.
Extended self-test routine
recommended polling time: 	 (  65) minutes.
Conveyance self-test routine
recommended polling time: 	 (   8) minutes.
SCT capabilities: 	       (0x003f)	SCT Status supported.
					SCT Error Recovery Control supported.
					SCT Feature Control supported.
					SCT Data Table supported.

SMART Attributes Data Structure revision number: 16
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     POSR--   099   002   051    Past 10870
  3 Spin_Up_Time            POS---   093   093   011    -    2970
  4 Start_Stop_Count        -O--CK   096   096   000    -    3665
  5 Reallocated_Sector_Ct   PO--CK   100   100   010    -    0
  7 Seek_Error_Rate         POSR--   100   100   051    -    0
  8 Seek_Time_Performance   P-S--K   100   100   015    -    0
  9 Power_On_Hours          -O--CK   099   099   000    -    4170
 10 Spin_Retry_Count        PO--CK   100   100   051    -    0
 11 Calibration_Retry_Count -O--C-   100   100   000    -    96
 12 Power_Cycle_Count       -O--CK   097   097   000    -    3269
 13 Read_Soft_Error_Rate    -OSR--   099   005   000    -    10153
183 Runtime_Bad_Block       -O--CK   100   100   000    -    35
184 End-to-End_Error        PO--CK   100   100   000    -    0
187 Reported_Uncorrect      -O--CK   100   100   000    -    28474
188 Command_Timeout         -O--CK   100   100   000    -    0
190 Airflow_Temperature_Cel -O---K   080   056   000    -    20 (Min/Max 13/20)
194 Temperature_Celsius     -O---K   075   053   000    -    25 (Min/Max 13/25)
195 Hardware_ECC_Recovered  -O-RC-   100   100   000    -    4202
196 Reallocated_Event_Count -O--CK   099   099   000    -    30
197 Current_Pending_Sector  -O--C-   089   089   000    -    479
198 Offline_Uncorrectable   ----CK   100   100   000    -    0
199 UDMA_CRC_Error_Count    -OSRCK   100   100   000    -    5
200 Multi_Zone_Error_Rate   -O-R--   099   099   000    -    1679
201 Soft_Read_Error_Rate    -O-R--   253   253   000    -    0
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory Version 1
SMART           Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00       GPL,SL  R/O      1  Log Directory
0x01           SL  R/O      1  Summary SMART error log
0x02           SL  R/O      2  Comprehensive SMART error log
0x03       GPL     R/O      2  Ext. Comprehensive SMART error log
0x04       GPL     R/O      2  Device Statistics log
0x06           SL  R/O      1  SMART self-test log
0x07       GPL     R/O      2  Extended self-test log
0x09           SL  R/W      1  Selective self-test log
0x10       GPL     R/O      1  NCQ Command Error log
0x11       GPL     R/O      1  SATA Phy Event Counters log
0x21       GPL     R/O      2  Write stream error log
0x22       GPL     R/O      2  Read stream error log
0x80-0x9f  GPL,SL  R/W     16  Host vendor specific log
0xe0       GPL,SL  R/W      1  SCT Command/Status
0xe1       GPL,SL  R/W      1  SCT Data Transfer

SMART Extended Comprehensive Error Log Version: 1 (2 sectors)
Device Error Count: 29753 (device log contains only the most recent 8 errors)
	CR     = Command Register
	FEATR  = Features Register
	COUNT  = Count (was: Sector Count) Register
	LBA_48 = Upper bytes of LBA High/Mid/Low Registers ]  ATA-8
	LH     = LBA High (was: Cylinder High) Register    ]   LBA
	LM     = LBA Mid (was: Cylinder Low) Register      ] Register
	LL     = LBA Low (was: Sector Number) Register     ]
	DV     = Device (was: Device/Head) Register
	DC     = Device Control Register
	ER     = Error register
	ST     = Status register
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 29753 [0] occurred at disk power-on lifetime: 1866 hours (77 days + 18 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  00 -- 58 00 06 00 00 00 00 09 3a e0 00   at LBA = 0x0000093a = 2362

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  39 00 00 00 08 00 00 00 00 09 38 e0 00     00:35:46.830  WRITE MULTIPLE EXT
  c6 00 00 00 10 00 00 00 00 00 00 a0 00     00:35:45.910  SET MULTIPLE MODE
  ef 00 03 00 46 00 00 00 00 00 00 a0 00     00:35:45.890  SET FEATURES [Set transfer mode]
  ef 00 03 00 0c 00 00 00 00 00 00 a0 00     00:35:45.880  SET FEATURES [Set transfer mode]
  00 00 00 00 01 00 00 00 00 00 01 a0 00     00:35:45.820  NOP [Abort queued commands]

Error 29752 [7] occurred at disk power-on lifetime: 1866 hours (77 days + 18 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  00 -- 58 00 06 00 00 00 00 09 3a e0 00   6 sectors at LBA = 0x0000093a = 2362

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  35 00 00 00 08 00 00 00 00 09 38 e0 00     00:34:45.350  WRITE DMA EXT
  35 00 00 00 08 00 00 00 01 13 68 e0 00     00:34:45.350  WRITE DMA EXT
  35 00 00 00 08 00 00 00 01 12 d8 e0 00     00:34:45.350  WRITE DMA EXT
  25 00 00 00 08 00 00 00 01 12 d8 e0 00     00:34:45.350  READ DMA EXT
  25 00 00 00 08 00 00 00 00 09 38 e0 00     00:34:45.350  READ DMA EXT

Error 29751 [6] occurred at disk power-on lifetime: 1866 hours (77 days + 18 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  00 -- 58 00 05 00 00 00 00 f7 83 e0 00   at LBA = 0x0000f783 = 63363

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  39 00 00 00 08 00 00 00 00 f7 80 e0 00     00:31:05.050  WRITE MULTIPLE EXT
  29 00 00 00 08 00 00 00 00 f7 88 e0 00     00:31:05.050  READ MULTIPLE EXT
  29 00 00 00 08 00 00 00 00 f7 80 e0 00     00:31:05.040  READ MULTIPLE EXT
  29 00 00 00 08 00 00 00 00 f2 a0 e0 00     00:31:05.030  READ MULTIPLE EXT
  29 00 00 00 08 00 00 00 00 f2 a8 e0 00     00:31:05.030  READ MULTIPLE EXT

Error 29750 [5] occurred at disk power-on lifetime: 1866 hours (77 days + 18 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  00 -- 58 00 07 00 00 00 5e fa e1 e0 00   7 sectors at LBA = 0x005efae1 = 6224609

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  35 00 00 00 08 00 00 00 5e fa e0 e0 00     00:28:31.610  WRITE DMA EXT
  35 00 00 00 08 00 00 00 5e fa f0 e0 00     00:28:31.610  WRITE DMA EXT
  35 00 00 00 08 00 00 00 60 b7 e8 e0 00     00:28:31.610  WRITE DMA EXT
  35 00 00 00 08 00 00 00 00 f2 90 e0 00     00:28:31.610  WRITE DMA EXT
  35 00 00 00 08 00 00 00 00 f2 a0 e0 00     00:28:31.610  WRITE DMA EXT

Error 29749 [4] occurred at disk power-on lifetime: 1689 hours (70 days + 9 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 01 23 d7 ce e1 00  Error: UNC at LBA = 0x0123d7ce = 19126222

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  c8 00 00 00 08 00 00 00 23 d7 c8 e1 00     05:39:46.320  READ DMA
  27 00 00 00 00 00 00 00 00 00 00 e0 00     05:39:46.300  READ NATIVE MAX ADDRESS EXT [OBS-ACS-3]
  ec 00 00 00 00 00 00 00 00 00 00 a0 00     05:39:46.290  IDENTIFY DEVICE
  ef 00 03 00 45 00 00 00 00 00 00 a0 00     05:39:46.290  SET FEATURES [Set transfer mode]
  27 00 00 00 00 00 00 00 00 00 00 e0 00     05:39:46.290  READ NATIVE MAX ADDRESS EXT [OBS-ACS-3]

Error 29748 [3] occurred at disk power-on lifetime: 1689 hours (70 days + 9 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 01 23 d7 ce e1 00  Error: UNC at LBA = 0x0123d7ce = 19126222

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  c8 00 00 00 08 00 00 00 23 d7 c8 e1 00     05:39:44.350  READ DMA
  27 00 00 00 00 00 00 00 00 00 00 e0 00     05:39:43.540  READ NATIVE MAX ADDRESS EXT [OBS-ACS-3]
  ec 00 00 00 00 00 00 00 00 00 00 a0 00     05:39:43.530  IDENTIFY DEVICE
  ef 00 03 00 45 00 00 00 00 00 00 a0 00     05:39:43.530  SET FEATURES [Set transfer mode]
  27 00 00 00 00 00 00 00 00 00 00 e0 00     05:39:43.530  READ NATIVE MAX ADDRESS EXT [OBS-ACS-3]

Error 29747 [2] occurred at disk power-on lifetime: 1689 hours (70 days + 9 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 01 23 d7 ce e1 00  Error: UNC at LBA = 0x0123d7ce = 19126222

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  c8 00 00 00 08 00 00 00 23 d7 c8 e1 00     05:39:41.600  READ DMA
  27 00 00 00 00 00 00 00 00 00 00 e0 00     05:39:41.590  READ NATIVE MAX ADDRESS EXT [OBS-ACS-3]
  ec 00 00 00 00 00 00 00 00 00 00 a0 00     05:39:41.580  IDENTIFY DEVICE
  ef 00 03 00 45 00 00 00 00 00 00 a0 00     05:39:41.580  SET FEATURES [Set transfer mode]
  27 00 00 00 00 00 00 00 00 00 00 e0 00     05:39:41.580  READ NATIVE MAX ADDRESS EXT [OBS-ACS-3]

Error 29746 [1] occurred at disk power-on lifetime: 1689 hours (70 days + 9 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 01 23 d7 ce e1 00  Error: UNC at LBA = 0x0123d7ce = 19126222

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  c8 00 00 00 08 00 00 00 23 d7 c8 e1 00     05:39:39.640  READ DMA
  27 00 00 00 00 00 00 00 00 00 00 e0 00     05:39:38.830  READ NATIVE MAX ADDRESS EXT [OBS-ACS-3]
  ec 00 00 00 00 00 00 00 00 00 00 a0 00     05:39:38.820  IDENTIFY DEVICE
  ef 00 03 00 45 00 00 00 00 00 00 a0 00     05:39:38.820  SET FEATURES [Set transfer mode]
  27 00 00 00 00 00 00 00 00 00 00 e0 00     05:39:38.820  READ NATIVE MAX ADDRESS EXT [OBS-ACS-3]

SMART Extended Self-test Log Version: 1 (2 sectors)
No self-tests have been logged.  [To run self-tests, use: smartctl -t]

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Status Version:                  2
SCT Version (vendor specific):       256 (0x0100)
Device State:                        Active (0)
Current Temperature:                    26 Celsius
Power Cycle Min/Max Temperature:     --/26 Celsius
Lifetime    Min/Max Temperature:     --/60 Celsius

SCT Temperature History Version:     2
Temperature Sampling Period:         1 minute
Temperature Logging Interval:        1 minute
Min/Max recommended Temperature:     -4/72 Celsius
Min/Max Temperature Limit:           -9/77 Celsius
Temperature History Size (Index):    128 (66)

SCT Error Recovery Control:
           Read: Disabled
          Write: Disabled

ATA_READ_LOG_EXT (addr=0x04:0x00, page=0, n=1) failed: Input/output error
Read Device Statistics page 0x00 failed

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11)
ID      Size     Value  Description
0x000a  2            6  Device-to-host register FISes sent due to a COMRESET
0x0001  2            0  Command failed due to ICRC error
0x0002  2            0  R_ERR response for data FIS
0x0003  2            0  R_ERR response for device-to-host data FIS
0x0004  2            0  R_ERR response for host-to-device data FIS
0x0005  2            0  R_ERR response for non-data FIS
0x0006  2            0  R_ERR response for device-to-host non-data FIS
0x0007  2            0  R_ERR response for host-to-device non-data FIS
0x0008  2            0  Device-to-host non-data FIS retries
0x0009  2            6  Transition from drive PhyRdy to drive PhyNRdy
0x000b  2            0  CRC errors within host-to-device FIS
0x000d  2            0  Non-CRC errors within host-to-device FIS
0x000f  2            0  R_ERR response for host-to-device data FIS, CRC
0x0010  2            0  R_ERR response for host-to-device data FIS, non-CRC
0x0012  2            0  R_ERR response for host-to-device non-data FIS, CRC
0x0013  2            0  R_ERR response for host-to-device non-data FIS, non-CRC



