smartctl 7.2 2021-09-14 r5236 [FreeBSD 13.0-STABLE amd64] (local build)
Copyright (C) 2002-20, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Western Digital Caviar Blue Serial ATA
Device Model:     WDC WD2500AAJS-60B4A0
Serial Number:    --
LU WWN Device Id: 5 0014ee ...
Firmware Version: 02.03A02
User Capacity:    250,059,350,016 bytes [250 GB]
Sector Size:      512 bytes logical/physical
Device is:        In smartctl database [for details use: -P show]
ATA Version is:   ATA8-ACS (minor revision not indicated)
SATA Version is:  SATA 2.5, 3.0 Gb/s
Local Time is:    Tue Mar 22 23:03:58 2022 CET
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Unavailable
APM feature is:   Unavailable
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, frozen [SEC2]
Wt Cache Reorder: Enabled

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x82)	Offline data collection activity
					was completed without error.
					Auto Offline Data Collection: Enabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		( 5400) seconds.
Offline data collection
capabilities: 			 (0x5b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					No Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   2) minutes.
Extended self-test routine
recommended polling time: 	 (  66) minutes.
SCT capabilities: 	       (0x303f)	SCT Status supported.
					SCT Error Recovery Control supported.
					SCT Feature Control supported.
					SCT Data Table supported.

SMART Attributes Data Structure revision number: 16
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     POSR-K   200   200   051    -    0
  3 Spin_Up_Time            POS--K   155   154   021    -    3208
  4 Start_Stop_Count        -O--CK   089   089   000    -    11543
  5 Reallocated_Sector_Ct   PO--CK   200   200   140    -    0
  7 Seek_Error_Rate         POSR-K   100   253   051    -    0
  9 Power_On_Hours          -O--CK   078   078   000    -    16358
 10 Spin_Retry_Count        PO--CK   100   100   051    -    0
 11 Calibration_Retry_Count -O--CK   100   100   000    -    0
 12 Power_Cycle_Count       -O--CK   089   089   000    -    11539
184 End-to-End_Error        PO--CK   100   100   097    -    0
187 Reported_Uncorrect      -O--CK   100   094   000    -    87
188 Command_Timeout         -O--CK   100   098   000    -    11
190 Airflow_Temperature_Cel -O---K   055   053   040    -    45
192 Power-Off_Retract_Count -O--CK   200   200   000    -    141
193 Load_Cycle_Count        -O--CK   197   197   000    -    11543
196 Reallocated_Event_Count -O--CK   200   200   000    -    0
197 Current_Pending_Sector  -O--CK   200   200   000    -    0
198 Offline_Uncorrectable   ----CK   200   001   000    -    0
199 UDMA_CRC_Error_Count    -O--CK   200   200   000    -    0
200 Multi_Zone_Error_Rate   ---R--   200   001   000    -    0
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory Version 1
SMART           Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00       GPL,SL  R/O      1  Log Directory
0x01           SL  R/O      1  Summary SMART error log
0x02           SL  R/O      5  Comprehensive SMART error log
0x03       GPL     R/O      6  Ext. Comprehensive SMART error log
0x06           SL  R/O      1  SMART self-test log
0x07       GPL     R/O      1  Extended self-test log
0x09           SL  R/W      1  Selective self-test log
0x10       GPL     R/O      1  NCQ Command Error log
0x11       GPL     R/O      1  SATA Phy Event Counters log
0x80-0x9f  GPL,SL  R/W     16  Host vendor specific log
0xa0-0xa7  GPL,SL  VS      16  Device vendor specific log
0xa8-0xb7  GPL,SL  VS       1  Device vendor specific log
0xc0       GPL,SL  VS       1  Device vendor specific log
0xc1       GPL     VS      24  Device vendor specific log
0xe0       GPL,SL  R/W      1  SCT Command/Status
0xe1       GPL,SL  R/W      1  SCT Data Transfer

SMART Extended Comprehensive Error Log Version: 1 (6 sectors)
Device Error Count: 87 (device log contains only the most recent 24 errors)
	CR     = Command Register
	FEATR  = Features Register
	COUNT  = Count (was: Sector Count) Register
	LBA_48 = Upper bytes of LBA High/Mid/Low Registers ]  ATA-8
	LH     = LBA High (was: Cylinder High) Register    ]   LBA
	LM     = LBA Mid (was: Cylinder Low) Register      ] Register
	LL     = LBA Low (was: Sector Number) Register     ]
	DV     = Device (was: Device/Head) Register
	DC     = Device Control Register
	ER     = Error register
	ST     = Status register
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 87 [14] occurred at disk power-on lifetime: 15273 hours (636 days + 9 hours)
  When the command that caused the error occurred, the device was doing SMART Offline or Self-test.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 08 00 00 4d 00 65 f8 e0 00  Error: UNC 8 sectors at LBA = 0x4d0065f8 = 1291871736

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 08 00 00 00 65 4d f8 e0 00     19:03:31.888  READ DMA EXT
  35 00 00 00 08 00 00 00 60 b2 78 e0 00     19:03:31.888  WRITE DMA EXT
  25 00 00 00 08 00 00 00 65 4d f0 e0 00     19:03:31.888  READ DMA EXT
  35 00 00 00 08 00 00 04 d3 8c 12 e0 00     19:03:31.888  WRITE DMA EXT
  25 00 00 00 40 00 00 02 28 57 b0 e0 00     19:03:31.887  READ DMA EXT

Error 86 [13] occurred at disk power-on lifetime: 15273 hours (636 days + 9 hours)
  When the command that caused the error occurred, the device was in an unknown state.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 40 00 00 4d 00 65 c0 e0 00  Error: UNC 64 sectors at LBA = 0x4d0065c0 = 1291871680

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 40 00 00 00 65 4d c0 e0 00     19:03:29.496  READ DMA EXT
  35 00 00 00 08 00 00 00 65 4d 18 e0 00     19:03:29.496  WRITE DMA EXT
  35 00 00 00 20 00 00 07 11 db 00 e0 00     19:03:29.495  WRITE DMA EXT
  35 00 00 00 20 00 00 07 14 32 a0 e0 00     19:03:29.495  WRITE DMA EXT
  25 00 00 00 20 00 00 00 65 4d 00 e0 00     19:03:29.482  READ DMA EXT

Error 85 [12] occurred at disk power-on lifetime: 12825 hours (534 days + 9 hours)
  When the command that caused the error occurred, the device was doing SMART Offline or Self-test.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 08 00 00 4d 00 65 f8 e0 00  Error: UNC 8 sectors at LBA = 0x4d0065f8 = 1291871736

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 08 00 00 00 65 4d f8 e0 00     01:25:43.167  READ DMA EXT
  35 00 00 01 00 00 00 00 60 d6 b8 e0 00     01:25:43.166  WRITE DMA EXT
  35 00 00 01 00 00 00 00 60 d5 b8 e0 00     01:25:43.165  WRITE DMA EXT
  25 00 00 00 08 00 00 00 65 4d f0 e0 00     01:25:43.165  READ DMA EXT
  35 00 00 01 00 00 00 03 d4 64 98 e0 00     01:25:43.164  WRITE DMA EXT

Error 84 [11] occurred at disk power-on lifetime: 12825 hours (534 days + 9 hours)
  When the command that caused the error occurred, the device was doing SMART Offline or Self-test.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 20 00 00 4d 00 65 e0 e0 00  Error: UNC 32 sectors at LBA = 0x4d0065e0 = 1291871712

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 20 00 00 00 65 4d e0 e0 00     01:25:40.724  READ DMA EXT
  25 00 00 00 08 00 00 04 9f 47 88 e0 00     01:25:40.709  READ DMA EXT
  35 00 00 00 10 00 00 00 65 4d a8 e0 00     01:25:40.709  WRITE DMA EXT
  35 00 00 00 20 00 00 0e 65 76 20 e0 00     01:25:40.709  WRITE DMA EXT
  35 00 00 00 20 00 00 0e 6d bb 20 e0 00     01:25:40.709  WRITE DMA EXT

Error 83 [10] occurred at disk power-on lifetime: 12801 hours (533 days + 9 hours)
  When the command that caused the error occurred, the device was in an unknown state.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 08 00 00 4d 00 65 f8 e0 00  Error: UNC 8 sectors at LBA = 0x4d0065f8 = 1291871736

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 08 00 00 00 65 4d f8 e0 00     00:17:06.656  READ DMA EXT
  25 00 00 00 48 00 00 02 24 0b c0 e0 00     00:17:06.655  READ DMA EXT
  25 00 00 00 08 00 00 00 65 4d f0 e0 00     00:17:06.621  READ DMA EXT
  25 00 00 00 08 00 00 05 38 f7 28 e0 00     00:17:06.606  READ DMA EXT
  25 00 00 00 80 00 00 02 24 0c 88 e0 00     00:17:06.594  READ DMA EXT

Error 82 [9] occurred at disk power-on lifetime: 12801 hours (533 days + 9 hours)
  When the command that caused the error occurred, the device was doing SMART Offline or Self-test.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 a0 00 00 4d 00 65 60 e0 00  Error: UNC 160 sectors at LBA = 0x4d006560 = 1291871584

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 a0 00 00 00 65 4d 60 e0 00     00:17:04.035  READ DMA EXT
  35 00 00 00 20 00 00 0d 5c 72 60 e0 00     00:17:04.016  WRITE DMA EXT
  35 00 00 00 20 00 00 0d 60 5d 20 e0 00     00:17:04.015  WRITE DMA EXT
  25 00 00 00 80 00 00 02 24 0b 40 e0 00     00:17:04.003  READ DMA EXT
  25 00 00 00 20 00 00 00 65 4d 00 e0 00     00:17:04.002  READ DMA EXT

Error 81 [8] occurred at disk power-on lifetime: 12788 hours (532 days + 20 hours)
  When the command that caused the error occurred, the device was in an unknown state.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 08 00 00 4d 00 65 f8 e0 00  Error: UNC 8 sectors at LBA = 0x4d0065f8 = 1291871736

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 08 00 00 00 65 4d f8 e0 00     00:02:50.270  READ DMA EXT
  25 00 00 00 08 00 00 00 65 4d f0 e0 00     00:02:50.270  READ DMA EXT
  25 00 00 00 08 00 00 00 65 4d e8 e0 00     00:02:50.269  READ DMA EXT
  25 00 00 00 08 00 00 00 65 4d e0 e0 00     00:02:50.269  READ DMA EXT
  25 00 00 00 08 00 00 00 65 4d d8 e0 00     00:02:50.269  READ DMA EXT

Error 80 [7] occurred at disk power-on lifetime: 12788 hours (532 days + 20 hours)
  When the command that caused the error occurred, the device was doing SMART Offline or Self-test.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 a0 00 00 4d 00 65 60 e0 00  Error: UNC 160 sectors at LBA = 0x4d006560 = 1291871584

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 a0 00 00 00 65 4d 60 e0 00     00:02:46.036  READ DMA EXT
  35 00 00 00 20 00 00 0f 11 27 c0 e0 00     00:02:46.036  WRITE DMA EXT
  35 00 00 00 20 00 00 10 29 ea 00 e0 00     00:02:46.035  WRITE DMA EXT
  25 00 00 00 20 00 00 00 65 4d 00 e0 00     00:02:46.035  READ DMA EXT
  35 00 00 00 20 00 00 0f 11 27 c0 e0 00     00:02:46.035  WRITE DMA EXT

SMART Extended Self-test Log Version: 1 (1 sectors)
Num  Test_Description    Status                  Remaining  LifeTime(hours)  LBA_of_first_error
# 1  Extended offline    Aborted by host               90%         0         -

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Status Version:                  2
SCT Version (vendor specific):       258 (0x0102)
Device State:                        Active (0)
Current Temperature:                    45 Celsius
Power Cycle Min/Max Temperature:     25/45 Celsius
Lifetime    Min/Max Temperature:     26/47 Celsius
Under/Over Temperature Limit Count:   0/0

SCT Temperature History Version:     2
Temperature Sampling Period:         1 minute
Temperature Logging Interval:        1 minute
Min/Max recommended Temperature:      0/60 Celsius
Min/Max Temperature Limit:           -41/85 Celsius
Temperature History Size (Index):    128 (74)

SCT Error Recovery Control:
           Read:     85 (8.5 seconds)
          Write:     85 (8.5 seconds)

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11)
ID      Size     Value  Description
0x0001  2            0  Command failed due to ICRC error
0x0002  2            0  R_ERR response for data FIS
0x0003  2            0  R_ERR response for device-to-host data FIS
0x0004  2            0  R_ERR response for host-to-device data FIS
0x0005  2            0  R_ERR response for non-data FIS
0x0006  2            0  R_ERR response for device-to-host non-data FIS
0x0007  2            0  R_ERR response for host-to-device non-data FIS
0x000a  2            2  Device-to-host register FISes sent due to a COMRESET
0x8000  4        18166  Vendor specific

