Goodram Solid State Drives
==========================

This is a list of all tested Goodram solid state drive models and their MTBFs. See
more info on reliability test in the [README](https://github.com/bsdhw/SMART).

Contents
--------

1. [ SSD by Model  ](#ssd-by-model)
2. [ SSD by Family ](#ssd-by-family)

SSD by Model
------------

Please take all columns into account when reading the table. Pay attention on the
number of tested samples and power-on days. Simultaneous high values of both MTBF
and errors are possible if only rare drives in the subset encounter errors.

Days - avg. days per sample,
Err  - avg. errors per sample,
MTBF - avg. MTBF in years per sample.

| MFG       | Model              | Size   | Samples | Days  | Err   | MTBF |
|-----------|--------------------|--------|---------|-------|-------|------|
| Goodram   | SSDPR-CX300-120    | 120 GB | 1       | 1283  | 0     | 3.52   |
| Goodram   | SSD                | 240 GB | 4       | 983   | 0     | 2.70   |
| Goodram   | SSD                | 64 GB  | 1       | 820   | 0     | 2.25   |
| Goodram   | SSD                | 120 GB | 6       | 775   | 0     | 2.12   |
| Goodram   | SSDPR-CX400-128    | 128 GB | 3       | 657   | 0     | 1.80   |
| Goodram   | IRIDIUM PRO        | 120 GB | 1       | 599   | 0     | 1.64   |
| Goodram   | IRP-SSDPR-S25C-256 | 256 GB | 1       | 478   | 0     | 1.31   |
| Goodram   | IR-SSDPR-S25A-240  | 240 GB | 2       | 387   | 0     | 1.06   |
| Goodram   | SSDPR-CX400-256    | 256 GB | 3       | 246   | 0     | 0.67   |
| Goodram   | SSDPR-CL100-120-G2 | 120 GB | 2       | 183   | 0     | 0.50   |
| Goodram   | IRP_SSDPR_S25B_480 | 480 GB | 1       | 174   | 0     | 0.48   |
| Goodram   | SSDPR-CL100-120-G3 | 120 GB | 6       | 97    | 0     | 0.27   |
| Goodram   | SSDPR-CX400-128-G2 | 128 GB | 1       | 73    | 0     | 0.20   |
| Goodram   | SSDPR-CX400-512-G2 | 512 GB | 2       | 42    | 0     | 0.12   |
| Goodram   | SSDPR-CX400-256-G2 | 256 GB | 3       | 30    | 0     | 0.08   |
| Goodram   | SSDPR-CX400-01T-G2 | 1 TB   | 1       | 3     | 0     | 0.01   |
| Goodram   | SSDPR-CL100-240-G3 | 240 GB | 1       | 2     | 0     | 0.01   |

SSD by Family
-------------

Please take all columns into account when reading the table. Pay attention on the
number of tested samples and power-on days. Simultaneous high values of both MTBF
and errors are possible if only rare drives in the subset encounter errors.

Days - avg. days per sample,
Err  - avg. errors per sample,
MTBF - avg. MTBF in years per sample.

| MFG       | Family                 | Models | Samples | Days  | Err   | MTBF |
|-----------|------------------------|--------|---------|-------|-------|------|
| Goodram   | Phison Driven OEM SSDs | 3      | 11      | 855   | 0     | 2.34   |
| Goodram   | Phison Driven SSDs     | 4      | 9       | 453   | 0     | 1.24   |
| Goodram   | Unknown                | 10     | 19      | 165   | 0     | 0.45   |
