smartctl 7.1 2019-12-30 r5022 [x86_64-unknown-openbsd6.9] (local build)
Copyright (C) 2002-19, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Device Model:     3E128-TS2-550B01
Serial Number:    --
LU WWN Device Id: 5 001173 ...
Firmware Version: PRO6UI39
User Capacity:    100,000,000,512 bytes [100 GB]
Sector Size:      512 bytes logical/physical
Rotation Rate:    Solid State Device
Device is:        Not in smartctl database [for details use: -P showall]
ATA Version is:   ATA8-ACS, ACS-2 T13/2015-D revision 3
SATA Version is:  SATA 3.0, 6.0 Gb/s (current: 6.0 Gb/s)
Local Time is:    Mon Jun  7 19:22:09 2021 CDT
SMART support is: Available - device has SMART capability.
SMART support is: Enabled

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x00)	Offline data collection activity
					was never started.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(    0) seconds.
Offline data collection
capabilities: 			 (0x7b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   1) minutes.
Extended self-test routine
recommended polling time: 	 (  48) minutes.
Conveyance self-test routine
recommended polling time: 	 (   2) minutes.
SCT capabilities: 	       (0x0025)	SCT Status supported.
					SCT Data Table supported.

SMART Attributes Data Structure revision number: 10
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAG     VALUE WORST THRESH TYPE      UPDATED  WHEN_FAILED RAW_VALUE
  1 Raw_Read_Error_Rate     0x0033   120   120   050    Pre-fail  Always       -       0
  5 Reallocated_Sector_Ct   0x0033   100   100   003    Pre-fail  Always       -       0
  9 Power_On_Hours          0x0032   000   000   000    Old_age   Always       -       14428 (75 164 0)
 12 Power_Cycle_Count       0x0032   100   100   000    Old_age   Always       -       245
 13 Read_Soft_Error_Rate    0x0032   120   120   000    Old_age   Always       -       172704929939456
100 Unknown_Attribute       0x0032   000   000   000    Old_age   Always       -       2783
170 Unknown_Attribute       0x00ef   000   000   000    Pre-fail  Always       -       35072
171 Unknown_Attribute       0x000a   000   000   000    Old_age   Always       -       0
172 Unknown_Attribute       0x0032   000   000   000    Old_age   Always       -       0
174 Unknown_Attribute       0x0030   000   000   000    Old_age   Offline      -       250
177 Wear_Leveling_Count     0x0000   000   000   000    Old_age   Offline      -       0
181 Program_Fail_Cnt_Total  0x000a   000   000   000    Old_age   Always       -       0
182 Erase_Fail_Count_Total  0x0032   000   000   000    Old_age   Always       -       0
184 End-to-End_Error        0x0000   100   100   090    Old_age   Offline      -       0
187 Reported_Uncorrect      0x001c   100   100   000    Old_age   Offline      -       0
194 Temperature_Celsius     0x0022   054   061   000    Old_age   Always       -       54 (Min/Max 15/61)
195 Hardware_ECC_Recovered  0x001c   100   100   000    Old_age   Offline      -       0
196 Reallocated_Event_Count 0x0033   100   100   003    Pre-fail  Always       -       0
198 Offline_Uncorrectable   0x0010   120   120   000    Old_age   Offline      -       0
199 UDMA_CRC_Error_Count    0x0004   200   200   000    Old_age   Offline      -       0
201 Unknown_SSD_Attribute   0x001c   100   100   000    Old_age   Offline      -       0
204 Soft_ECC_Correction     0x001c   100   100   000    Old_age   Offline      -       0
230 Unknown_SSD_Attribute   0x0013   100   100   000    Pre-fail  Always       -       100
231 Temperature_Celsius     0x0013   100   100   010    Pre-fail  Always       -       0
232 Available_Reservd_Space 0x0032   000   000   000    Old_age   Always       -       34
233 Media_Wearout_Indicator 0x0032   000   000   000    Old_age   Always       -       2473
234 Unknown_Attribute       0x0032   000   000   000    Old_age   Always       -       9610
241 Total_LBAs_Written      0x0032   000   000   000    Old_age   Always       -       9610
242 Total_LBAs_Read         0x0032   000   000   000    Old_age   Always       -       203903

SMART Error Log not supported

SMART Self-test Log not supported

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.



