smartctl 7.3 2022-02-28 r5338 [FreeBSD 12.3-RELEASE-p3 amd64] (local build)
Copyright (C) 2002-22, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Seagate Constellation ES.3
Device Model:     ST4000NM0033-9ZM170
Serial Number:    --
LU WWN Device Id: 5 000c50 ...
Firmware Version: SN04
User Capacity:    4,000,787,030,016 bytes [4.00 TB]
Sector Size:      512 bytes logical/physical
Rotation Rate:    7200 rpm
Form Factor:      3.5 inches
Device is:        In smartctl database 7.3/5319
ATA Version is:   ACS-2 (minor revision not indicated)
SATA Version is:  SATA 3.0, 6.0 Gb/s (current: 6.0 Gb/s)
Local Time is:    Sun Sep 25 14:50:20 2022 CEST
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Unavailable
APM feature is:   Unavailable
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, NOT FROZEN [SEC1]
Wt Cache Reorder: Enabled

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x82)	Offline data collection activity
					was completed without error.
					Auto Offline Data Collection: Enabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(  609) seconds.
Offline data collection
capabilities: 			 (0x7b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   1) minutes.
Extended self-test routine
recommended polling time: 	 ( 484) minutes.
Conveyance self-test routine
recommended polling time: 	 (   2) minutes.
SCT capabilities: 	       (0x50bd)	SCT Status supported.
					SCT Error Recovery Control supported.
					SCT Feature Control supported.
					SCT Data Table supported.

SMART Attributes Data Structure revision number: 10
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     POSR--   078   063   044    -    59071667
  3 Spin_Up_Time            PO----   093   092   000    -    0
  4 Start_Stop_Count        -O--CK   100   100   020    -    36
  5 Reallocated_Sector_Ct   PO--CK   100   100   010    -    1
  7 Seek_Error_Rate         POSR--   091   060   030    -    1457811891
  9 Power_On_Hours          -O--CK   035   035   000    -    57494
 10 Spin_Retry_Count        PO--C-   100   100   097    -    0
 12 Power_Cycle_Count       -O--CK   100   100   020    -    36
184 End-to-End_Error        -O--CK   100   100   099    -    0
187 Reported_Uncorrect      -O--CK   092   092   000    -    8
188 Command_Timeout         -O--CK   100   100   000    -    0
189 High_Fly_Writes         -O-RCK   100   100   000    -    0
190 Airflow_Temperature_Cel -O---K   057   051   045    -    43 (Min/Max 41/47)
191 G-Sense_Error_Rate      -O--CK   100   100   000    -    0
192 Power-Off_Retract_Count -O--CK   100   100   000    -    35
193 Load_Cycle_Count        -O--CK   099   099   000    -    2416
194 Temperature_Celsius     -O---K   043   049   000    -    43 (0 25 0 0 0)
195 Hardware_ECC_Recovered  -O-RC-   060   005   000    -    59071667
197 Current_Pending_Sector  -O--C-   100   100   000    -    74
198 Offline_Uncorrectable   ----C-   100   100   000    -    74
199 UDMA_CRC_Error_Count    -OSRCK   200   200   000    -    0
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory Version 1
SMART           Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00       GPL,SL  R/O      1  Log Directory
0x01           SL  R/O      1  Summary SMART error log
0x02           SL  R/O      5  Comprehensive SMART error log
0x03       GPL     R/O      5  Ext. Comprehensive SMART error log
0x06           SL  R/O      1  SMART self-test log
0x07       GPL     R/O      1  Extended self-test log
0x08       GPL,SL  R/O      2  Power Conditions log
0x09           SL  R/W      1  Selective self-test log
0x10       GPL     R/O      1  NCQ Command Error log
0x11       GPL     R/O      1  SATA Phy Event Counters log
0x21       GPL     R/O      1  Write stream error log
0x22       GPL     R/O      1  Read stream error log
0x24       GPL     R/O    512  Current Device Internal Status Data log
0x30       GPL,SL  R/O      9  IDENTIFY DEVICE data log
0x80-0x9f  GPL,SL  R/W     16  Host vendor specific log
0xa1       GPL,SL  VS      20  Device vendor specific log
0xa2       GPL     VS    4496  Device vendor specific log
0xa8       GPL,SL  VS     129  Device vendor specific log
0xa9       GPL,SL  VS       1  Device vendor specific log
0xb0       GPL     VS    5176  Device vendor specific log
0xbd       GPL     VS     512  Device vendor specific log
0xbe-0xbf  GPL     VS   65535  Device vendor specific log
0xc1       GPL,SL  VS      10  Device vendor specific log
0xc2       GPL,SL  VS      50  Device vendor specific log
0xc3       GPL,SL  VS       8  Device vendor specific log
0xc4       GPL,SL  VS       5  Device vendor specific log
0xd1       GPL,SL  VS       8  Device vendor specific log
0xe0       GPL,SL  R/W      1  SCT Command/Status
0xe1       GPL,SL  R/W      1  SCT Data Transfer

SMART Extended Comprehensive Error Log Version: 1 (5 sectors)
Device Error Count: 8
	CR     = Command Register
	FEATR  = Features Register
	COUNT  = Count (was: Sector Count) Register
	LBA_48 = Upper bytes of LBA High/Mid/Low Registers ]  ATA-8
	LH     = LBA High (was: Cylinder High) Register    ]   LBA
	LM     = LBA Mid (was: Cylinder Low) Register      ] Register
	LL     = LBA Low (was: Sector Number) Register     ]
	DV     = Device (was: Device/Head) Register
	DC     = Device Control Register
	ER     = Error register
	ST     = Status register
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 8 [7] occurred at disk power-on lifetime: 50103 hours (2087 days + 15 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 01 ce 95 9f e4 00 00  Error: UNC at LBA = 0x1ce959fe4 = 7760879588

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 01 00 00 01 ce 95 9f 53 40 00 39d+22:54:47.562  READ FPDMA QUEUED
  60 00 00 01 00 00 01 ce 95 a0 53 40 00 39d+22:54:47.555  READ FPDMA QUEUED
  60 00 00 01 00 00 01 ce 95 a1 53 40 00 39d+22:54:47.548  READ FPDMA QUEUED
  60 00 00 01 00 00 01 ce 95 a2 53 40 00 39d+22:54:47.542  READ FPDMA QUEUED
  60 00 00 00 29 00 01 ce 95 a4 53 40 00 39d+22:54:47.524  READ FPDMA QUEUED

Error 7 [6] occurred at disk power-on lifetime: 50103 hours (2087 days + 15 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 01 ce 95 99 73 00 00  Error: UNC at LBA = 0x1ce959973 = 7760877939

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 01 00 00 01 ce 95 99 53 40 00 39d+22:54:44.906  READ FPDMA QUEUED
  60 00 00 00 29 00 01 ce 95 a4 53 40 00 39d+22:54:44.906  READ FPDMA QUEUED
  60 00 00 01 00 00 01 ce 95 a2 53 40 00 39d+22:54:44.906  READ FPDMA QUEUED
  60 00 00 01 00 00 01 ce 95 a1 53 40 00 39d+22:54:44.906  READ FPDMA QUEUED
  60 00 00 01 00 00 01 ce 95 a0 53 40 00 39d+22:54:44.906  READ FPDMA QUEUED

Error 6 [5] occurred at disk power-on lifetime: 50103 hours (2087 days + 15 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 01 ce 95 99 73 00 00  Error: UNC at LBA = 0x1ce959973 = 7760877939

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 00 29 00 01 ce 95 a4 53 40 00 39d+22:54:42.220  READ FPDMA QUEUED
  60 00 00 01 00 00 01 ce 95 a3 53 40 00 39d+22:54:42.220  READ FPDMA QUEUED
  60 00 00 01 00 00 01 ce 95 a2 53 40 00 39d+22:54:42.220  READ FPDMA QUEUED
  60 00 00 01 00 00 01 ce 95 a1 53 40 00 39d+22:54:42.220  READ FPDMA QUEUED
  60 00 00 01 00 00 01 ce 95 a0 53 40 00 39d+22:54:42.220  READ FPDMA QUEUED

Error 5 [4] occurred at disk power-on lifetime: 50102 hours (2087 days + 14 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 59 3b 0a 6c 00 00  Error: UNC at LBA = 0x593b0a6c = 1497041516

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 01 00 00 00 59 3b 09 bd 40 00 39d+22:28:53.447  READ FPDMA QUEUED
  60 00 00 01 00 00 00 59 3b 0a bd 40 00 39d+22:28:53.447  READ FPDMA QUEUED
  60 00 00 00 ed 00 00 59 3b 16 34 40 00 39d+22:28:53.447  READ FPDMA QUEUED
  60 00 00 01 00 00 00 59 3b 15 34 40 00 39d+22:28:53.447  READ FPDMA QUEUED
  60 00 00 01 00 00 00 59 3b 14 34 40 00 39d+22:28:53.447  READ FPDMA QUEUED

Error 4 [3] occurred at disk power-on lifetime: 50102 hours (2087 days + 14 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 59 3b 0a 6c 00 00  Error: UNC at LBA = 0x593b0a6c = 1497041516

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 01 00 00 00 59 3b 0a bd 40 00 39d+22:28:50.777  READ FPDMA QUEUED
  60 00 00 01 00 00 00 59 33 20 ca 40 00 39d+22:28:49.077  READ FPDMA QUEUED
  60 00 00 01 00 00 00 59 33 1f ca 40 00 39d+22:28:49.077  READ FPDMA QUEUED
  60 00 00 01 00 00 00 59 33 1e ca 40 00 39d+22:28:49.077  READ FPDMA QUEUED
  60 00 00 01 00 00 00 59 33 1d ca 40 00 39d+22:28:49.077  READ FPDMA QUEUED

Error 3 [2] occurred at disk power-on lifetime: 50100 hours (2087 days + 12 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 01 32 08 da 66 00 00  Error: UNC at LBA = 0x13208da66 = 5134408294

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 01 00 00 01 32 08 da 5c 40 00 39d+20:45:15.287  READ FPDMA QUEUED
  60 00 00 01 00 00 01 32 08 db 5c 40 00 39d+20:45:15.285  READ FPDMA QUEUED
  60 00 00 01 00 00 01 32 08 dc 5c 40 00 39d+20:45:15.284  READ FPDMA QUEUED
  60 00 00 01 00 00 01 32 08 dd 5c 40 00 39d+20:45:15.284  READ FPDMA QUEUED
  60 00 00 01 00 00 01 32 08 de 5c 40 00 39d+20:45:15.283  READ FPDMA QUEUED

Error 2 [1] occurred at disk power-on lifetime: 50100 hours (2087 days + 12 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 01 32 08 da 26 00 00  Error: UNC at LBA = 0x13208da26 = 5134408230

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 01 00 00 01 32 08 d9 5c 40 00 39d+20:45:10.706  READ FPDMA QUEUED
  60 00 00 01 00 00 01 32 08 e7 67 40 00 39d+20:45:10.706  READ FPDMA QUEUED
  60 00 00 01 00 00 01 32 08 e6 67 40 00 39d+20:45:10.706  READ FPDMA QUEUED
  60 00 00 01 00 00 01 32 08 e5 67 40 00 39d+20:45:10.706  READ FPDMA QUEUED
  60 00 00 00 0b 00 01 32 08 e0 5c 40 00 39d+20:45:10.706  READ FPDMA QUEUED

Error 1 [0] occurred at disk power-on lifetime: 50100 hours (2087 days + 12 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 01 32 08 da 25 00 00  Error: UNC at LBA = 0x13208da25 = 5134408229

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 00 0b 00 01 32 08 e0 5c 40 00 39d+20:45:06.649  READ FPDMA QUEUED
  60 00 00 01 00 00 01 32 08 df 5c 40 00 39d+20:45:06.649  READ FPDMA QUEUED
  60 00 00 01 00 00 01 32 08 de 5c 40 00 39d+20:45:06.649  READ FPDMA QUEUED
  60 00 00 01 00 00 01 32 08 dd 5c 40 00 39d+20:45:06.649  READ FPDMA QUEUED
  60 00 00 01 00 00 01 32 08 dc 5c 40 00 39d+20:45:06.649  READ FPDMA QUEUED

SMART Extended Self-test Log Version: 1 (1 sectors)
No self-tests have been logged.  [To run self-tests, use: smartctl -t]

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Status Version:                  3
SCT Version (vendor specific):       522 (0x020a)
Device State:                        Active (0)
Current Temperature:                    43 Celsius
Power Cycle Min/Max Temperature:     40/47 Celsius
Lifetime    Min/Max Temperature:     25/49 Celsius
Under/Over Temperature Limit Count:   0/26704

SCT Temperature History Version:     2
Temperature Sampling Period:         1 minute
Temperature Logging Interval:        10 minutes
Min/Max recommended Temperature:      0/ 0 Celsius
Min/Max Temperature Limit:            0/ 0 Celsius
Temperature History Size (Index):    128 (65)

SCT Error Recovery Control:
           Read:    100 (10.0 seconds)
          Write:    100 (10.0 seconds)

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11)
ID      Size     Value  Description
0x000a  2            1  Device-to-host register FISes sent due to a COMRESET
0x0001  2            0  Command failed due to ICRC error
0x0003  2            0  R_ERR response for device-to-host data FIS
0x0004  2            0  R_ERR response for host-to-device data FIS
0x0006  2            0  R_ERR response for device-to-host non-data FIS
0x0007  2            0  R_ERR response for host-to-device non-data FIS



