smartctl 7.2 2020-12-30 r5155 [FreeBSD 12.2-RELEASE-p4 amd64] (local build)
Copyright (C) 2002-20, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Device Model:     Corsair Neutron GTX SSD
Serial Number:    --
Firmware Version: M312
User Capacity:    120,034,123,776 bytes [120 GB]
Sector Size:      512 bytes logical/physical
Rotation Rate:    Solid State Device
TRIM Command:     Available
Device is:        Not in smartctl database [for details use: -P showall]
ATA Version is:   ATA8-ACS (minor revision not indicated)
SATA Version is:  SATA 2.5, 6.0 Gb/s
Local Time is:    Thu Apr 29 12:59:36 2021 EEST
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Unavailable
APM feature is:   Unavailable
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, frozen [SEC2]
Wt Cache Reorder: Unavailable

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x02)	Offline data collection activity
					was completed without error.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(    3) seconds.
Offline data collection
capabilities: 			 (0x19) SMART execute Offline immediate.
					No Auto Offline data collection support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					No Conveyance Self-test supported.
					No Selective Self-test supported.
SMART capabilities:            (0x0002)	Does not save SMART data before
					entering power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					No General Purpose Logging support.
Short self-test routine 
recommended polling time: 	 (   1) minutes.
Extended self-test routine
recommended polling time: 	 (   5) minutes.

SMART Attributes Data Structure revision number: 0
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     -OSR--   166   166   006    -    0
  5 Reallocated_Sector_Ct   -O--CK   099   099   036    -    149
  9 Power_On_Hours          -O--CK   082   082   000    -    16277
 12 Power_Cycle_Count       -O--CK   100   100   000    -    5709
171 Unknown_Attribute       -O--CK   253   253   000    -    0
172 Unknown_Attribute       -O--CK   100   100   000    -    152
181 Program_Fail_Cnt_Total  -O--CK   253   253   000    -    0
182 Erase_Fail_Count_Total  -O--CK   100   100   000    -    152
194 Temperature_Celsius     -O----   036   000   000    -    36 (Min/Max 14/48)
201 Unknown_SSD_Attribute   -OSR--   100   100   000    -    0
204 Soft_ECC_Correction     -OSR--   100   100   000    -    0
231 Unknown_SSD_Attribute   PO--CK   090   090   010    -    11
234 Unknown_Attribute       -O--CK   100   100   000    -    61626
241 Total_LBAs_Written      -O--CK   100   100   000    -    9324
242 Total_LBAs_Read         -O--CK   100   100   000    -    10291
250 Read_Error_Retry_Rate   -O--CK   100   100   000    -    184498
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory not supported

SMART Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00           SL  R/O      1  Log Directory
0x01           SL  R/O      1  Summary SMART error log
0x02           SL  R/O      4  Comprehensive SMART error log
0x03           SL  R/O      5  Ext. Comprehensive SMART error log
0x04           SL  R/O      8  Device Statistics log
0x06           SL  R/O      1  SMART self-test log

SMART Extended Comprehensive Error Log (GP Log 0x03) not supported

SMART Error Log Version: 1
ATA Error Count: 23323 (device log contains only the most recent five errors)
	CR = Command Register [HEX]
	FR = Features Register [HEX]
	SC = Sector Count Register [HEX]
	SN = Sector Number Register [HEX]
	CL = Cylinder Low Register [HEX]
	CH = Cylinder High Register [HEX]
	DH = Device/Head Register [HEX]
	DC = Device Command Register [HEX]
	ER = Error register [HEX]
	ST = Status register [HEX]
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 23323 occurred at disk power-on lifetime: 16277 hours (678 days + 5 hours)
  When the command that caused the error occurred, the device was in an unknown state.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  04 51 00 00 4f c2 e0  Error: ABRT

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  b0 d5 81 04 4f c2 40 40      05:38:07.770  SMART READ LOG
  b0 d5 01 04 4f c2 40 40      05:38:07.770  SMART READ LOG
  b0 d5 01 06 4f c2 40 40      05:38:07.770  SMART READ LOG
  b0 d5 01 01 4f c2 40 40      05:38:07.770  SMART READ LOG
  b0 d5 01 00 4f c2 40 40      05:38:07.770  SMART READ LOG

Error 23322 occurred at disk power-on lifetime: 16277 hours (678 days + 5 hours)
  When the command that caused the error occurred, the device was in an unknown state.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  04 51 00 00 4f c2 e0  Error: ABRT

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  b0 d5 81 04 4f c2 40 40      05:37:39.640  SMART READ LOG
  b0 d5 01 04 4f c2 40 40      05:37:39.640  SMART READ LOG
  b0 d5 01 06 4f c2 40 40      05:37:39.640  SMART READ LOG
  b0 d5 01 01 4f c2 40 40      05:37:39.640  SMART READ LOG
  b0 d5 01 00 4f c2 40 40      05:37:39.640  SMART READ LOG

Error 23321 occurred at disk power-on lifetime: 16277 hours (678 days + 5 hours)
  When the command that caused the error occurred, the device was in an unknown state.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  04 51 00 00 4f c2 e0  Error: ABRT

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  b0 d5 81 04 4f c2 40 40      05:35:55.150  SMART READ LOG
  b0 d5 01 04 4f c2 40 40      05:35:55.150  SMART READ LOG
  b0 d5 01 06 4f c2 40 40      05:35:55.150  SMART READ LOG
  b0 d5 01 01 4f c2 40 40      05:35:55.150  SMART READ LOG
  b0 d5 01 00 4f c2 40 40      05:35:55.150  SMART READ LOG

Error 23320 occurred at disk power-on lifetime: 16272 hours (678 days + 0 hours)
  When the command that caused the error occurred, the device was in an unknown state.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  01 50 01 01 00 00 00

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  00 00 00 00 00 00 00 00      00:01:15.230  NOP [Abort queued commands]
  00 00 00 00 00 00 00 00      00:01:15.240  NOP [Abort queued commands]
  00 00 00 00 00 00 00 00      00:01:15.220  NOP [Abort queued commands]
  00 00 00 00 00 00 00 00      00:01:15.230  NOP [Abort queued commands]
  25 00 08 a8 4b f9 e0 e0      00:00:58.300  READ DMA EXT

Error 23319 occurred at disk power-on lifetime: 16272 hours (678 days + 0 hours)
  When the command that caused the error occurred, the device was in an unknown state.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  01 50 01 01 00 00 00

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  00 00 00 00 00 00 00 00      00:01:15.220  NOP [Abort queued commands]
  00 00 00 00 00 00 00 00      00:01:15.230  NOP [Abort queued commands]
  25 00 08 a8 4b f9 e0 e0      00:00:58.300  READ DMA EXT
  25 00 01 af 4b f9 e0 e0      00:00:58.300  READ DMA EXT
  25 00 20 02 00 00 e0 e0      00:00:58.300  READ DMA EXT

SMART Extended Self-test Log (GP Log 0x07) not supported

SMART Self-test log structure revision number 1
Num  Test_Description    Status                  Remaining  LifeTime(hours)  LBA_of_first_error
# 1  Short offline       Completed without error       00%       451         -

Selective Self-tests/Logging not supported

SCT Commands not supported

Device Statistics (SMART Log 0x04)
Page  Offset Size        Value Flags Description
ATA_SMART_READ_LOG failed: Input/output error
Read Device Statistics pages 0x00-0x80 failed

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11)
ID      Size     Value  Description
0x0001  2            0  Command failed due to ICRC error
0x0002  2            0  R_ERR response for data FIS
0x0003  2            0  R_ERR response for device-to-host data FIS
0x0004  2            0  R_ERR response for host-to-device data FIS
0x0005  2            0  R_ERR response for non-data FIS
0x0006  2            0  R_ERR response for device-to-host non-data FIS
0x0007  2            0  R_ERR response for host-to-device non-data FIS
0x0008  2            0  Device-to-host non-data FIS retries
0x0009  2            0  Transition from drive PhyRdy to drive PhyNRdy
0x000a  2           11  Device-to-host register FISes sent due to a COMRESET
0x000b  2            0  CRC errors within host-to-device FIS
0x000d  2            0  Non-CRC errors within host-to-device FIS
0x000f  2            0  R_ERR response for host-to-device data FIS, CRC
0x0010  2            0  R_ERR response for host-to-device data FIS, non-CRC
0x0012  2            0  R_ERR response for host-to-device non-data FIS, CRC
0x0013  2            0  R_ERR response for host-to-device non-data FIS, non-CRC

