smartctl 6.6 2017-11-05 r4594 [FreeBSD 11.2-RELEASE-p10 amd64] (local build)
Copyright (C) 2002-17, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Seagate Barracuda 7200.7 and 7200.7 Plus
Device Model:     ST3160023A
Serial Number:    --
Firmware Version: 3.01
User Capacity:    160,040,803,840 bytes [160 GB]
Sector Size:      512 bytes logical/physical
Device is:        In smartctl database [for details use: -P show]
ATA Version is:   ATA/ATAPI-6 T13/1410D revision 2
Local Time is:    Mon May 25 18:19:33 2020 MSK
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Unavailable
APM feature is:   Unavailable
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, frozen [SEC2]
Wt Cache Reorder: Unavailable

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x82)	Offline data collection activity
					was completed without error.
					Auto Offline Data Collection: Enabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(  430) seconds.
Offline data collection
capabilities: 			 (0x5b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					No Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					No General Purpose Logging support.
Short self-test routine 
recommended polling time: 	 (   1) minutes.
Extended self-test routine
recommended polling time: 	 ( 111) minutes.

SMART Attributes Data Structure revision number: 10
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     POSR--   065   054   006    -    0
  3 Spin_Up_Time            PO----   097   096   000    -    0
  4 Start_Stop_Count        -O--CK   098   098   020    -    2054
  5 Reallocated_Sector_Ct   PO--CK   100   100   036    -    0
  7 Seek_Error_Rate         POSR--   084   060   030    -    321042941
  9 Power_On_Hours          -O--CK   072   072   000    -    25344
 10 Spin_Retry_Count        PO--C-   100   099   097    -    0
 12 Power_Cycle_Count       -O--CK   098   098   020    -    2655
194 Temperature_Celsius     -O---K   033   064   000    -    33
195 Hardware_ECC_Recovered  -O-RC-   065   054   000    -    0
197 Current_Pending_Sector  -O--C-   100   100   000    -    0
198 Offline_Uncorrectable   ----C-   100   100   000    -    0
199 UDMA_CRC_Error_Count    -OSRCK   200   081   000    -    4637
200 Multi_Zone_Error_Rate   ------   100   253   000    -    0
202 Data_Address_Mark_Errs  -O--CK   100   253   000    -    0
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory not supported

SMART Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00           SL  R/O      1  Log Directory
0x01           SL  R/O      1  Summary SMART error log
0x02           SL  R/O      5  Comprehensive SMART error log
0x03           SL  R/O      5  Ext. Comprehensive SMART error log
0x06           SL  R/O      1  SMART self-test log
0x07           SL  R/O      1  Extended self-test log
0x09           SL  R/W      1  Selective self-test log
0x20           SL  R/O      1  Streaming performance log [OBS-8]
0x21           SL  R/O      1  Write stream error log
0x22           SL  R/O      1  Read stream error log
0x23           SL  R/O      1  Delayed sector log [OBS-8]
0x80-0x9f      SL  R/W     16  Host vendor specific log
0xa0           SL  VS       1  Device vendor specific log
0xa1           SL  VS      20  Device vendor specific log
0xa2           SL  VS     101  Device vendor specific log
0xa8           SL  VS      20  Device vendor specific log
0xa9           SL  VS       1  Device vendor specific log

SMART Extended Comprehensive Error Log (GP Log 0x03) not supported

SMART Error Log Version: 1
ATA Error Count: 7128 (device log contains only the most recent five errors)
	CR = Command Register [HEX]
	FR = Features Register [HEX]
	SC = Sector Count Register [HEX]
	SN = Sector Number Register [HEX]
	CL = Cylinder Low Register [HEX]
	CH = Cylinder High Register [HEX]
	DH = Device/Head Register [HEX]
	DC = Device Command Register [HEX]
	ER = Error register [HEX]
	ST = Status register [HEX]
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 7128 occurred at disk power-on lifetime: 25235 hours (1051 days + 11 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  84 51 01 46 fb 38 e2  Error: ICRC, ABRT 1 sectors at LBA = 0x0238fb46 = 37288774

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  25 03 08 3f fb 38 e2 00      00:00:40.631  READ DMA EXT
  25 03 08 37 fb 38 e2 00      00:00:40.631  READ DMA EXT
  25 03 08 2f fb 38 e2 00      00:00:40.631  READ DMA EXT
  25 03 08 27 fb 38 e2 00      00:00:40.631  READ DMA EXT
  25 03 08 1f fb 38 e2 00      00:00:40.630  READ DMA EXT

Error 7127 occurred at disk power-on lifetime: 25128 hours (1047 days + 0 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  84 51 01 1f d2 00 e0  Error: ICRC, ABRT 1 sectors at LBA = 0x0000d21f = 53791

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  25 03 20 00 d2 00 e0 00      00:03:12.525  READ DMA EXT
  25 03 20 e0 d1 00 e0 00      00:03:12.524  READ DMA EXT
  25 03 20 c0 d1 00 e0 00      00:03:12.522  READ DMA EXT
  25 03 20 a0 d1 00 e0 00      00:03:12.521  READ DMA EXT
  25 03 20 80 d1 00 e0 00      00:03:12.519  READ DMA EXT

Error 7126 occurred at disk power-on lifetime: 25044 hours (1043 days + 12 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  84 51 01 5f 88 a0 e0  Error: ICRC, ABRT 1 sectors at LBA = 0x00a0885f = 10520671

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  25 03 80 e0 87 a0 e0 00      02:52:43.818  READ DMA EXT
  25 03 80 60 87 a0 e0 00      02:52:43.815  READ DMA EXT
  25 03 80 e0 86 a0 e0 00      02:52:43.813  READ DMA EXT
  25 03 80 60 86 a0 e0 00      02:52:43.810  READ DMA EXT
  25 03 80 e0 85 a0 e0 00      02:52:43.808  READ DMA EXT

Error 7125 occurred at disk power-on lifetime: 24336 hours (1014 days + 0 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  84 51 01 a3 cf c6 e0  Error: ICRC, ABRT 1 sectors at LBA = 0x00c6cfa3 = 13029283

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  25 03 20 84 cf c6 e0 00      00:11:27.479  READ DMA EXT
  35 03 20 60 43 c6 e0 00      00:11:27.478  WRITE DMA EXT
  35 03 08 80 d0 c6 e0 00      00:11:27.476  WRITE DMA EXT
  25 03 20 80 cf c6 e0 00      00:11:27.476  READ DMA EXT
  35 03 20 60 43 c6 e0 00      00:11:27.475  WRITE DMA EXT

Error 7124 occurred at disk power-on lifetime: 24295 hours (1012 days + 7 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  84 51 01 df 9f 4a e0  Error: ICRC, ABRT 1 sectors at LBA = 0x004a9fdf = 4890591

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  25 03 80 60 9f 4a e0 00      00:59:42.541  READ DMA EXT
  25 03 80 e0 9e 4a e0 00      00:59:42.537  READ DMA EXT
  25 03 80 60 9e 4a e0 00      00:59:42.533  READ DMA EXT
  25 03 80 e0 9d 4a e0 00      00:59:42.530  READ DMA EXT
  25 03 80 60 9d 4a e0 00      00:59:42.526  READ DMA EXT

SMART Extended Self-test Log (GP Log 0x07) not supported

SMART Self-test log structure revision number 1
No self-tests have been logged.  [To run self-tests, use: smartctl -t]

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Commands not supported

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11) not supported

