smartctl 7.2 2021-09-14 r5236 [FreeBSD 13.0-RELEASE-p6 amd64] (local build)
Copyright (C) 2002-20, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Fujitsu MHZ BH
Device Model:     FUJITSU MHZ2160BH G2
Serial Number:    --
LU WWN Device Id: 5 00000e ...
Firmware Version: 00000009
User Capacity:    160,041,885,696 bytes [160 GB]
Sector Size:      512 bytes logical/physical
Device is:        In smartctl database [for details use: -P show]
ATA Version is:   ATA8-ACS T13/1699-D revision 3f
SATA Version is:  SATA 2.5, 3.0 Gb/s
Local Time is:    Tue Jan 18 19:45:16 2022 EET
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM level is:     254 (maximum performance), recommended: 254
APM level is:     128 (minimum power consumption without standby)
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, frozen [SEC2]
Wt Cache Reorder: Enabled

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x00)	Offline data collection activity
					was never started.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(  649) seconds.
Offline data collection
capabilities: 			 (0x7b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   2) minutes.
Extended self-test routine
recommended polling time: 	 (  92) minutes.
Conveyance self-test routine
recommended polling time: 	 (   2) minutes.
SCT capabilities: 	       (0x003d)	SCT Status supported.
					SCT Error Recovery Control supported.
					SCT Feature Control supported.
					SCT Data Table supported.

SMART Attributes Data Structure revision number: 16
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     POSR--   100   100   046    -    224373
  2 Throughput_Performance  P-S---   100   100   030    -    28901376
  3 Spin_Up_Time            PO----   100   100   025    -    1
  4 Start_Stop_Count        -O--CK   097   097   000    -    12454
  5 Reallocated_Sector_Ct   PO--CK   100   100   024    -    2 (1998 2)
  7 Seek_Error_Rate         POSR--   100   100   047    -    1821
  8 Seek_Time_Performance   P-S---   100   100   019    -    0
  9 Power_On_Hours          -O--CK   066   066   000    -    17315
 10 Spin_Retry_Count        PO--C-   100   100   020    -    0
 12 Power_Cycle_Count       -O--CK   098   098   000    -    11247
192 Power-Off_Retract_Count -O--CK   100   100   000    -    109
193 Load_Cycle_Count        -O--CK   096   096   000    -    87023
194 Temperature_Celsius     -O---K   100   065   000    -    27 (Min/Max 10/67)
195 Hardware_ECC_Recovered  -O-RC-   100   100   000    -    89
196 Reallocated_Event_Count -O--CK   100   100   000    -    2 (1 6909)
197 Current_Pending_Sector  -O--C-   100   100   000    -    0
198 Offline_Uncorrectable   ----C-   099   099   000    -    2
199 UDMA_CRC_Error_Count    -OSRCK   200   253   000    -    0
200 Multi_Zone_Error_Rate   POSR--   100   100   060    -    27869
203 Run_Out_Cancel          -O----   100   100   000    -    1533270950194
240 Head_Flying_Hours       -OSRCK   200   200   000    -    0
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory Version 1
SMART           Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00       GPL,SL  R/O      1  Log Directory
0x01       GPL,SL  R/O      1  Summary SMART error log
0x02       GPL,SL  R/O     51  Comprehensive SMART error log
0x03       GPL,SL  R/O     64  Ext. Comprehensive SMART error log
0x06       GPL,SL  R/O      1  SMART self-test log
0x07       GPL,SL  R/O      2  Extended self-test log
0x09       GPL,SL  R/W      1  Selective self-test log
0x10       GPL,SL  R/O      1  NCQ Command Error log
0x11       GPL,SL  R/O      1  SATA Phy Event Counters log
0x23       GPL,SL  R/O      1  Delayed sector log [OBS-8]
0x80-0x9f  GPL,SL  R/W     16  Host vendor specific log
0xa1       GPL,SL  VS       1  Device vendor specific log

SMART Extended Comprehensive Error Log Version: 1 (64 sectors)
Device Error Count: 65282 (device log contains only the most recent 256 errors)
	CR     = Command Register
	FEATR  = Features Register
	COUNT  = Count (was: Sector Count) Register
	LBA_48 = Upper bytes of LBA High/Mid/Low Registers ]  ATA-8
	LH     = LBA High (was: Cylinder High) Register    ]   LBA
	LM     = LBA Mid (was: Cylinder Low) Register      ] Register
	LL     = LBA Low (was: Sector Number) Register     ]
	DV     = Device (was: Device/Head) Register
	DC     = Device Control Register
	ER     = Error register
	ST     = Status register
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 65282 [1] occurred at disk power-on lifetime: 17294 hours (720 days + 14 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 01 00 01 a1 00 ce 5f 40 00  Error: UNC 1 sectors at LBA = 0x1a100ce5f = 6996151903

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 08 00 01 a1 00 ce 58 40 00     00:22:03.520  READ DMA EXT
  25 00 00 00 08 00 01 a1 00 ce 58 40 00     00:21:58.830  READ DMA EXT
  25 00 00 00 08 00 01 a1 00 ce 58 40 00     00:21:54.218  READ DMA EXT
  2f 00 00 00 01 00 00 00 00 00 10 00 00     00:21:54.130  READ LOG EXT
  60 00 08 00 f8 00 01 a1 00 ce 58 40 00     00:21:49.518  READ FPDMA QUEUED

Error 65281 [0] occurred at disk power-on lifetime: 17294 hours (720 days + 14 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 01 00 01 a1 00 ce 5f 40 00  Error: UNC 1 sectors at LBA = 0x1a100ce5f = 6996151903

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 08 00 01 a1 00 ce 58 40 00     00:21:58.830  READ DMA EXT
  25 00 00 00 08 00 01 a1 00 ce 58 40 00     00:21:54.218  READ DMA EXT
  2f 00 00 00 01 00 00 00 00 00 10 00 00     00:21:54.130  READ LOG EXT
  60 00 08 00 f8 00 01 a1 00 ce 58 40 00     00:21:49.518  READ FPDMA QUEUED
  60 00 08 00 f0 00 01 a1 00 ce 50 40 00     00:21:49.518  READ FPDMA QUEUED

Error 65280 [255] occurred at disk power-on lifetime: 17294 hours (720 days + 14 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 01 00 01 a1 00 ce 5f 40 00  Error: UNC 1 sectors at LBA = 0x1a100ce5f = 6996151903

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 08 00 01 a1 00 ce 58 40 00     00:21:54.218  READ DMA EXT
  2f 00 00 00 01 00 00 00 00 00 10 00 00     00:21:54.130  READ LOG EXT
  60 00 08 00 f8 00 01 a1 00 ce 58 40 00     00:21:49.518  READ FPDMA QUEUED
  60 00 08 00 f0 00 01 a1 00 ce 50 40 00     00:21:49.518  READ FPDMA QUEUED
  60 00 08 00 e8 00 01 a1 00 ce 48 40 00     00:21:49.517  READ FPDMA QUEUED

Error 65279 [254] occurred at disk power-on lifetime: 17294 hours (720 days + 14 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 41 00 fb 00 01 a1 00 ce 5f 40 00  Error: UNC at LBA = 0x1a100ce5f = 6996151903

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 08 00 f8 00 01 a1 00 ce 58 40 00     00:21:49.518  READ FPDMA QUEUED
  60 00 08 00 f0 00 01 a1 00 ce 50 40 00     00:21:49.518  READ FPDMA QUEUED
  60 00 08 00 e8 00 01 a1 00 ce 48 40 00     00:21:49.517  READ FPDMA QUEUED
  60 00 08 00 e0 00 01 a1 00 ce 40 40 00     00:21:49.517  READ FPDMA QUEUED
  60 00 08 00 d8 00 01 a1 00 ce 38 40 00     00:21:49.517  READ FPDMA QUEUED

Error 65278 [253] occurred at disk power-on lifetime: 17294 hours (720 days + 14 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 01 71 00 01 a1 00 ce 5f 40 00  Error: UNC 369 sectors at LBA = 0x1a100ce5f = 6996151903

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 02 70 00 01 a0 00 ce 60 40 00     00:21:44.841  READ DMA EXT
  25 00 00 02 70 00 01 a0 00 ce 60 40 00     00:21:40.229  READ DMA EXT
  25 00 00 02 70 00 01 a0 00 ce 60 40 00     00:21:35.542  READ DMA EXT
  25 00 00 08 00 00 01 a2 00 ce d0 40 00     00:21:35.517  READ DMA EXT
  25 00 00 02 70 00 01 a0 00 ce 60 40 00     00:21:30.904  READ DMA EXT

Error 65277 [252] occurred at disk power-on lifetime: 17294 hours (720 days + 14 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 01 71 00 01 a1 00 ce 5f 40 00  Error: UNC 369 sectors at LBA = 0x1a100ce5f = 6996151903

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 02 70 00 01 a0 00 ce 60 40 00     00:21:40.229  READ DMA EXT
  25 00 00 02 70 00 01 a0 00 ce 60 40 00     00:21:35.542  READ DMA EXT
  25 00 00 08 00 00 01 a2 00 ce d0 40 00     00:21:35.517  READ DMA EXT
  25 00 00 02 70 00 01 a0 00 ce 60 40 00     00:21:30.904  READ DMA EXT
  2f 00 00 00 01 00 00 00 00 00 10 00 00     00:21:30.828  READ LOG EXT

Error 65276 [251] occurred at disk power-on lifetime: 17294 hours (720 days + 14 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 01 71 00 01 a1 00 ce 5f 40 00  Error: UNC 369 sectors at LBA = 0x1a100ce5f = 6996151903

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 02 70 00 01 a0 00 ce 60 40 00     00:21:35.542  READ DMA EXT
  25 00 00 08 00 00 01 a2 00 ce d0 40 00     00:21:35.517  READ DMA EXT
  25 00 00 02 70 00 01 a0 00 ce 60 40 00     00:21:30.904  READ DMA EXT
  2f 00 00 00 01 00 00 00 00 00 10 00 00     00:21:30.828  READ LOG EXT
  60 08 00 00 d0 00 01 a2 00 ce d0 40 00     00:21:26.219  READ FPDMA QUEUED

Error 65275 [250] occurred at disk power-on lifetime: 17294 hours (720 days + 14 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 01 71 00 01 a1 00 ce 5f 40 00  Error: UNC 369 sectors at LBA = 0x1a100ce5f = 6996151903

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 02 70 00 01 a0 00 ce 60 40 00     00:21:30.904  READ DMA EXT
  2f 00 00 00 01 00 00 00 00 00 10 00 00     00:21:30.828  READ LOG EXT
  60 08 00 00 d0 00 01 a2 00 ce d0 40 00     00:21:26.219  READ FPDMA QUEUED
  60 02 70 00 c8 00 01 a0 00 ce 60 40 00     00:21:26.219  READ FPDMA QUEUED
  60 04 10 00 c0 00 01 9a 00 ce d0 40 00     00:21:26.204  READ FPDMA QUEUED

SMART Extended Self-test Log Version: 1 (2 sectors)
No self-tests have been logged.  [To run self-tests, use: smartctl -t]

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Status Version:                  2
SCT Version (vendor specific):       0 (0x0000)
Device State:                        Active (0)
Current Temperature:                    27 Celsius
Power Cycle Min/Max Temperature:     21/27 Celsius
Lifetime    Min/Max Temperature:     10/67 Celsius
Under/Over Temperature Limit Count:   0/0

SCT Temperature History Version:     2
Temperature Sampling Period:         1 minute
Temperature Logging Interval:        1 minute
Min/Max recommended Temperature:      5/60 Celsius
Min/Max Temperature Limit:           -40/65 Celsius
Temperature History Size (Index):    478 (453)

SCT Error Recovery Control:
           Read: Disabled
          Write: Disabled

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11)
ID      Size     Value  Description
0x0001  4            0  Command failed due to ICRC error
0x0002  4            0  R_ERR response for data FIS
0x0003  4            0  R_ERR response for device-to-host data FIS
0x0004  4            0  R_ERR response for host-to-device data FIS
0x0005  4            0  R_ERR response for non-data FIS
0x0006  4            0  R_ERR response for device-to-host non-data FIS
0x0008  4            0  Device-to-host non-data FIS retries
0x0009  4            3  Transition from drive PhyRdy to drive PhyNRdy
0x000a  4            3  Device-to-host register FISes sent due to a COMRESET
0x000b  4            0  CRC errors within host-to-device FIS
0x000d  4            0  Non-CRC errors within host-to-device FIS
0x000f  4            0  R_ERR response for host-to-device data FIS, CRC
0x0010  4            0  R_ERR response for host-to-device data FIS, non-CRC

