smartctl 7.3 2022-02-28 r5338 [FreeBSD 12.3-RELEASE amd64] (local build)
Copyright (C) 2002-22, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Seagate Constellation ES.3
Device Model:     ST4000NM0033-9ZM170
Serial Number:    --
LU WWN Device Id: 5 000c50 ...
Firmware Version: SN04
User Capacity:    4,000,787,030,016 bytes [4.00 TB]
Sector Size:      512 bytes logical/physical
Rotation Rate:    7200 rpm
Form Factor:      3.5 inches
Device is:        In smartctl database 7.3/5319
ATA Version is:   ACS-2 (minor revision not indicated)
SATA Version is:  SATA 3.0, 6.0 Gb/s (current: 3.0 Gb/s)
Local Time is:    Tue Oct  4 10:54:04 2022 CEST
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Unavailable
APM feature is:   Unavailable
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, frozen [SEC2]
Wt Cache Reorder: Enabled

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x82)	Offline data collection activity
					was completed without error.
					Auto Offline Data Collection: Enabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(  584) seconds.
Offline data collection
capabilities: 			 (0x7b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   1) minutes.
Extended self-test routine
recommended polling time: 	 ( 494) minutes.
Conveyance self-test routine
recommended polling time: 	 (   2) minutes.
SCT capabilities: 	       (0x50bd)	SCT Status supported.
					SCT Error Recovery Control supported.
					SCT Feature Control supported.
					SCT Data Table supported.

SMART Attributes Data Structure revision number: 10
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     POSR--   072   063   044    -    15291137
  3 Spin_Up_Time            PO----   092   091   000    -    0
  4 Start_Stop_Count        -O--CK   100   100   020    -    37
  5 Reallocated_Sector_Ct   PO--CK   093   093   010    -    1273
  7 Seek_Error_Rate         POSR--   095   060   030    -    3472874972
  9 Power_On_Hours          -O--CK   038   038   000    -    54843
 10 Spin_Retry_Count        PO--C-   100   100   097    -    0
 12 Power_Cycle_Count       -O--CK   100   100   020    -    42
184 End-to-End_Error        -O--CK   100   100   099    -    0
187 Reported_Uncorrect      -O--CK   074   074   000    -    26
188 Command_Timeout         -O--CK   100   097   000    -    12885098500
189 High_Fly_Writes         -O-RCK   100   100   000    -    0
190 Airflow_Temperature_Cel -O---K   057   048   045    -    43 (Min/Max 43/48)
191 G-Sense_Error_Rate      -O--CK   100   100   000    -    0
192 Power-Off_Retract_Count -O--CK   100   100   000    -    32
193 Load_Cycle_Count        -O--CK   099   099   000    -    2304
194 Temperature_Celsius     -O---K   043   052   000    -    43 (0 18 0 0 0)
195 Hardware_ECC_Recovered  -O-RC-   012   005   000    -    15291137
197 Current_Pending_Sector  -O--C-   098   097   000    -    421
198 Offline_Uncorrectable   ----C-   098   097   000    -    421
199 UDMA_CRC_Error_Count    -OSRCK   200   200   000    -    0
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory Version 1
SMART           Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00       GPL,SL  R/O      1  Log Directory
0x01           SL  R/O      1  Summary SMART error log
0x02           SL  R/O      5  Comprehensive SMART error log
0x03       GPL     R/O      5  Ext. Comprehensive SMART error log
0x06           SL  R/O      1  SMART self-test log
0x07       GPL     R/O      1  Extended self-test log
0x08       GPL,SL  R/O      2  Power Conditions log
0x09           SL  R/W      1  Selective self-test log
0x10       GPL     R/O      1  NCQ Command Error log
0x11       GPL     R/O      1  SATA Phy Event Counters log
0x21       GPL     R/O      1  Write stream error log
0x22       GPL     R/O      1  Read stream error log
0x24       GPL     R/O    512  Current Device Internal Status Data log
0x30       GPL,SL  R/O      9  IDENTIFY DEVICE data log
0x80-0x9f  GPL,SL  R/W     16  Host vendor specific log
0xa1       GPL,SL  VS      20  Device vendor specific log
0xa2       GPL     VS    4496  Device vendor specific log
0xa8       GPL,SL  VS     129  Device vendor specific log
0xa9       GPL,SL  VS       1  Device vendor specific log
0xb0       GPL     VS    5176  Device vendor specific log
0xbd       GPL     VS     512  Device vendor specific log
0xbe-0xbf  GPL     VS   65535  Device vendor specific log
0xc1       GPL,SL  VS      10  Device vendor specific log
0xc2       GPL,SL  VS      50  Device vendor specific log
0xc3       GPL,SL  VS       8  Device vendor specific log
0xc4       GPL,SL  VS       5  Device vendor specific log
0xd1       GPL,SL  VS       8  Device vendor specific log
0xe0       GPL,SL  R/W      1  SCT Command/Status
0xe1       GPL,SL  R/W      1  SCT Data Transfer

SMART Extended Comprehensive Error Log Version: 1 (5 sectors)
Device Error Count: 26 (device log contains only the most recent 20 errors)
	CR     = Command Register
	FEATR  = Features Register
	COUNT  = Count (was: Sector Count) Register
	LBA_48 = Upper bytes of LBA High/Mid/Low Registers ]  ATA-8
	LH     = LBA High (was: Cylinder High) Register    ]   LBA
	LM     = LBA Mid (was: Cylinder Low) Register      ] Register
	LL     = LBA Low (was: Sector Number) Register     ]
	DV     = Device (was: Device/Head) Register
	DC     = Device Control Register
	ER     = Error register
	ST     = Status register
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 26 [5] occurred at disk power-on lifetime: 51391 hours (2141 days + 7 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 01 39 f7 b4 9f 00 00  Error: UNC at LBA = 0x139f7b49f = 5267502239

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 04 00 00 01 39 f7 b2 00 40 00 11d+06:33:03.570  READ DMA EXT
  ea 00 00 00 00 00 00 00 00 00 00 00 00 11d+06:33:03.545  FLUSH CACHE EXT
  25 00 00 04 00 00 01 39 f7 ae 00 40 00 11d+06:33:02.668  READ DMA EXT
  35 00 00 00 80 00 01 c9 00 2a 00 40 00 11d+06:33:02.667  WRITE DMA EXT
  35 00 00 00 d0 00 01 c9 00 29 00 40 00 11d+06:33:02.666  WRITE DMA EXT

Error 25 [4] occurred at disk power-on lifetime: 51387 hours (2141 days + 3 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 01 3a 07 9a 3a 00 00  Error: UNC at LBA = 0x13a079a3a = 5268544058

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 04 00 00 01 3a 07 99 00 40 00 11d+02:20:44.897  READ DMA EXT
  35 00 00 00 80 00 01 c8 c4 dc 00 40 00 11d+02:20:44.896  WRITE DMA EXT
  35 00 00 00 08 00 00 00 00 08 80 40 00 11d+02:20:44.896  WRITE DMA EXT
  35 00 00 00 10 00 01 a1 d8 fd 00 40 00 11d+02:20:44.895  WRITE DMA EXT
  35 00 00 00 08 00 01 c8 c4 d8 80 40 00 11d+02:20:44.895  WRITE DMA EXT

Error 24 [3] occurred at disk power-on lifetime: 51387 hours (2141 days + 3 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 01 3a 07 32 2a 00 00  Error: UNC at LBA = 0x13a07322a = 5268517418

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 04 00 00 01 3a 07 2f 80 40 00 11d+02:20:40.733  READ DMA EXT
  25 00 00 00 08 00 01 3a 07 0a 80 40 00 11d+02:20:40.726  READ DMA EXT
  25 00 00 00 08 00 01 3a 06 a4 80 40 00 11d+02:20:40.721  READ DMA EXT
  25 00 00 00 08 00 01 3a 06 1c 80 40 00 11d+02:20:40.718  READ DMA EXT
  25 00 00 00 08 00 01 3a 05 f6 80 40 00 11d+02:20:40.712  READ DMA EXT

Error 23 [2] occurred at disk power-on lifetime: 51367 hours (2140 days + 7 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 01 39 f8 9c ce 00 00  Error: UNC at LBA = 0x139f89cce = 5267561678

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 04 00 00 01 39 f8 9c 80 40 00 10d+06:00:47.641  READ DMA EXT
  25 00 00 00 08 00 01 39 f7 ee 80 40 00 10d+06:00:47.600  READ DMA EXT
  25 00 00 00 08 00 01 39 f7 01 00 40 00 10d+06:00:47.594  READ DMA EXT
  25 00 00 04 00 00 01 39 f6 86 80 40 00 10d+06:00:47.579  READ DMA EXT
  25 00 00 04 00 00 01 39 f6 82 80 40 00 10d+06:00:47.575  READ DMA EXT

Error 22 [1] occurred at disk power-on lifetime: 51367 hours (2140 days + 7 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 01 39 f7 86 44 00 00  Error: UNC at LBA = 0x139f78644 = 5267490372

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 04 00 00 01 39 f7 86 00 40 00 10d+05:42:44.334  READ DMA EXT
  25 00 00 00 08 00 01 39 f6 97 00 40 00 10d+05:42:44.325  READ DMA EXT
  25 00 00 00 10 00 01 39 f5 69 80 40 00 10d+05:42:44.321  READ DMA EXT
  25 00 00 04 00 00 01 39 f4 8c 00 40 00 10d+05:42:44.306  READ DMA EXT
  25 00 00 04 00 00 01 39 f4 88 00 40 00 10d+05:42:44.302  READ DMA EXT

Error 21 [0] occurred at disk power-on lifetime: 51364 hours (2140 days + 4 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 01 39 f8 1a bf 00 00  Error: UNC at LBA = 0x139f81abf = 5267528383

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 04 00 00 01 39 f8 19 80 40 00 10d+02:48:44.052  READ DMA EXT
  25 00 00 00 08 00 01 39 f7 c6 80 40 00 10d+02:48:44.045  READ DMA EXT
  25 00 00 00 08 00 01 39 f7 02 00 40 00 10d+02:48:44.042  READ DMA EXT
  25 00 00 00 08 00 01 39 f6 db 00 40 00 10d+02:48:44.034  READ DMA EXT
  25 00 00 00 08 00 01 39 f6 53 80 40 00 10d+02:48:44.025  READ DMA EXT

Error 20 [19] occurred at disk power-on lifetime: 51363 hours (2140 days + 3 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 01 39 f8 10 6e 00 00  Error: UNC at LBA = 0x139f8106e = 5267525742

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 04 00 00 01 39 f8 0c 80 40 00 10d+02:03:45.413  READ DMA EXT
  25 00 00 04 00 00 01 39 f8 08 80 40 00 10d+02:03:44.768  READ DMA EXT
  25 00 00 04 00 00 01 39 f8 04 80 40 00 10d+02:03:43.665  READ DMA EXT
  25 00 00 04 00 00 01 39 f8 00 80 40 00 10d+02:03:43.170  READ DMA EXT
  25 00 00 04 00 00 01 39 f7 fc 80 40 00 10d+02:03:41.974  READ DMA EXT

Error 19 [18] occurred at disk power-on lifetime: 51333 hours (2138 days + 21 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 01 39 ef b3 23 00 00  Error: UNC at LBA = 0x139efb323 = 5266977571

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 04 00 00 01 39 ef b3 00 40 00  8d+20:23:37.011  READ DMA EXT
  25 00 00 04 00 00 01 39 ed e4 80 40 00  8d+20:23:36.995  READ DMA EXT
  25 00 00 04 00 00 01 39 ed e0 80 40 00  8d+20:23:36.992  READ DMA EXT
  25 00 00 04 00 00 01 39 ed dc 80 40 00  8d+20:23:36.988  READ DMA EXT
  25 00 00 04 00 00 01 39 ed d8 80 40 00  8d+20:23:36.984  READ DMA EXT

SMART Extended Self-test Log Version: 1 (1 sectors)
No self-tests have been logged.  [To run self-tests, use: smartctl -t]

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Status Version:                  3
SCT Version (vendor specific):       522 (0x020a)
Device State:                        Active (0)
Current Temperature:                    43 Celsius
Power Cycle Min/Max Temperature:     43/48 Celsius
Lifetime    Min/Max Temperature:     18/52 Celsius
Under/Over Temperature Limit Count:   0/212

SCT Temperature History Version:     2
Temperature Sampling Period:         1 minute
Temperature Logging Interval:        10 minutes
Min/Max recommended Temperature:      0/ 0 Celsius
Min/Max Temperature Limit:            0/ 0 Celsius
Temperature History Size (Index):    128 (115)

SCT Error Recovery Control:
           Read:    100 (10.0 seconds)
          Write:    100 (10.0 seconds)

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11)
ID      Size     Value  Description
0x000a  2            3  Device-to-host register FISes sent due to a COMRESET
0x0001  2            0  Command failed due to ICRC error
0x0003  2            0  R_ERR response for device-to-host data FIS
0x0004  2            0  R_ERR response for host-to-device data FIS
0x0006  2            0  R_ERR response for device-to-host non-data FIS
0x0007  2            0  R_ERR response for host-to-device non-data FIS



