smartctl 7.3 2022-02-28 r5338 [FreeBSD 13.1-RC3 amd64] (local build)
Copyright (C) 2002-22, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Seagate Momentus 5400.3
Device Model:     ST9160821AS
Serial Number:    --
Firmware Version: 3.ALC
User Capacity:    160,041,885,696 bytes [160 GB]
Sector Size:      512 bytes logical/physical
Device is:        In smartctl database 7.3/5319
ATA Version is:   ATA/ATAPI-7 (minor revision not indicated)
Local Time is:    Sun May  8 15:06:23 2022 EDT
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Unavailable
APM level is:     128 (minimum power consumption without standby)
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, frozen [SEC2]
Wt Cache Reorder: Unavailable

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED
See vendor-specific Attribute list for marginal Attributes.

General SMART Values:
Offline data collection status:  (0x82)	Offline data collection activity
					was completed without error.
					Auto Offline Data Collection: Enabled.
Self-test execution status:      (  24)	The self-test routine was aborted by
					the host.
Total time to complete Offline 
data collection: 		(  426) seconds.
Offline data collection
capabilities: 			 (0x5b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					No Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					No General Purpose Logging support.
Short self-test routine 
recommended polling time: 	 (   1) minutes.
Extended self-test routine
recommended polling time: 	 ( 111) minutes.
SCT capabilities: 	       (0x0001)	SCT Status supported.

SMART Attributes Data Structure revision number: 10
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     POSR--   118   093   006    -    188213950
  3 Spin_Up_Time            PO----   099   099   000    -    0
  4 Start_Stop_Count        -O--CK   094   094   020    -    6396
  5 Reallocated_Sector_Ct   PO--CK   100   100   036    -    1
  7 Seek_Error_Rate         POSR--   072   060   030    -    327415158068
  9 Power_On_Hours          -O--CK   075   075   000    -    22686
 10 Spin_Retry_Count        PO--C-   100   100   034    -    0
 12 Power_Cycle_Count       -O--CK   094   094   020    -    6540
187 Reported_Uncorrect      -O--CK   087   087   000    -    13
189 High_Fly_Writes         -O-RCK   084   084   000    -    16
190 Airflow_Temperature_Cel -O---K   061   040   045    Past 39 (Min/Max 38/42)
192 Power-Off_Retract_Count -O--CK   099   099   000    -    2798
193 Load_Cycle_Count        -O--CK   001   001   000    -    590568
194 Temperature_Celsius     -O---K   039   060   000    -    39 (0 13 0 0 0)
195 Hardware_ECC_Recovered  -O-RC-   085   054   000    -    202394141
197 Current_Pending_Sector  -O--C-   100   100   000    -    0
198 Offline_Uncorrectable   ----C-   100   100   000    -    0
199 UDMA_CRC_Error_Count    -OSRCK   200   200   000    -    1
200 Multi_Zone_Error_Rate   ------   100   253   000    -    0
202 Data_Address_Mark_Errs  -O--CK   100   253   000    -    0
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory not supported

SMART Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00           SL  R/O      1  Log Directory
0x01           SL  R/O      1  Summary SMART error log
0x02           SL  R/O      5  Comprehensive SMART error log
0x03           SL  R/O      5  Ext. Comprehensive SMART error log
0x06           SL  R/O      1  SMART self-test log
0x07           SL  R/O      1  Extended self-test log
0x09           SL  R/W      1  Selective self-test log
0x10           SL  R/O      1  NCQ Command Error log
0x11           SL  R/O      1  SATA Phy Event Counters log
0x20           SL  R/O      1  Streaming performance log [OBS-8]
0x21           SL  R/O      1  Write stream error log
0x22           SL  R/O      1  Read stream error log
0x23           SL  R/O      1  Delayed sector log [OBS-8]
0x80-0x9f      SL  R/W     16  Host vendor specific log
0xa0           SL  VS       1  Device vendor specific log
0xa1           SL  VS      20  Device vendor specific log
0xa2           SL  VS     101  Device vendor specific log
0xa8           SL  VS      20  Device vendor specific log
0xa9           SL  VS       1  Device vendor specific log
0xe0           SL  R/W      1  SCT Command/Status
0xe1           SL  R/W      1  SCT Data Transfer

SMART Extended Comprehensive Error Log (GP Log 0x03) not supported

SMART Error Log Version: 1
ATA Error Count: 13 (device log contains only the most recent five errors)
	CR = Command Register [HEX]
	FR = Features Register [HEX]
	SC = Sector Count Register [HEX]
	SN = Sector Number Register [HEX]
	CL = Cylinder Low Register [HEX]
	CH = Cylinder High Register [HEX]
	DH = Device/Head Register [HEX]
	DC = Device Command Register [HEX]
	ER = Error register [HEX]
	ST = Status register [HEX]
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 13 occurred at disk power-on lifetime: 10983 hours (457 days + 15 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  40 51 00 6c 52 94 e0  Error: UNC at LBA = 0x0094526c = 9720428

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  25 00 08 65 52 94 e0 00      00:01:11.661  READ DMA EXT
  35 00 00 60 72 be e0 00      00:01:11.660  WRITE DMA EXT
  35 00 00 60 71 be e0 00      00:01:11.658  WRITE DMA EXT
  35 00 00 60 70 be e0 00      00:01:11.657  WRITE DMA EXT
  35 00 00 60 6f be e0 00      00:01:11.656  WRITE DMA EXT

Error 12 occurred at disk power-on lifetime: 10983 hours (457 days + 15 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  40 51 00 6c 52 94 e0  Error: UNC at LBA = 0x0094526c = 9720428

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  25 00 08 65 52 94 e0 00      00:01:09.356  READ DMA EXT
  25 00 08 6d 52 94 e0 00      00:01:09.355  READ DMA EXT
  35 00 00 60 6a be e0 00      00:01:09.354  WRITE DMA EXT
  35 00 00 60 69 be e0 00      00:01:09.352  WRITE DMA EXT
  35 00 00 60 68 be e0 00      00:01:09.351  WRITE DMA EXT

Error 11 occurred at disk power-on lifetime: 10983 hours (457 days + 15 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  40 51 00 6c 52 94 e0  Error: UNC at LBA = 0x0094526c = 9720428

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  25 00 08 65 52 94 e0 00      00:01:07.070  READ DMA EXT
  35 00 00 60 62 be e0 00      00:01:07.069  WRITE DMA EXT
  35 00 00 60 61 be e0 00      00:01:07.068  WRITE DMA EXT
  35 00 00 60 60 be e0 00      00:01:07.067  WRITE DMA EXT
  35 00 00 60 5f be e0 00      00:01:07.067  WRITE DMA EXT

Error 10 occurred at disk power-on lifetime: 10983 hours (457 days + 15 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  40 51 00 6c 52 94 e0  Error: UNC at LBA = 0x0094526c = 9720428

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  25 00 08 65 52 94 e0 00      00:01:04.784  READ DMA EXT
  25 00 08 5d 52 94 e0 00      00:01:04.783  READ DMA EXT
  35 00 00 60 5a be e0 00      00:01:04.783  WRITE DMA EXT
  35 00 00 60 59 be e0 00      00:01:04.782  WRITE DMA EXT
  35 00 00 60 58 be e0 00      00:01:04.686  WRITE DMA EXT

Error 9 occurred at disk power-on lifetime: 10983 hours (457 days + 15 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  40 51 00 6c 52 94 e0  Error: UNC at LBA = 0x0094526c = 9720428

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  25 00 80 0d 52 94 e0 00      00:01:01.847  READ DMA EXT
  25 00 08 8d 51 94 e0 00      00:01:01.846  READ DMA EXT
  35 00 00 60 0a be e0 00      00:01:01.846  WRITE DMA EXT
  35 00 00 60 09 be e0 00      00:01:01.846  WRITE DMA EXT
  35 00 00 60 08 be e0 00      00:01:01.868  WRITE DMA EXT

SMART Extended Self-test Log (GP Log 0x07) not supported

SMART Self-test log structure revision number 1
Num  Test_Description    Status                  Remaining  LifeTime(hours)  LBA_of_first_error
# 1  Short offline       Aborted by host               80%     15162         -
# 2  Short offline       Aborted by host               80%     15162         -

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Status Version:                  2
SCT Version (vendor specific):       521 (0x0209)
Device State:                        Active (0)
Current Temperature:                    39 Celsius
Power Cycle Min/Max Temperature:     --/ 0 Celsius
Lifetime    Min/Max Temperature:     --/ 0 Celsius

SCT Data Table command not supported

SCT Error Recovery Control command not supported

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11)
ID      Size     Value  Description
0x000a  2           11  Device-to-host register FISes sent due to a COMRESET
0x0001  2            0  Command failed due to ICRC error
0x0003  2            0  R_ERR response for device-to-host data FIS
0x0004  2            0  R_ERR response for host-to-device data FIS
0x0006  2            0  R_ERR response for device-to-host non-data FIS
0x0007  2            0  R_ERR response for host-to-device non-data FIS
0x0009  2           10  Transition from drive PhyRdy to drive PhyNRdy
0x8002  2            0  Vendor specific
0x8003  2            3  Vendor specific
0x8004  2            0  Vendor specific

