smartctl 7.1 2019-12-30 r5022 [x86_64-unknown-openbsd6.8] (local build)
Copyright (C) 2002-19, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Device Model:     KINGSTON SMSM151S3128GD
Serial Number:    --
Firmware Version: S9FM01.8
User Capacity:    128,035,676,160 bytes [128 GB]
Sector Size:      512 bytes logical/physical
Rotation Rate:    Solid State Device
Form Factor:      2.5 inches
Device is:        Not in smartctl database [for details use: -P showall]
ATA Version is:   ACS-3 (minor revision not indicated)
SATA Version is:  SATA 3.1, 6.0 Gb/s (current: 6.0 Gb/s)
Local Time is:    Sun Oct 18 21:48:55 2020 PDT
SMART support is: Available - device has SMART capability.
SMART support is: Enabled

=== START OF READ SMART DATA SECTION ===
SMART Status not supported: Incomplete response, ATA output registers missing
SMART overall-health self-assessment test result: PASSED
Warning: This result is based on an Attribute check.

General SMART Values:
Offline data collection status:  (0x00)	Offline data collection activity
					was never started.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(   30) seconds.
Offline data collection
capabilities: 			 (0x7b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   1) minutes.
Extended self-test routine
recommended polling time: 	 (   2) minutes.
Conveyance self-test routine
recommended polling time: 	 (   2) minutes.

SMART Attributes Data Structure revision number: 16
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAG     VALUE WORST THRESH TYPE      UPDATED  WHEN_FAILED RAW_VALUE
  1 Raw_Read_Error_Rate     0x000a   099   099   000    Old_age   Always       -       113
  2 Throughput_Performance  0x0005   100   100   050    Pre-fail  Offline      -       0
  3 Spin_Up_Time            0x0007   100   100   050    Pre-fail  Always       -       0
  5 Reallocated_Sector_Ct   0x0013   100   100   050    Pre-fail  Always       -       0
  7 Unknown_SSD_Attribute   0x000b   100   100   050    Pre-fail  Always       -       0
  8 Unknown_SSD_Attribute   0x0005   100   100   050    Pre-fail  Offline      -       0
  9 Power_On_Hours          0x0012   100   100   000    Old_age   Always       -       14370
 10 Unknown_SSD_Attribute   0x0013   100   100   050    Pre-fail  Always       -       0
 12 Power_Cycle_Count       0x0012   100   100   000    Old_age   Always       -       7320
167 Unknown_Attribute       0x0022   100   100   000    Old_age   Always       -       0
168 Unknown_Attribute       0x0012   100   100   000    Old_age   Always       -       0
169 Unknown_Attribute       0x0000   100   100   000    Old_age   Offline      -       70
170 Unknown_Attribute       0x0013   100   100   010    Pre-fail  Always       -       43
172 Unknown_Attribute       0x0032   100   100   000    Old_age   Always       -       0
173 Unknown_Attribute       0x0000   100   100   000    Old_age   Offline      -       26280080
175 Program_Fail_Count_Chip 0x0013   100   100   010    Pre-fail  Always       -       0
181 Program_Fail_Cnt_Total  0x0012   100   100   000    Old_age   Always       -       0
187 Reported_Uncorrect      0x0032   100   100   000    Old_age   Always       -       5
192 Power-Off_Retract_Count 0x0012   100   100   000    Old_age   Always       -       137
196 Reallocated_Event_Count 0x0000   100   100   000    Old_age   Offline      -       2
197 Current_Pending_Sector  0x0032   100   100   000    Old_age   Always       -       0
199 UDMA_CRC_Error_Count    0x0032   100   100   000    Old_age   Always       -       0
218 Unknown_Attribute       0x0000   100   100   000    Old_age   Offline      -       0
233 Media_Wearout_Indicator 0x0013   100   100   000    Pre-fail  Always       -       14528931
240 Unknown_SSD_Attribute   0x0013   100   100   050    Pre-fail  Always       -       0
241 Total_LBAs_Written      0x0012   100   100   000    Old_age   Always       -       8338138
242 Total_LBAs_Read         0x0012   100   100   000    Old_age   Always       -       7039109
243 Unknown_Attribute       0x0012   100   100   000    Old_age   Always       -       110382343808100
244 Unknown_Attribute       0x0000   100   100   000    Old_age   Offline      -       144
245 Unknown_Attribute       0x0000   100   100   000    Old_age   Offline      -       401

SMART Error Log Version: 1
No Errors Logged

SMART Self-test log structure revision number 1
No self-tests have been logged.  [To run self-tests, use: smartctl -t]

SMART Selective self-test log data structure revision number 0
Note: revision number not 1 implies that no selective self-test has ever been run
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.



