smartctl 7.3 2022-02-28 r5338 [FreeBSD 13.1-RELEASE-p1 amd64] (local build)
Copyright (C) 2002-22, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Device Model:     Innodisk DEMSR- 16GB mSATA 3ME3
Serial Number:    --
LU WWN Device Id: 5 24693e ...
Firmware Version: S16425G3
User Capacity:    16,013,942,784 bytes [16.0 GB]
Sector Size:      512 bytes logical/physical
Rotation Rate:    Solid State Device
Form Factor:      2.5 inches
TRIM Command:     Available
Device is:        Not in smartctl database 7.3/5319
ATA Version is:   ATA8-ACS (minor revision not indicated)
SATA Version is:  SATA 3.0, 6.0 Gb/s (current: 6.0 Gb/s)
Local Time is:    Sat Sep 10 19:23:01 2022 CEST
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Unavailable
APM feature is:   Unavailable
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, NOT FROZEN [SEC1]
Read SCT Status failed: Input/output error
Wt Cache Reorder: Unknown (SCT Feature Control command failed)

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x00)	Offline data collection activity
					was never started.
					Auto Offline Data Collection: Disabled.
Total time to complete Offline 
data collection: 		(   32) seconds.
Offline data collection
capabilities: 			 (0x00) 	Offline data collection not supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x00)	Error logging NOT supported.
					No General Purpose Logging support.
SCT capabilities: 	       (0x0039)	SCT Status supported.
					SCT Error Recovery Control supported.
					SCT Feature Control supported.
					SCT Data Table supported.

SMART Attributes Data Structure revision number: 16
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     ------   000   000   000    -    0
  2 Throughput_Performance  ------   000   000   000    -    0
  3 Spin_Up_Time            ------   000   000   000    -    0
  5 Reallocated_Sector_Ct   PO--C-   100   100   001    -    0
  7 Unknown_SSD_Attribute   ------   000   000   000    -    0
  8 Unknown_SSD_Attribute   ------   000   000   000    -    0
  9 Power_On_Hours          -O----   141   000   000    -    2701
 10 Unknown_SSD_Attribute   ------   000   000   000    -    0
 12 Power_Cycle_Count       -O----   093   000   000    -    349
163 Unknown_Attribute       ------   000   000   000    -    7
168 Unknown_Attribute       ------   000   000   000    -    0
169 Unknown_Attribute       ------   099   000   000    -    99
175 Program_Fail_Count_Chip ------   000   000   000    -    0
192 Power-Off_Retract_Count ------   000   000   000    -    0
194 Temperature_Celsius     ------   030   100   000    -    30 (2 100 0 0 0)
197 Current_Pending_Sector  -O--C-   000   100   000    -    0
225 Unknown_SSD_Attribute   ------   000   170   000    -    720891
240 Unknown_SSD_Attribute   ------   000   000   000    -    0
165 Unknown_Attribute       -O----   033   001   000    -    33
167 Unknown_Attribute       -O----   021   001   000    -    21
170 Unknown_Attribute       PO----   100   001   000    -    71
171 Unknown_Attribute       -O----   000   001   000    -    0
172 Unknown_Attribute       -O----   000   001   000    -    0
176 Erase_Fail_Count_Chip   ------   100   001   000    -    0
187 Reported_Uncorrect      -O----   000   001   000    -    0
229 Unknown_Attribute       -O----   100   001   000    -    89569723997848
232 Available_Reservd_Space PO----   100   001   000    -    0
235 Unknown_Attribute       -O----   000   000   000    -    0
241 Total_LBAs_Written      -O----   100   001   000    -    2815
242 Total_LBAs_Read         -O----   100   001   000    -    2876
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

Read SMART Log Directory failed: Input/output error

General Purpose Log Directory not supported

SMART Extended Comprehensive Error Log (GP Log 0x03) not supported

SMART Error Log not supported

SMART Extended Self-test Log (GP Log 0x07) not supported

SMART Self-test Log not supported

Selective Self-tests/Logging not supported

Read SCT Status failed: Input/output error

Read SCT Status failed: Input/output error
SCT (Get) Error Recovery Control command failed

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11)
ID      Size     Value  Description
0x0001  2            0  Command failed due to ICRC error
0x0003  2            0  R_ERR response for device-to-host data FIS
0x0004  2            0  R_ERR response for host-to-device data FIS
0x0006  2            0  R_ERR response for device-to-host non-data FIS
0x0007  2            0  R_ERR response for host-to-device non-data FIS
0x0008  2            0  Device-to-host non-data FIS retries
0x0009  4            0  Transition from drive PhyRdy to drive PhyNRdy
0x000a  4            3  Device-to-host register FISes sent due to a COMRESET
0x000f  2            0  R_ERR response for host-to-device data FIS, CRC
0x0010  2            0  R_ERR response for host-to-device data FIS, non-CRC
0x0012  2            0  R_ERR response for host-to-device non-data FIS, CRC
0x0013  2            0  R_ERR response for host-to-device non-data FIS, non-CRC

