Innodisk Solid State Drives
===========================

This is a list of all tested Innodisk solid state drive models and their MTBFs. See
more info on reliability test in the [README](https://github.com/bsdhw/SMART).

Contents
--------

1. [ SSD by Model  ](#ssd-by-model)
2. [ SSD by Family ](#ssd-by-family)

SSD by Model
------------

Please take all columns into account when reading the table. Pay attention on the
number of tested samples and power-on days. Simultaneous high values of both MTBF
and errors are possible if only rare drives in the subset encounter errors.

Days - avg. days per sample,
Err  - avg. errors per sample,
MTBF - avg. MTBF in years per sample.

| MFG       | Model              | Size   | Samples | Days  | Err   | MTBF |
|-----------|--------------------|--------|---------|-------|-------|------|
| Innodisk  | Corp. - mSATA 3ME4 | 16 GB  | 1       | 1456  | 0     | 3.99   |
| Innodisk  | Corp. DRPS-08GJ... | 8 GB   | 1       | 1364  | 0     | 3.74   |
| Innodisk  | M.2 (S42) 3ME4     | 64 GB  | 1       | 1101  | 0     | 3.02   |
| Innodisk  | DEMSR- 32GB mSA... | 32 GB  | 1       | 956   | 0     | 2.62   |
| Innodisk  | DEMSR- 08GB mSA... | 8 GB   | 3       | 876   | 0     | 2.40   |
| Innodisk  | DEMSR- 16GB mSA... | 16 GB  | 1       | 748   | 0     | 2.05   |
| Innodisk  | Corp. mSATA 3SE... | 2 GB   | 1       | 617   | 0     | 1.69   |
| Innodisk  | Corp. - mSATA 3IE3 | 64 GB  | 1       | 523   | 0     | 1.44   |
| Innodisk  | DEMSR- 16GB mSA... | 16 GB  | 4       | 448   | 0     | 1.23   |
| Innodisk  | mSATA mini 3ME4    | 64 GB  | 1       | 411   | 0     | 1.13   |
| Innodisk  | Corp. - mSATA 3ME3 | 32 GB  | 3       | 215   | 0     | 0.59   |
| Innodisk  | Corp. DRPS-16GJ... | 16 GB  | 1       | 187   | 0     | 0.51   |
| Innodisk  | DEMSR- 08GB mSA... | 8 GB   | 13      | 177   | 0     | 0.49   |
| Innodisk  | DEM24-16GM41BC1... | 16 GB  | 1       | 153   | 0     | 0.42   |
| Innodisk  | DEMSR-64GM41BC1... | 64 GB  | 1       | 152   | 0     | 0.42   |
| Innodisk  | Corp. - mSATA 3... | 64 GB  | 1       | 74    | 0     | 0.20   |
| Innodisk  | DEM24-32GM41BC1... | 32 GB  | 1       | 67    | 0     | 0.19   |
| Innodisk  | 2.5" SATA SSD 3ME2 | 128 GB | 1       | 187   | 15    | 0.03   |
| Innodisk  | CFast 3ME3         | 128 GB | 1       | 10    | 0     | 0.03   |
| Innodisk  | M.2 (S80) 3MG2-P   | 992 GB | 1       | 7     | 0     | 0.02   |
| Innodisk  | 2.5" SATA SSD 3... | 128 GB | 1       | 3     | 0     | 0.01   |

SSD by Family
-------------

Please take all columns into account when reading the table. Pay attention on the
number of tested samples and power-on days. Simultaneous high values of both MTBF
and errors are possible if only rare drives in the subset encounter errors.

Days - avg. days per sample,
Err  - avg. errors per sample,
MTBF - avg. MTBF in years per sample.

| MFG       | Family                 | Models | Samples | Days  | Err   | MTBF |
|-----------|------------------------|--------|---------|-------|-------|------|
| Innodisk  | 1IE3/3IE3/3ME3/3IE4... | 5      | 7       | 534   | 0     | 1.46   |
| Innodisk  | 3IE3/3ME3/3ME4 SSDs    | 1      | 1       | 411   | 0     | 1.13   |
| Innodisk  | Unknown                | 12     | 29      | 381   | 0     | 1.04   |
| Innodisk  | 3IE2/3ME2/3MG2/3SE2... | 2      | 2       | 97    | 8     | 0.03   |
| Innodisk  | 3IE2/3ME2/3MG2/3SE2... | 1      | 1       | 3     | 0     | 0.01   |
