smartctl 7.1 2019-12-30 r5022 [FreeBSD 12.1-RELEASE amd64] (local build)
Copyright (C) 2002-19, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Seagate Desktop SSHD
Device Model:     ST1000DX001-1CM162
Serial Number:    --
LU WWN Device Id: 5 000c50 ...
Firmware Version: CC43
User Capacity:    1,000,204,886,016 bytes [1.00 TB]
Sector Sizes:     512 bytes logical, 4096 bytes physical
Rotation Rate:    7200 rpm
Form Factor:      3.5 inches
Device is:        In smartctl database [for details use: -P show]
ATA Version is:   ACS-2, ACS-3 T13/2161-D revision 3b
SATA Version is:  SATA 3.1, 6.0 Gb/s (current: 6.0 Gb/s)
Local Time is:    Sat Mar 13 14:01:18 2021 EST
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Unavailable
APM level is:     128 (minimum power consumption without standby)
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, frozen [SEC2]
Wt Cache Reorder: Unavailable

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED
See vendor-specific Attribute list for marginal Attributes.

General SMART Values:
Offline data collection status:  (0x00)	Offline data collection activity
					was never started.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(  575) seconds.
Offline data collection
capabilities: 			 (0x73) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					No Offline surface scan supported.
					Self-test supported.
					Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   1) minutes.
Extended self-test routine
recommended polling time: 	 ( 112) minutes.
Conveyance self-test routine
recommended polling time: 	 (   2) minutes.
SCT capabilities: 	       (0x1081)	SCT Status supported.

SMART Attributes Data Structure revision number: 10
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     POSR--   110   091   006    -    26268808
  3 Spin_Up_Time            PO----   098   097   000    -    0
  4 Start_Stop_Count        -O--CK   098   098   020    -    2813
  5 Reallocated_Sector_Ct   PO--CK   100   100   010    -    0
  7 Seek_Error_Rate         POSR--   080   060   030    -    106497953
  9 Power_On_Hours          -O--CK   082   082   000    -    16131
 10 Spin_Retry_Count        PO--C-   100   100   097    -    0
 12 Power_Cycle_Count       -O--CK   097   097   020    -    3869
183 Runtime_Bad_Block       -O--CK   089   089   000    -    11
184 End-to-End_Error        -O--CK   099   099   099    NOW  1
187 Reported_Uncorrect      -O--CK   082   082   000    -    18
188 Command_Timeout         -O--CK   100   096   000    -    6 8 41
189 High_Fly_Writes         -O-RCK   100   100   000    -    0
190 Airflow_Temperature_Cel -O---K   065   052   045    -    35 (Min/Max 34/35)
191 G-Sense_Error_Rate      -O--CK   100   100   000    -    0
192 Power-Off_Retract_Count -O--CK   100   100   000    -    461
193 Load_Cycle_Count        -O--CK   096   096   000    -    8796
194 Temperature_Celsius     -O---K   035   048   000    -    35 (0 15 0 0 0)
197 Current_Pending_Sector  -O--C-   100   100   000    -    0
198 Offline_Uncorrectable   ----C-   100   100   000    -    0
199 UDMA_CRC_Error_Count    -OSRCK   200   192   000    -    188
240 Head_Flying_Hours       ------   100   253   000    -    25041h+07m+17.616s
241 Total_LBAs_Written      ------   100   253   000    -    24254591171
242 Total_LBAs_Read         ------   100   253   000    -    22311313780
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory Version 1
SMART           Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00       GPL,SL  R/O      1  Log Directory
0x01           SL  R/O      1  Summary SMART error log
0x02           SL  R/O      5  Comprehensive SMART error log
0x03       GPL     R/O      5  Ext. Comprehensive SMART error log
0x06           SL  R/O      1  SMART self-test log
0x07       GPL     R/O      1  Extended self-test log
0x09           SL  R/W      1  Selective self-test log
0x10       GPL     R/O      1  NCQ Command Error log
0x11       GPL     R/O      1  SATA Phy Event Counters log
0x21       GPL     R/O      1  Write stream error log
0x22       GPL     R/O      1  Read stream error log
0x30       GPL,SL  R/O      9  IDENTIFY DEVICE data log
0x80-0x9f  GPL,SL  R/W     16  Host vendor specific log
0xa1       GPL,SL  VS      20  Device vendor specific log
0xa2       GPL     VS    3900  Device vendor specific log
0xa8       GPL,SL  VS     129  Device vendor specific log
0xa9       GPL,SL  VS       1  Device vendor specific log
0xab       GPL     VS       1  Device vendor specific log
0xb0       GPL     VS    4580  Device vendor specific log
0xbe-0xbf  GPL     VS   65535  Device vendor specific log
0xc0       GPL,SL  VS       1  Device vendor specific log
0xc1       GPL,SL  VS      10  Device vendor specific log
0xc4       GPL,SL  VS       5  Device vendor specific log
0xe0       GPL,SL  R/W      1  SCT Command/Status
0xe1       GPL,SL  R/W      1  SCT Data Transfer

SMART Extended Comprehensive Error Log Version: 1 (5 sectors)
Device Error Count: 8
	CR     = Command Register
	FEATR  = Features Register
	COUNT  = Count (was: Sector Count) Register
	LBA_48 = Upper bytes of LBA High/Mid/Low Registers ]  ATA-8
	LH     = LBA High (was: Cylinder High) Register    ]   LBA
	LM     = LBA Mid (was: Cylinder Low) Register      ] Register
	LL     = LBA Low (was: Sector Number) Register     ]
	DV     = Device (was: Device/Head) Register
	DC     = Device Control Register
	ER     = Error register
	ST     = Status register
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 8 [7] occurred at disk power-on lifetime: 862 hours (35 days + 22 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 32 03 e9 c8 00 00  Error: UNC at LBA = 0x3203e9c8 = 839117256

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 00 08 00 00 32 03 e9 c5 40 00     06:12:06.278  READ FPDMA QUEUED
  60 00 00 00 18 00 00 27 54 32 40 40 00     06:12:06.278  READ FPDMA QUEUED
  60 00 00 00 18 00 00 27 54 32 20 40 00     06:12:06.278  READ FPDMA QUEUED
  60 00 00 00 10 00 00 27 54 32 08 40 00     06:12:06.278  READ FPDMA QUEUED
  60 00 00 00 08 00 00 27 54 31 f8 40 00     06:12:06.278  READ FPDMA QUEUED

Error 7 [6] occurred at disk power-on lifetime: 862 hours (35 days + 22 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 32 03 e9 c8 00 00  Error: UNC at LBA = 0x3203e9c8 = 839117256

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 00 18 00 00 32 01 a3 95 40 00     06:12:02.425  READ FPDMA QUEUED
  60 00 00 00 40 00 00 32 01 a3 55 40 00     06:12:02.425  READ FPDMA QUEUED
  60 00 00 00 20 00 00 32 01 a3 35 40 00     06:12:02.419  READ FPDMA QUEUED
  60 00 00 00 08 00 00 32 03 e9 c5 40 00     06:12:02.386  READ FPDMA QUEUED
  60 00 00 00 08 00 00 32 03 e9 ad 40 00     06:12:02.377  READ FPDMA QUEUED

Error 6 [5] occurred at disk power-on lifetime: 539 hours (22 days + 11 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 32 03 e9 c8 00 00  Error: UNC at LBA = 0x3203e9c8 = 839117256

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 00 08 00 00 32 03 e9 c5 40 00     09:26:23.683  READ FPDMA QUEUED
  ea 00 00 00 00 00 00 00 00 00 00 a0 00     09:26:23.666  FLUSH CACHE EXT
  61 00 00 00 08 00 00 28 84 dd 18 40 00     09:26:23.666  WRITE FPDMA QUEUED
  ea 00 00 00 00 00 00 00 00 00 00 a0 00     09:26:23.664  FLUSH CACHE EXT
  61 00 00 00 08 00 00 27 15 2a 50 40 00     09:26:23.663  WRITE FPDMA QUEUED

Error 5 [4] occurred at disk power-on lifetime: 539 hours (22 days + 11 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 32 03 e9 c8 00 00  Error: WP at LBA = 0x3203e9c8 = 839117256

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 00 00 00 08 00 00 2a a9 bb c5 40 00     09:26:20.553  WRITE FPDMA QUEUED
  60 00 00 00 08 00 00 32 03 e9 c5 40 00     09:26:19.856  READ FPDMA QUEUED
  60 00 00 00 08 00 00 32 03 e9 ad 40 00     09:26:19.856  READ FPDMA QUEUED
  60 00 00 00 08 00 00 32 03 e9 8d 40 00     09:26:19.855  READ FPDMA QUEUED
  60 00 00 00 08 00 00 32 03 e9 75 40 00     09:26:19.855  READ FPDMA QUEUED

Error 4 [3] occurred at disk power-on lifetime: 499 hours (20 days + 19 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 32 03 e9 c8 00 00  Error: UNC at LBA = 0x3203e9c8 = 839117256

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 00 80 00 00 32 03 e9 75 40 00     03:21:08.144  READ FPDMA QUEUED
  60 00 00 02 00 00 00 2a e1 8e cd 40 00     03:21:08.144  READ FPDMA QUEUED
  60 00 00 02 00 00 00 42 13 63 cd 40 00     03:21:08.144  READ FPDMA QUEUED
  60 00 00 02 00 00 00 3b 10 eb 9d 40 00     03:21:08.143  READ FPDMA QUEUED
  60 00 00 00 08 00 00 2a 6d f5 0d 40 00     03:21:08.143  READ FPDMA QUEUED

Error 3 [2] occurred at disk power-on lifetime: 499 hours (20 days + 19 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 32 03 e9 c8 00 00  Error: UNC at LBA = 0x3203e9c8 = 839117256

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 00 88 00 00 32 03 e9 75 40 00     03:21:04.194  READ FPDMA QUEUED
  60 00 00 01 00 00 00 32 03 e8 75 40 00     03:21:04.186  READ FPDMA QUEUED
  60 00 00 02 00 00 00 32 03 e6 75 40 00     03:21:04.166  READ FPDMA QUEUED
  60 00 00 01 00 00 00 2a e1 81 cd 40 00     03:21:04.041  READ FPDMA QUEUED
  60 00 00 02 00 00 00 2a e1 7f cd 40 00     03:21:04.023  READ FPDMA QUEUED

Error 2 [1] occurred at disk power-on lifetime: 347 hours (14 days + 11 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 32 03 e9 c8 00 00  Error: UNC at LBA = 0x3203e9c8 = 839117256

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 00 80 00 00 32 03 e9 75 40 00     03:35:33.971  READ FPDMA QUEUED
  60 00 00 00 48 00 00 27 41 e4 a8 40 00     03:35:33.943  READ FPDMA QUEUED
  60 00 00 00 50 00 00 27 41 e4 50 40 00     03:35:33.935  READ FPDMA QUEUED
  60 00 00 00 58 00 00 27 41 e3 f0 40 00     03:35:33.934  READ FPDMA QUEUED
  60 00 00 00 18 00 00 27 4a 6f 00 40 00     03:35:33.934  READ FPDMA QUEUED

Error 1 [0] occurred at disk power-on lifetime: 347 hours (14 days + 11 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 32 03 e9 c8 00 00  Error: UNC at LBA = 0x3203e9c8 = 839117256

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 00 88 00 00 32 03 e9 75 40 00     03:35:30.144  READ FPDMA QUEUED
  60 00 00 01 00 00 00 32 03 e8 75 40 00     03:35:30.134  READ FPDMA QUEUED
  60 00 00 01 00 00 00 32 03 e7 75 40 00     03:35:30.127  READ FPDMA QUEUED
  60 00 00 02 00 00 00 42 91 7e 35 40 00     03:35:30.127  READ FPDMA QUEUED
  60 00 00 01 00 00 00 32 03 e6 75 40 00     03:35:30.115  READ FPDMA QUEUED

SMART Extended Self-test Log Version: 1 (1 sectors)
Num  Test_Description    Status                  Remaining  LifeTime(hours)  LBA_of_first_error
# 1  Short offline       Completed without error       00%     12943         -

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Status Version:                  3
SCT Version (vendor specific):       522 (0x020a)
Device State:                        Active (0)
Current Temperature:                    35 Celsius
Power Cycle Min/Max Temperature:     25/35 Celsius
Lifetime    Min/Max Temperature:     16/48 Celsius
Under/Over Temperature Limit Count:   0/0

SCT Data Table command not supported

SCT Error Recovery Control command not supported

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11)
ID      Size     Value  Description
0x000a  2            4  Device-to-host register FISes sent due to a COMRESET
0x0001  2            0  Command failed due to ICRC error
0x0003  2            0  R_ERR response for device-to-host data FIS
0x0004  2            0  R_ERR response for host-to-device data FIS
0x0006  2            0  R_ERR response for device-to-host non-data FIS
0x0007  2            0  R_ERR response for host-to-device non-data FIS



