smartctl 7.3 2022-02-28 r5338 [OpenBSD 7.1 amd64] (local build)
Copyright (C) 2002-22, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Device Model:     XPG SX950U
Serial Number:    --
LU WWN Device Id: 5 707c18 ...
Firmware Version: R0126A
User Capacity:    240,057,409,536 bytes [240 GB]
Sector Size:      512 bytes logical/physical
Rotation Rate:    Solid State Device
Form Factor:      2.5 inches
TRIM Command:     Available, deterministic, zeroed
Device is:        Not in smartctl database 7.3/5319
ATA Version is:   ACS-3 T13/2161-D revision 5
SATA Version is:  SATA 3.3, 6.0 Gb/s (current: 6.0 Gb/s)
Local Time is:    Fri Apr 22 20:19:41 2022 MSK
SMART support is: Available - device has SMART capability.
SMART support is: Enabled

=== START OF READ SMART DATA SECTION ===
SMART Status not supported: Incomplete response, ATA output registers missing
SMART overall-health self-assessment test result: PASSED
Warning: This result is based on an Attribute check.

General SMART Values:
Offline data collection status:  (0x82)	Offline data collection activity
					was completed without error.
					Auto Offline Data Collection: Enabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(    0) seconds.
Offline data collection
capabilities: 			 (0x7b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0002)	Does not save SMART data before
					entering power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   2) minutes.
Extended self-test routine
recommended polling time: 	 (  30) minutes.
Conveyance self-test routine
recommended polling time: 	 (   2) minutes.
SCT capabilities: 	       (0x0035)	SCT Status supported.
					SCT Feature Control supported.
					SCT Data Table supported.

SMART Attributes Data Structure revision number: 16
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAG     VALUE WORST THRESH TYPE      UPDATED  WHEN_FAILED RAW_VALUE
  1 Raw_Read_Error_Rate     0x0000   100   100   000    Old_age   Offline      -       0
  5 Reallocated_Sector_Ct   0x0000   100   100   000    Old_age   Offline      -       8
  9 Power_On_Hours          0x0000   100   100   000    Old_age   Offline      -       8889
 12 Power_Cycle_Count       0x0000   100   100   000    Old_age   Offline      -       2446
148 Unknown_Attribute       0x0000   100   100   000    Old_age   Offline      -       18829
149 Unknown_Attribute       0x0000   100   100   000    Old_age   Offline      -       1299
150 Unknown_Attribute       0x0000   100   100   000    Old_age   Offline      -       1219
151 Unknown_Attribute       0x0000   100   100   000    Old_age   Offline      -       1255
159 Unknown_Attribute       0x0000   100   100   000    Old_age   Offline      -       0
160 Unknown_Attribute       0x0000   100   100   000    Old_age   Offline      -       11
161 Unknown_Attribute       0x0000   100   100   000    Old_age   Offline      -       35
163 Unknown_Attribute       0x0000   100   100   000    Old_age   Offline      -       23
164 Unknown_Attribute       0x0000   100   100   000    Old_age   Offline      -       106287
165 Unknown_Attribute       0x0000   100   100   000    Old_age   Offline      -       252
166 Unknown_Attribute       0x0000   100   100   000    Old_age   Offline      -       179
167 Unknown_Attribute       0x0000   100   100   000    Old_age   Offline      -       230
168 Unknown_Attribute       0x0000   100   100   000    Old_age   Offline      -       1500
169 Unknown_Attribute       0x0000   100   100   000    Old_age   Offline      -       100
177 Wear_Leveling_Count     0x0000   100   100   050    Old_age   Offline      -       4
181 Program_Fail_Cnt_Total  0x0000   100   100   000    Old_age   Offline      -       0
182 Erase_Fail_Count_Total  0x0000   100   100   000    Old_age   Offline      -       0
192 Power-Off_Retract_Count 0x0000   100   100   000    Old_age   Offline      -       236
194 Temperature_Celsius     0x0000   100   100   000    Old_age   Offline      -       37
195 Hardware_ECC_Recovered  0x0000   100   100   000    Old_age   Offline      -       9
196 Reallocated_Event_Count 0x0000   100   100   016    Old_age   Offline      -       2
199 UDMA_CRC_Error_Count    0x0000   100   100   050    Old_age   Offline      -       8580
232 Available_Reservd_Space 0x0000   100   100   000    Old_age   Offline      -       100
241 Total_LBAs_Written      0x0000   100   100   000    Old_age   Offline      -       270161
242 Total_LBAs_Read         0x0000   100   100   000    Old_age   Offline      -       326315
245 Unknown_Attribute       0x0000   100   100   000    Old_age   Offline      -       1913166

SMART Error Log Version: 1
ATA Error Count: 0
	CR = Command Register [HEX]
	FR = Features Register [HEX]
	SC = Sector Count Register [HEX]
	SN = Sector Number Register [HEX]
	CL = Cylinder Low Register [HEX]
	CH = Cylinder High Register [HEX]
	DH = Device/Head Register [HEX]
	DC = Device Command Register [HEX]
	ER = Error register [HEX]
	ST = Status register [HEX]
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error -4 occurred at disk power-on lifetime: 0 hours (0 days + 0 hours)
  When the command that caused the error occurred, the device was in an unknown state.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  00 ec 00 00 00 00 00

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  ec 00 00 00 00 00 00 00      00:00:00.000  IDENTIFY DEVICE
  ec 00 00 00 00 00 00 00      00:00:00.000  IDENTIFY DEVICE
  ec 00 00 00 00 00 00 00      00:00:00.000  IDENTIFY DEVICE
  ec 00 00 00 00 00 00 00      00:00:00.000  IDENTIFY DEVICE
  c8 00 00 00 00 00 00 00      00:00:00.000  READ DMA

SMART Self-test log structure revision number 1
Num  Test_Description    Status                  Remaining  LifeTime(hours)  LBA_of_first_error
# 1  Short offline       Completed without error       00%      5857         -
# 2  Short offline       Completed without error       00%      5839         -
# 3  Short offline       Completed without error       00%      5831         -
# 4  Extended offline    Completed without error       00%      5829         -
# 5  Short offline       Completed without error       00%      5820         -
# 6  Short offline       Completed without error       00%      5816         -
# 7  Short offline       Completed without error       00%      5815         -
# 8  Short offline       Completed without error       00%      5814         -
# 9  Short offline       Completed without error       00%      5805         -
#10  Short offline       Completed without error       00%      5800         -
#11  Short offline       Completed without error       00%      5796         -
#12  Short offline       Completed without error       00%      5791         -
#13  Short offline       Completed without error       00%      5787         -
#14  Short offline       Completed without error       00%      5784         -
#15  Short offline       Completed without error       00%      5765         -
#16  Short offline       Completed without error       00%      5751         -
#17  Short offline       Completed without error       00%      5746         -
#18  Short offline       Completed without error       00%      5743         -
#19  Short offline       Completed without error       00%      5739         -
#20  Short offline       Completed without error       00%      5736         -
#21  Short offline       Completed without error       00%      5722         -

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.



