smartctl 7.2 2020-12-30 r5155 [FreeBSD 12.1-RELEASE-p16-HBSD amd64] (local build)
Copyright (C) 2002-20, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Toshiba 2.5" HDD MK..55GSX
Device Model:     TOSHIBA MK2555GSX
Serial Number:    --
LU WWN Device Id: 5 000039 ...
Firmware Version: FG001A
User Capacity:    250,059,350,016 bytes [250 GB]
Sector Size:      512 bytes logical/physical
Device is:        In smartctl database [for details use: -P show]
ATA Version is:   ATA8-ACS (minor revision not indicated)
SATA Version is:  SATA 2.6, 1.5 Gb/s
Local Time is:    Fri May 14 22:35:48 2021 BST
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Unavailable
APM level is:     128 (minimum power consumption without standby)
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, frozen [SEC2]
Wt Cache Reorder: Enabled

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x00)	Offline data collection activity
					was never started.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(  120) seconds.
Offline data collection
capabilities: 			 (0x5b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					No Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   2) minutes.
Extended self-test routine
recommended polling time: 	 (  91) minutes.
SCT capabilities: 	       (0x0039)	SCT Status supported.
					SCT Error Recovery Control supported.
					SCT Feature Control supported.
					SCT Data Table supported.

SMART Attributes Data Structure revision number: 16
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     PO-R--   100   100   050    -    0
  2 Throughput_Performance  P-S---   100   100   050    -    0
  3 Spin_Up_Time            POS--K   100   100   001    -    951
  4 Start_Stop_Count        -O--CK   100   100   000    -    1984
  5 Reallocated_Sector_Ct   PO--CK   100   100   050    -    0
  7 Seek_Error_Rate         PO-R--   100   100   050    -    0
  8 Seek_Time_Performance   P-S---   100   100   050    -    0
  9 Power_On_Hours          -O--CK   001   001   000    -    42727
 10 Spin_Retry_Count        PO--CK   139   100   030    -    0
 12 Power_Cycle_Count       -O--CK   100   100   000    -    1533
191 G-Sense_Error_Rate      -O--CK   100   100   000    -    2540
192 Power-Off_Retract_Count -O--CK   100   100   000    -    74
193 Load_Cycle_Count        -O--CK   001   001   000    -    2201932
194 Temperature_Celsius     -O---K   100   100   000    -    54 (Min/Max 17/80)
196 Reallocated_Event_Count -O--CK   100   100   000    -    0
197 Current_Pending_Sector  -O--CK   100   100   000    -    0
198 Offline_Uncorrectable   ----CK   100   100   000    -    0
199 UDMA_CRC_Error_Count    -O--CK   200   200   000    -    2
220 Disk_Shift              -O----   100   100   000    -    71
222 Loaded_Hours            -O--CK   028   028   000    -    28805
223 Load_Retry_Count        -O--CK   100   100   000    -    0
224 Load_Friction           -O---K   100   100   000    -    0
226 Load-in_Time            -OS--K   100   100   000    -    332
240 Head_Flying_Hours       P-----   100   100   001    -    0
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory Version 1
SMART           Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00       GPL,SL  R/O      1  Log Directory
0x01           SL  R/O      1  Summary SMART error log
0x02           SL  R/O     51  Comprehensive SMART error log
0x03       GPL     R/O     64  Ext. Comprehensive SMART error log
0x06           SL  R/O      1  SMART self-test log
0x07       GPL     R/O      1  Extended self-test log
0x09           SL  R/W      1  Selective self-test log
0x10       GPL     R/O      1  NCQ Command Error log
0x11       GPL     R/O      1  SATA Phy Event Counters log
0x80-0x9f  GPL,SL  R/W     16  Host vendor specific log
0xe0       GPL,SL  R/W      1  SCT Command/Status
0xe1       GPL,SL  R/W      1  SCT Data Transfer

SMART Extended Comprehensive Error Log Version: 1 (64 sectors)
Device Error Count: 111
	CR     = Command Register
	FEATR  = Features Register
	COUNT  = Count (was: Sector Count) Register
	LBA_48 = Upper bytes of LBA High/Mid/Low Registers ]  ATA-8
	LH     = LBA High (was: Cylinder High) Register    ]   LBA
	LM     = LBA Mid (was: Cylinder Low) Register      ] Register
	LL     = LBA Low (was: Sector Number) Register     ]
	DV     = Device (was: Device/Head) Register
	DC     = Device Control Register
	ER     = Error register
	ST     = Status register
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 111 [110] occurred at disk power-on lifetime: 22132 hours (922 days + 4 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  84 -- 51 00 01 00 00 02 9c b8 de e0 00  Error: ICRC, ABRT 1 sectors at LBA = 0x029cb8de = 43825374

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  35 00 00 00 30 00 00 02 9c b8 af e0 00     00:30:33.533  WRITE DMA EXT
  25 00 00 00 30 00 00 00 3f 6c cf e0 00     00:30:33.532  READ DMA EXT
  35 00 00 00 38 00 00 02 9c b8 77 e0 00     00:30:33.532  WRITE DMA EXT
  25 00 00 00 38 00 00 00 3f 6c 97 e0 00     00:30:33.532  READ DMA EXT
  35 00 00 00 18 00 00 02 9c b8 5f e0 00     00:30:33.531  WRITE DMA EXT

Error 110 [109] occurred at disk power-on lifetime: 6594 hours (274 days + 18 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 01 00 00 1b 20 51 03 eb 00  Error: UNC 1 sectors at LBA = 0x1b205103 = 455102723

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 28 00 00 1b 20 50 dc e0 00     16:58:33.262  READ DMA EXT
  25 00 00 00 01 00 00 00 00 00 00 e0 00     16:58:33.253  READ DMA EXT
  25 00 00 00 28 00 00 1b 20 50 dc e0 00     16:58:29.418  READ DMA EXT
  25 00 00 00 01 00 00 00 00 00 00 e0 00     16:58:29.408  READ DMA EXT
  25 00 00 00 28 00 00 1b 20 50 dc e0 00     16:58:25.573  READ DMA EXT

Error 109 [108] occurred at disk power-on lifetime: 6594 hours (274 days + 18 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 01 00 00 1b 20 51 03 eb 00  Error: UNC 1 sectors at LBA = 0x1b205103 = 455102723

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 28 00 00 1b 20 50 dc e0 00     16:58:29.418  READ DMA EXT
  25 00 00 00 01 00 00 00 00 00 00 e0 00     16:58:29.408  READ DMA EXT
  25 00 00 00 28 00 00 1b 20 50 dc e0 00     16:58:25.573  READ DMA EXT
  25 00 00 00 01 00 00 00 00 00 00 e0 00     16:58:25.564  READ DMA EXT
  25 00 00 00 28 00 00 1b 20 50 dc e0 00     16:58:21.751  READ DMA EXT

Error 108 [107] occurred at disk power-on lifetime: 6594 hours (274 days + 18 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 01 00 00 1b 20 51 03 eb 00  Error: UNC 1 sectors at LBA = 0x1b205103 = 455102723

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 28 00 00 1b 20 50 dc e0 00     16:58:25.573  READ DMA EXT
  25 00 00 00 01 00 00 00 00 00 00 e0 00     16:58:25.564  READ DMA EXT
  25 00 00 00 28 00 00 1b 20 50 dc e0 00     16:58:21.751  READ DMA EXT
  25 00 00 00 50 00 00 1b 20 50 8c e0 00     16:58:21.744  READ DMA EXT
  25 00 00 00 08 00 00 1b 20 0d 24 e0 00     16:58:21.620  READ DMA EXT

Error 107 [106] occurred at disk power-on lifetime: 6594 hours (274 days + 18 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 01 00 00 1b 20 51 03 eb 00  Error: UNC 1 sectors at LBA = 0x1b205103 = 455102723

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 28 00 00 1b 20 50 dc e0 00     16:58:21.751  READ DMA EXT
  25 00 00 00 50 00 00 1b 20 50 8c e0 00     16:58:21.744  READ DMA EXT
  25 00 00 00 08 00 00 1b 20 0d 24 e0 00     16:58:21.620  READ DMA EXT
  25 00 00 00 08 00 00 1b 1f 5c 44 e0 00     16:58:21.336  READ DMA EXT
  25 00 00 00 08 00 00 1b 1b 03 dc e0 00     16:58:19.701  READ DMA EXT

Error 106 [105] occurred at disk power-on lifetime: 6594 hours (274 days + 18 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 01 00 00 1b 20 51 03 eb 00  Error: UNC 1 sectors at LBA = 0x1b205103 = 455102723

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 78 00 00 1b 20 50 8c e0 00     16:52:34.789  READ DMA EXT
  25 00 00 00 30 00 00 05 2e af c1 e0 00     16:52:34.776  READ DMA EXT
  35 00 00 00 08 00 00 04 ff 32 07 e0 00     16:52:34.776  WRITE DMA EXT
  25 00 00 00 08 00 00 04 fd 91 1f e0 00     16:52:34.764  READ DMA EXT
  35 00 00 00 80 00 00 04 e7 af af e0 00     16:52:34.763  WRITE DMA EXT

Error 105 [104] occurred at disk power-on lifetime: 6594 hours (274 days + 18 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 01 00 00 1b 20 51 03 eb 00  Error: UNC 1 sectors at LBA = 0x1b205103 = 455102723

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 78 00 00 1b 20 50 8c e0 00     16:52:30.899  READ DMA EXT
  25 00 00 00 08 00 00 05 1f 52 d9 e0 00     16:52:30.899  READ DMA EXT
  25 00 00 00 08 00 00 04 fa 5d 9f e0 00     16:52:30.889  READ DMA EXT
  35 00 00 00 80 00 00 04 e7 af 2f e0 00     16:52:30.888  WRITE DMA EXT
  ea 00 00 00 00 00 00 00 00 00 00 a0 00     16:52:30.827  FLUSH CACHE EXT

Error 104 [103] occurred at disk power-on lifetime: 6594 hours (274 days + 18 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 01 00 00 1b 20 51 03 eb 00  Error: UNC 1 sectors at LBA = 0x1b205103 = 455102723

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 78 00 00 1b 20 50 8c e0 00     16:52:26.505  READ DMA EXT
  35 00 00 00 08 00 00 11 af d7 8c e0 00     16:52:26.505  WRITE DMA EXT
  25 00 00 00 01 00 00 06 43 69 4d e0 00     16:52:26.493  READ DMA EXT
  35 00 00 00 08 00 00 05 7d aa a7 e0 00     16:52:26.493  WRITE DMA EXT
  35 00 00 00 08 00 00 05 22 ac 3f e0 00     16:52:26.492  WRITE DMA EXT

SMART Extended Self-test Log Version: 1 (1 sectors)
Num  Test_Description    Status                  Remaining  LifeTime(hours)  LBA_of_first_error
# 1  Short offline       Completed without error       00%      6555         -

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Status Version:                  2
SCT Version (vendor specific):       1 (0x0001)
Device State:                        Active (0)
Current Temperature:                    54 Celsius
Power Cycle Min/Max Temperature:     --/54 Celsius
Lifetime    Min/Max Temperature:     --/80 Celsius

SCT Temperature History Version:     2
Temperature Sampling Period:         1 minute
Temperature Logging Interval:        1 minute
Min/Max recommended Temperature:      5/55 Celsius
Min/Max Temperature Limit:            5/55 Celsius
Temperature History Size (Index):    478 (190)

SCT Error Recovery Control:
           Read: Disabled
          Write: Disabled

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11)
ID      Size     Value  Description
0x0001  4            0  Command failed due to ICRC error
0x0002  4            0  R_ERR response for data FIS
0x0003  4            0  R_ERR response for device-to-host data FIS
0x0004  4            0  R_ERR response for host-to-device data FIS
0x0005  4            0  R_ERR response for non-data FIS
0x0006  4            0  R_ERR response for device-to-host non-data FIS
0x0007  4            0  R_ERR response for host-to-device non-data FIS
0x0008  4            0  Device-to-host non-data FIS retries
0x0009  4            2  Transition from drive PhyRdy to drive PhyNRdy
0x000a  4            2  Device-to-host register FISes sent due to a COMRESET
0x000b  4            0  CRC errors within host-to-device FIS
0x000d  4            0  Non-CRC errors within host-to-device FIS
0x000f  4            0  R_ERR response for host-to-device data FIS, CRC
0x0010  4            0  R_ERR response for host-to-device data FIS, non-CRC
0x0012  4            0  R_ERR response for host-to-device non-data FIS, CRC
0x0013  4            0  R_ERR response for host-to-device non-data FIS, non-CRC

