smartctl 7.3 2022-02-28 r5338 [FreeBSD 13.1-RELEASE amd64] (local build)
Copyright (C) 2002-22, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Western Digital Caviar Green
Device Model:     WDC WD10EACS-00D6B1
Serial Number:    --
LU WWN Device Id: 5 0014ee ...
Firmware Version: 01.01A01
User Capacity:    1,000,204,886,016 bytes [1.00 TB]
Sector Size:      512 bytes logical/physical
Device is:        In smartctl database 7.3/5319
ATA Version is:   ATA8-ACS (minor revision not indicated)
SATA Version is:  SATA 2.5, 3.0 Gb/s
Local Time is:    Tue Feb 14 22:34:36 2023 UTC
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Disabled
APM feature is:   Unavailable
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, NOT FROZEN [SEC1]
Wt Cache Reorder: Unknown

=== START OF READ SMART DATA SECTION ===
SMART Status not supported: Incomplete response, ATA output registers missing
SMART overall-health self-assessment test result: PASSED
Warning: This result is based on an Attribute check.

General SMART Values:
Offline data collection status:  (0x84)	Offline data collection activity
					was suspended by an interrupting command from host.
					Auto Offline Data Collection: Enabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(23400) seconds.
Offline data collection
capabilities: 			 (0x7b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   2) minutes.
Extended self-test routine
recommended polling time: 	 ( 268) minutes.
Conveyance self-test routine
recommended polling time: 	 (   5) minutes.
SCT capabilities: 	       (0x303f)	SCT Status supported.
					SCT Error Recovery Control supported.
					SCT Feature Control supported.
					SCT Data Table supported.

SMART Attributes Data Structure revision number: 16
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     POSR-K   200   200   051    -    0
  3 Spin_Up_Time            POS--K   191   157   021    -    5425
  4 Start_Stop_Count        -O--CK   079   079   000    -    21564
  5 Reallocated_Sector_Ct   PO--CK   200   200   140    -    0
  7 Seek_Error_Rate         -OSR-K   100   253   000    -    0
  9 Power_On_Hours          -O--CK   076   076   000    -    18065
 10 Spin_Retry_Count        -O--CK   100   100   000    -    0
 11 Calibration_Retry_Count -O--CK   100   100   000    -    0
 12 Power_Cycle_Count       -O--CK   097   097   000    -    3858
192 Power-Off_Retract_Count -O--CK   200   200   000    -    479
193 Load_Cycle_Count        -O--CK   193   193   000    -    21160
194 Temperature_Celsius     -O---K   118   098   000    -    32
196 Reallocated_Event_Count -O--CK   200   200   000    -    0
197 Current_Pending_Sector  -O--CK   200   200   000    -    0
198 Offline_Uncorrectable   ----CK   200   200   000    -    0
199 UDMA_CRC_Error_Count    -O--CK   200   200   000    -    0
200 Multi_Zone_Error_Rate   ---R--   200   200   000    -    0
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory Version 1
SMART           Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00       GPL,SL  R/O      1  Log Directory
0x01           SL  R/O      1  Summary SMART error log
0x02           SL  R/O      5  Comprehensive SMART error log
0x03       GPL     R/O      6  Ext. Comprehensive SMART error log
0x06           SL  R/O      1  SMART self-test log
0x07       GPL     R/O      1  Extended self-test log
0x09           SL  R/W      1  Selective self-test log
0x10       GPL     R/O      1  NCQ Command Error log
0x11       GPL     R/O      1  SATA Phy Event Counters log
0x80-0x9f  GPL,SL  R/W     16  Host vendor specific log
0xa0-0xa7  GPL,SL  VS      16  Device vendor specific log
0xa8-0xb7  GPL,SL  VS       1  Device vendor specific log
0xc0       GPL,SL  VS       1  Device vendor specific log
0xc1       GPL     VS      24  Device vendor specific log
0xe0       GPL,SL  R/W      1  SCT Command/Status
0xe1       GPL,SL  R/W      1  SCT Data Transfer

SMART Extended Comprehensive Error Log Version: 1 (6 sectors)
Device Error Count: 11
	CR     = Command Register
	FEATR  = Features Register
	COUNT  = Count (was: Sector Count) Register
	LBA_48 = Upper bytes of LBA High/Mid/Low Registers ]  ATA-8
	LH     = LBA High (was: Cylinder High) Register    ]   LBA
	LM     = LBA Mid (was: Cylinder Low) Register      ] Register
	LL     = LBA Low (was: Sector Number) Register     ]
	DV     = Device (was: Device/Head) Register
	DC     = Device Control Register
	ER     = Error register
	ST     = Status register
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 11 [10] occurred at disk power-on lifetime: 16861 hours (702 days + 13 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 f0 00 00 02 6b 8e e0 40 00  Error: UNC 240 sectors at LBA = 0x026b8ee0 = 40603360

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 f0 00 6b 00 8e 02 e0 40 00     00:42:37.507  READ DMA EXT
  25 00 00 00 f0 00 6b 00 8d 02 f0 40 00     00:42:37.504  READ DMA EXT
  25 00 00 00 f0 00 6b 00 8d 02 00 40 00     00:42:37.501  READ DMA EXT
  25 00 00 00 f0 00 6b 00 8c 02 10 40 00     00:42:37.498  READ DMA EXT
  25 00 00 00 f0 00 6b 00 8b 02 20 40 00     00:42:37.495  READ DMA EXT

Error 10 [9] occurred at disk power-on lifetime: 688 hours (28 days + 16 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 08 00 00 51 c6 33 88 40 00  Error: UNC 8 sectors at LBA = 0x51c63388 = 1371943816

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 08 00 c6 00 33 51 88 40 00     00:44:32.215  READ DMA EXT
  25 00 00 00 40 00 08 00 86 00 38 40 00     00:44:32.213  READ DMA EXT
  25 00 00 00 58 00 16 00 ee 1d 18 40 00     00:44:32.211  READ DMA EXT
  25 00 00 00 08 00 c6 00 33 51 88 40 00     00:44:29.155  READ DMA EXT
  25 00 00 00 40 00 08 00 85 00 f8 40 00     00:44:29.124  READ DMA EXT

Error 9 [8] occurred at disk power-on lifetime: 688 hours (28 days + 16 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 08 00 00 51 c6 33 88 40 00  Error: UNC 8 sectors at LBA = 0x51c63388 = 1371943816

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 08 00 c6 00 33 51 88 40 00     00:44:29.155  READ DMA EXT
  25 00 00 00 40 00 08 00 85 00 f8 40 00     00:44:29.124  READ DMA EXT
  35 00 00 00 10 00 08 00 a0 00 38 40 00     00:44:29.123  WRITE DMA EXT
  35 00 00 00 10 00 08 00 9c 00 48 40 00     00:44:29.123  WRITE DMA EXT
  35 00 00 00 10 00 08 00 96 00 e8 40 00     00:44:29.122  WRITE DMA EXT

Error 8 [7] occurred at disk power-on lifetime: 688 hours (28 days + 16 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 08 00 00 51 c6 33 88 40 00  Error: UNC 8 sectors at LBA = 0x51c63388 = 1371943816

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 08 00 c6 00 33 51 88 40 00     00:44:26.047  READ DMA EXT
  35 00 00 00 01 00 06 00 bd 00 f8 40 00     00:44:26.046  WRITE DMA EXT
  35 00 00 00 01 00 e8 00 f4 3e 30 40 00     00:44:26.046  WRITE DMA EXT
  25 00 00 00 80 00 fc 00 04 1d d8 40 00     00:44:26.043  READ DMA EXT
  25 00 00 00 08 00 c6 00 33 51 88 40 00     00:44:23.112  READ DMA EXT

Error 7 [6] occurred at disk power-on lifetime: 688 hours (28 days + 16 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 08 00 00 51 c6 33 88 40 00  Error: UNC 8 sectors at LBA = 0x51c63388 = 1371943816

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 08 00 c6 00 33 51 88 40 00     00:44:23.112  READ DMA EXT
  35 00 00 00 d9 00 07 00 1a 00 b4 40 00     00:44:23.107  WRITE DMA EXT
  35 00 00 00 89 00 e9 00 5b 3e 07 40 00     00:44:23.104  WRITE DMA EXT
  35 00 00 00 08 00 e4 00 75 6b e8 40 00     00:44:23.104  WRITE DMA EXT
  35 00 00 00 08 00 e4 00 76 6b 90 40 00     00:44:23.103  WRITE DMA EXT

Error 6 [5] occurred at disk power-on lifetime: 688 hours (28 days + 16 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 08 00 00 51 c6 33 88 40 00  Error: UNC 8 sectors at LBA = 0x51c63388 = 1371943816

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 08 00 c6 00 33 51 88 40 00     00:44:20.157  READ DMA EXT
  25 00 00 00 08 00 e4 00 76 6b a0 40 00     00:44:20.156  READ DMA EXT
  25 00 00 00 08 00 e4 00 76 6b 98 40 00     00:44:20.155  READ DMA EXT
  25 00 00 00 08 00 e4 00 76 6b 90 40 00     00:44:20.154  READ DMA EXT
  25 00 00 00 08 00 e4 00 75 6b e8 40 00     00:44:20.153  READ DMA EXT

Error 5 [4] occurred at disk power-on lifetime: 687 hours (28 days + 15 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 08 00 00 51 c6 33 88 40 00  Error: UNC 8 sectors at LBA = 0x51c63388 = 1371943816

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 08 00 c6 00 33 51 88 40 00     00:22:03.215  READ DMA EXT
  25 00 00 00 08 00 c6 00 33 51 88 40 00     00:22:00.043  READ DMA EXT
  25 00 00 00 08 00 c6 00 33 51 88 40 00     00:21:56.994  READ DMA EXT
  25 00 00 00 08 00 c6 00 33 51 88 40 00     00:21:54.080  READ DMA EXT
  25 00 00 00 08 00 06 00 40 00 40 40 00     00:21:54.079  READ DMA EXT

Error 4 [3] occurred at disk power-on lifetime: 687 hours (28 days + 15 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 08 00 00 51 c6 33 88 40 00  Error: UNC 8 sectors at LBA = 0x51c63388 = 1371943816

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 08 00 c6 00 33 51 88 40 00     00:22:00.043  READ DMA EXT
  25 00 00 00 08 00 c6 00 33 51 88 40 00     00:21:56.994  READ DMA EXT
  25 00 00 00 08 00 c6 00 33 51 88 40 00     00:21:54.080  READ DMA EXT
  25 00 00 00 08 00 06 00 40 00 40 40 00     00:21:54.079  READ DMA EXT
  25 00 00 00 08 00 c6 00 33 51 88 40 00     00:21:50.896  READ DMA EXT

SMART Extended Self-test Log Version: 1 (1 sectors)
No self-tests have been logged.  [To run self-tests, use: smartctl -t]

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Status Version:                  2
SCT Version (vendor specific):       258 (0x0102)
Device State:                        SMART Off-line Data Collection executing in background (4)
Current Temperature:                    32 Celsius
Power Cycle Min/Max Temperature:     26/32 Celsius
Lifetime    Min/Max Temperature:     26/52 Celsius
Under/Over Temperature Limit Count:   0/0

SCT Temperature History Version:     2
Temperature Sampling Period:         1 minute
Temperature Logging Interval:        1 minute
Min/Max recommended Temperature:      0/60 Celsius
Min/Max Temperature Limit:           -41/85 Celsius
Temperature History Size (Index):    478 (326)

SMART WRITE LOG does not return COUNT and LBA_LOW register
SCT (Get) Error Recovery Control command failed

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11)
ID      Size     Value  Description
0x0001  2            0  Command failed due to ICRC error
0x0002  2            0  R_ERR response for data FIS
0x0003  2            0  R_ERR response for device-to-host data FIS
0x0004  2            0  R_ERR response for host-to-device data FIS
0x0005  2            0  R_ERR response for non-data FIS
0x0006  2            0  R_ERR response for device-to-host non-data FIS
0x0007  2            0  R_ERR response for host-to-device non-data FIS
0x000a  2            1  Device-to-host register FISes sent due to a COMRESET
0x8000  4         2302  Vendor specific



