smartctl 7.2 2020-12-30 r5155 [FreeBSD 12.2-RELEASE amd64] (local build)
Copyright (C) 2002-20, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Western Digital Caviar Green (AF)
Device Model:     WDC WD20EARS-00MVWB0
Serial Number:    --
LU WWN Device Id: 5 0014ee ...
Firmware Version: 50.0AB50
User Capacity:    2,000,398,934,016 bytes [2.00 TB]
Sector Size:      512 bytes logical/physical
Device is:        In smartctl database [for details use: -P show]
ATA Version is:   ATA8-ACS (minor revision not indicated)
SATA Version is:  SATA 2.6, 3.0 Gb/s
Local Time is:    Tue Aug 17 17:53:48 2021 EDT
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Disabled
APM feature is:   Unavailable
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, frozen [SEC2]
Wt Cache Reorder: Enabled

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x84)	Offline data collection activity
					was suspended by an interrupting command from host.
					Auto Offline Data Collection: Enabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(36000) seconds.
Offline data collection
capabilities: 			 (0x7b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   2) minutes.
Extended self-test routine
recommended polling time: 	 ( 410) minutes.
Conveyance self-test routine
recommended polling time: 	 (   5) minutes.
SCT capabilities: 	       (0x3035)	SCT Status supported.
					SCT Feature Control supported.
					SCT Data Table supported.

SMART Attributes Data Structure revision number: 16
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     POSR-K   192   192   051    -    1866
  3 Spin_Up_Time            POS--K   166   160   021    -    6683
  4 Start_Stop_Count        -O--CK   094   094   000    -    6425
  5 Reallocated_Sector_Ct   PO--CK   193   193   140    -    53
  7 Seek_Error_Rate         -OSR-K   200   200   000    -    0
  9 Power_On_Hours          -O--CK   027   027   000    -    53923
 10 Spin_Retry_Count        -O--CK   100   100   000    -    0
 11 Calibration_Retry_Count -O--CK   100   100   000    -    0
 12 Power_Cycle_Count       -O--CK   098   098   000    -    2219
192 Power-Off_Retract_Count -O--CK   200   200   000    -    615
193 Load_Cycle_Count        -O--CK   067   067   000    -    400106
194 Temperature_Celsius     -O---K   122   094   000    -    28
196 Reallocated_Event_Count -O--CK   165   165   000    -    35
197 Current_Pending_Sector  -O--CK   197   197   000    -    1198
198 Offline_Uncorrectable   ----CK   199   197   000    -    556
199 UDMA_CRC_Error_Count    -O--CK   200   164   000    -    735
200 Multi_Zone_Error_Rate   ---R--   199   197   000    -    432
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory Version 1
SMART           Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00       GPL,SL  R/O      1  Log Directory
0x01           SL  R/O      1  Summary SMART error log
0x02           SL  R/O      5  Comprehensive SMART error log
0x03       GPL     R/O      6  Ext. Comprehensive SMART error log
0x06           SL  R/O      1  SMART self-test log
0x07       GPL     R/O      1  Extended self-test log
0x09           SL  R/W      1  Selective self-test log
0x10       GPL     R/O      1  NCQ Command Error log
0x11       GPL     R/O      1  SATA Phy Event Counters log
0x80-0x9f  GPL,SL  R/W     16  Host vendor specific log
0xa0-0xa7  GPL,SL  VS      16  Device vendor specific log
0xa8-0xb7  GPL,SL  VS       1  Device vendor specific log
0xc0       GPL,SL  VS       1  Device vendor specific log
0xc1       GPL     VS      93  Device vendor specific log
0xe0       GPL,SL  R/W      1  SCT Command/Status
0xe1       GPL,SL  R/W      1  SCT Data Transfer

SMART Extended Comprehensive Error Log Version: 1 (6 sectors)
Device Error Count: 1517 (device log contains only the most recent 24 errors)
	CR     = Command Register
	FEATR  = Features Register
	COUNT  = Count (was: Sector Count) Register
	LBA_48 = Upper bytes of LBA High/Mid/Low Registers ]  ATA-8
	LH     = LBA High (was: Cylinder High) Register    ]   LBA
	LM     = LBA Mid (was: Cylinder Low) Register      ] Register
	LL     = LBA Low (was: Sector Number) Register     ]
	DV     = Device (was: Device/Head) Register
	DC     = Device Control Register
	ER     = Error register
	ST     = Status register
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 1517 [4] occurred at disk power-on lifetime: 53920 hours (2246 days + 16 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 1c 00 1d 68 40 00  Error: UNC at LBA = 0x1c001d68 = 469769576

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 01 00 00 c0 00 00 1c 00 1d 80 40 08     00:00:57.017  READ FPDMA QUEUED
  60 01 00 00 b8 00 00 1c 00 1c 80 40 08     00:00:57.016  READ FPDMA QUEUED
  60 00 08 00 b0 00 00 1c 01 15 c0 40 08     00:00:57.016  READ FPDMA QUEUED
  60 01 00 00 a8 00 00 1c 00 1b 80 40 08     00:00:57.016  READ FPDMA QUEUED
  60 00 08 00 a0 00 00 1c 01 17 f0 40 08     00:00:57.010  READ FPDMA QUEUED

Error 1516 [3] occurred at disk power-on lifetime: 53920 hours (2246 days + 16 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 1c 00 13 c0 40 00  Error: UNC at LBA = 0x1c0013c0 = 469767104

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 01 00 00 78 00 00 1c 00 14 80 40 08     00:00:53.995  READ FPDMA QUEUED
  60 01 00 00 70 00 00 1c 00 13 80 40 08     00:00:53.995  READ FPDMA QUEUED
  60 00 80 00 68 00 00 1c 00 13 00 40 08     00:00:53.963  READ FPDMA QUEUED
  60 00 08 00 60 00 00 1c 01 1a d0 40 08     00:00:53.960  READ FPDMA QUEUED
  60 00 08 00 58 00 00 1c 01 18 20 40 08     00:00:53.948  READ FPDMA QUEUED

Error 1515 [2] occurred at disk power-on lifetime: 53919 hours (2246 days + 15 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 1c 00 13 e0 40 00  Error: UNC at LBA = 0x1c0013e0 = 469767136

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 01 00 00 78 00 00 1c 00 14 80 40 08     00:00:50.493  READ FPDMA QUEUED
  60 01 00 00 70 00 00 1c 00 13 80 40 08     00:00:50.493  READ FPDMA QUEUED
  60 00 80 00 68 00 00 1c 00 13 00 40 08     00:00:50.493  READ FPDMA QUEUED
  60 00 08 00 60 00 00 1c 01 1a d0 40 08     00:00:50.479  READ FPDMA QUEUED
  60 00 08 00 58 00 00 1c 01 18 20 40 08     00:00:50.477  READ FPDMA QUEUED

Error 1514 [1] occurred at disk power-on lifetime: 53919 hours (2246 days + 15 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 1c 01 0d 50 40 00  Error: UNC at LBA = 0x1c010d50 = 469830992

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 08 00 50 00 00 1c 01 0d 50 40 08     00:03:13.285  READ FPDMA QUEUED
  60 00 08 00 48 00 00 be 01 0b d0 40 08     00:03:13.257  READ FPDMA QUEUED
  60 00 08 00 40 00 00 be 01 0b c8 40 08     00:03:13.256  READ FPDMA QUEUED
  60 00 08 00 38 00 00 be 01 0b c0 40 08     00:03:13.256  READ FPDMA QUEUED
  60 00 08 00 30 00 00 be 01 0b b0 40 08     00:03:13.224  READ FPDMA QUEUED

Error 1513 [0] occurred at disk power-on lifetime: 53919 hours (2246 days + 15 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 1c 01 0d 50 40 00  Error: UNC at LBA = 0x1c010d50 = 469830992

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 08 00 b8 00 00 1c 01 0d 50 40 08     00:02:47.756  READ FPDMA QUEUED
  60 00 18 00 b0 00 00 d4 04 e1 78 40 08     00:02:47.700  READ FPDMA QUEUED
  60 00 20 00 a8 00 00 1c 09 97 18 40 08     00:02:47.689  READ FPDMA QUEUED
  60 00 08 00 a0 00 00 d1 c1 18 00 40 08     00:02:47.681  READ FPDMA QUEUED
  60 00 30 00 98 00 00 1c 09 97 58 40 08     00:02:47.680  READ FPDMA QUEUED

Error 1512 [23] occurred at disk power-on lifetime: 53919 hours (2246 days + 15 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 1c 01 0d 50 40 00  Error: UNC at LBA = 0x1c010d50 = 469830992

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 08 00 40 00 00 1c 01 0d 50 40 08     00:02:20.537  READ FPDMA QUEUED
  60 00 48 00 38 00 00 d1 86 c0 d0 40 08     00:02:20.526  READ FPDMA QUEUED
  60 00 20 00 30 00 00 d1 86 c0 b0 40 08     00:02:20.512  READ FPDMA QUEUED
  ea 00 00 00 00 00 00 00 00 00 00 e0 08     00:02:20.488  FLUSH CACHE EXT
  60 00 f0 00 10 00 00 00 b2 ac 20 40 08     00:02:20.476  READ FPDMA QUEUED

Error 1511 [22] occurred at disk power-on lifetime: 53913 hours (2246 days + 9 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 00 11 b2 48 40 00  Error: UNC at LBA = 0x0011b248 = 1159752

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 01 00 00 98 00 00 00 11 b1 50 40 08     00:06:00.870  READ FPDMA QUEUED
  60 00 20 00 90 00 00 01 28 77 00 40 08     00:06:00.854  READ FPDMA QUEUED
  60 00 e0 00 88 00 00 00 11 b0 70 40 08     00:06:00.854  READ FPDMA QUEUED
  60 00 08 00 80 00 00 d2 94 4c 90 40 08     00:06:00.791  READ FPDMA QUEUED
  60 00 28 00 78 00 00 ad 1a ae 50 40 08     00:06:00.791  READ FPDMA QUEUED

Error 1510 [21] occurred at disk power-on lifetime: 53913 hours (2246 days + 9 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 00 ec 74 20 40 00  Error: UNC at LBA = 0x00ec7420 = 15496224

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 08 00 e8 00 00 00 ec 74 20 40 08     00:01:15.040  READ FPDMA QUEUED
  61 00 a8 00 88 00 00 74 54 35 e0 40 08     00:01:15.040  WRITE FPDMA QUEUED
  60 00 e0 00 70 00 00 c9 a4 c1 70 40 08     00:01:15.040  READ FPDMA QUEUED
  60 00 20 00 68 00 00 00 e3 83 00 40 08     00:01:15.040  READ FPDMA QUEUED
  61 00 10 00 60 00 00 ad 1b a8 20 40 08     00:01:15.040  WRITE FPDMA QUEUED

SMART Extended Self-test Log Version: 1 (1 sectors)
Num  Test_Description    Status                  Remaining  LifeTime(hours)  LBA_of_first_error
# 1  Short offline       Completed without error       00%     53919         -

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Status Version:                  3
SCT Version (vendor specific):       258 (0x0102)
Device State:                        Active (0)
Current Temperature:                    28 Celsius
Power Cycle Min/Max Temperature:     22/28 Celsius
Lifetime    Min/Max Temperature:     20/56 Celsius
Under/Over Temperature Limit Count:   0/0

SCT Temperature History Version:     2
Temperature Sampling Period:         1 minute
Temperature Logging Interval:        1 minute
Min/Max recommended Temperature:      0/60 Celsius
Min/Max Temperature Limit:           -41/85 Celsius
Temperature History Size (Index):    478 (64)

SCT Error Recovery Control command not supported

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11)
ID      Size     Value  Description
0x0001  2            0  Command failed due to ICRC error
0x0002  2            0  R_ERR response for data FIS
0x0003  2            0  R_ERR response for device-to-host data FIS
0x0004  2            0  R_ERR response for host-to-device data FIS
0x0005  2            0  R_ERR response for non-data FIS
0x0006  2            0  R_ERR response for device-to-host non-data FIS
0x0007  2            0  R_ERR response for host-to-device non-data FIS
0x000a  2            2  Device-to-host register FISes sent due to a COMRESET
0x000b  2            0  CRC errors within host-to-device FIS
0x8000  4         1644  Vendor specific

