smartctl 7.2 2020-12-30 r5155 [FreeBSD 13.0-RELEASE amd64] (local build)
Copyright (C) 2002-20, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Toshiba 2.5" HDD (80 GB and above)
Device Model:     TOSHIBA MK1234GSX
Serial Number:    --
Firmware Version: AH001J
User Capacity:    120,034,123,776 bytes [120 GB]
Sector Size:      512 bytes logical/physical
Device is:        In smartctl database [for details use: -P show]
ATA Version is:   ATA/ATAPI-7 (minor revision not indicated)
Local Time is:    Thu Aug 26 18:38:10 2021 CEST
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Unavailable
APM level is:     128 (minimum power consumption without standby)
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, frozen [SEC2]
Wt Cache Reorder: Unavailable

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x02)	Offline data collection activity
					was completed without error.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(  435) seconds.
Offline data collection
capabilities: 			 (0x5b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					No Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   2) minutes.
Extended self-test routine
recommended polling time: 	 (  86) minutes.

SMART Attributes Data Structure revision number: 16
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     PO-R--   100   100   050    -    0
  2 Throughput_Performance  P-S---   100   100   050    -    0
  3 Spin_Up_Time            POS--K   100   100   001    -    1752
  4 Start_Stop_Count        -O--CK   100   100   000    -    6346
  5 Reallocated_Sector_Ct   PO--CK   100   100   050    -    0
  7 Seek_Error_Rate         PO-R--   100   100   050    -    0
  8 Seek_Time_Performance   P-S---   100   100   050    -    0
  9 Power_On_Hours          -O--CK   084   084   000    -    6621
 10 Spin_Retry_Count        PO--CK   226   100   030    -    0
 12 Power_Cycle_Count       -O--CK   100   100   000    -    6283
192 Power-Off_Retract_Count -O--CK   100   100   000    -    396
193 Load_Cycle_Count        -O--CK   085   085   000    -    154472
194 Temperature_Celsius     -O---K   100   100   000    -    30 (Min/Max 6/59)
196 Reallocated_Event_Count -O--CK   100   100   000    -    0
197 Current_Pending_Sector  -O--CK   100   100   000    -    0
198 Offline_Uncorrectable   ----CK   100   100   000    -    0
199 UDMA_CRC_Error_Count    -O--CK   200   200   000    -    7
220 Disk_Shift              -O----   100   100   000    -    8286
222 Loaded_Hours            -O--CK   086   086   000    -    5666
223 Load_Retry_Count        -O--CK   100   100   000    -    0
224 Load_Friction           -O---K   100   100   000    -    0
226 Load-in_Time            -OS--K   100   100   000    -    312
240 Head_Flying_Hours       P-----   100   100   001    -    0
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory Version 1
SMART           Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00       GPL,SL  R/O      1  Log Directory
0x01           SL  R/O      1  Summary SMART error log
0x02           SL  R/O     51  Comprehensive SMART error log
0x03       GPL     R/O     64  Ext. Comprehensive SMART error log
0x06           SL  R/O      1  SMART self-test log
0x07       GPL     R/O      1  Extended self-test log
0x09           SL  R/W      1  Selective self-test log
0x10       GPL     R/O      1  NCQ Command Error log
0x11       GPL     R/O      1  SATA Phy Event Counters log
0x80-0x9f  GPL,SL  R/W     16  Host vendor specific log

SMART Extended Comprehensive Error Log Version: 1 (64 sectors)
Device Error Count: 48
	CR     = Command Register
	FEATR  = Features Register
	COUNT  = Count (was: Sector Count) Register
	LBA_48 = Upper bytes of LBA High/Mid/Low Registers ]  ATA-8
	LH     = LBA High (was: Cylinder High) Register    ]   LBA
	LM     = LBA Mid (was: Cylinder Low) Register      ] Register
	LL     = LBA Low (was: Sector Number) Register     ]
	DV     = Device (was: Device/Head) Register
	DC     = Device Control Register
	ER     = Error register
	ST     = Status register
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 48 [47] occurred at disk power-on lifetime: 6321 hours (263 days + 9 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  84 -- 51 00 01 00 00 01 f9 d6 06 e1 00  Error: ICRC, ABRT 1 sectors at LBA = 0x01f9d606 = 33150470

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  c8 00 00 00 08 f9 7c 97 f9 d4 50 e1 00     00:41:40.705  READ DMA
  c8 00 00 00 08 ee b9 ef f9 7c 90 e1 00     00:41:40.700  READ DMA
  c8 00 00 00 08 f8 46 ef ee b9 e8 e1 00     00:41:40.685  READ DMA
  c8 00 00 00 08 ef f4 bf f8 46 e8 e1 00     00:41:40.680  READ DMA
  c8 00 00 00 08 ef f4 ef ef f4 b8 e1 00     00:41:40.679  READ DMA

Error 47 [46] occurred at disk power-on lifetime: 6272 hours (261 days + 8 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  84 -- 51 00 01 00 00 00 0a cb a1 e0 00  Error: ICRC, ABRT 1 sectors at LBA = 0x000acba1 = 707489

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  c8 00 00 00 10 0a ca 77 0a c9 a0 e0 00     03:19:43.586  READ DMA
  c8 00 00 00 08 0d 19 ff 0a ca 70 e0 00     03:19:43.580  READ DMA
  c8 00 00 00 10 07 f8 c7 0d 19 f0 e0 00     03:19:43.571  READ DMA
  c8 00 00 00 08 d1 be 0f 07 f8 c0 e0 00     03:19:43.563  READ DMA
  c8 00 00 00 18 d1 bd f7 d1 bd f8 e0 00     03:19:43.556  READ DMA

Error 46 [45] occurred at disk power-on lifetime: 5967 hours (248 days + 15 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  84 -- 51 00 01 00 00 00 b5 1e 34 e0 00  Error: ICRC, ABRT 1 sectors at LBA = 0x00b51e34 = 11869748

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  c8 00 00 00 a8 05 f5 97 b5 1b e8 e0 00     00:02:06.829  READ DMA
  c8 00 00 00 18 00 3e 07 05 f5 80 e0 00     00:02:06.819  READ DMA
  c8 00 00 00 00 8f 9d cf 00 3d 08 e0 00     00:02:06.802  READ DMA
  c8 00 00 00 88 05 f8 7f 8f 9d 48 e0 00     00:02:06.784  READ DMA
  c8 00 00 00 10 d6 c9 ff 05 f8 70 e0 00     00:02:06.772  READ DMA

Error 45 [44] occurred at disk power-on lifetime: 5821 hours (242 days + 13 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  84 -- 51 00 01 00 00 02 c1 29 af e2 00  Error: ICRC, ABRT 1 sectors at LBA = 0x02c129af = 46213551

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  c8 00 00 00 08 40 0d 07 c1 29 80 e2 00     00:02:11.688  READ DMA
  c8 00 00 00 e8 40 0c 1f 40 0c 20 e3 00     00:02:11.686  READ DMA
  c8 00 00 00 08 40 0c 17 40 0c 18 e3 00     00:02:11.686  READ DMA
  c8 00 00 00 08 40 0c 0f 40 0c 10 e3 00     00:02:11.685  READ DMA
  c8 00 00 00 08 41 13 e7 40 0c 08 e3 00     00:02:11.685  READ DMA

Error 44 [43] occurred at disk power-on lifetime: 5795 hours (241 days + 11 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  84 -- 51 00 01 00 00 01 84 11 0c e1 00  Error: ICRC, ABRT 1 sectors at LBA = 0x0184110c = 25432332

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  c8 00 00 00 10 84 09 e7 84 0f 80 e1 00     00:01:42.464  READ DMA
  c8 00 00 00 08 84 09 cf 84 09 e0 e1 00     00:01:42.464  READ DMA
  c8 00 00 00 f8 59 98 07 84 08 d8 e1 00     00:01:42.450  READ DMA
  c8 00 00 00 08 49 c2 6f 59 98 00 e1 00     00:01:42.440  READ DMA
  c8 00 00 00 38 49 c1 27 49 c2 38 e1 00     00:01:42.436  READ DMA

Error 43 [42] occurred at disk power-on lifetime: 5737 hours (239 days + 1 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  84 -- 51 00 01 00 00 00 1c 51 ca e0 00  Error: ICRC, ABRT 1 sectors at LBA = 0x001c51ca = 1855946

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 04 00 00 00 00 1c 4c 78 e0 00     00:00:25.611  READ DMA EXT
  25 00 00 03 40 00 00 00 1c 47 f0 e0 00     00:00:25.587  READ DMA EXT
  25 00 00 01 a8 00 00 00 1c 46 18 e0 00     00:00:25.579  READ DMA EXT
  25 00 00 02 98 00 00 00 1c 43 20 e0 00     00:00:25.569  READ DMA EXT
  25 00 00 02 60 00 00 00 1c 40 b0 e0 00     00:00:25.558  READ DMA EXT

Error 42 [41] occurred at disk power-on lifetime: 5674 hours (236 days + 10 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  84 -- 51 00 01 00 00 00 3c 3a 52 e0 00  Error: ICRC, ABRT 1 sectors at LBA = 0x003c3a52 = 3947090

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 01 20 00 00 00 3c 38 00 e0 00     00:01:12.691  READ DMA EXT
  c8 00 00 00 88 3c 26 7f 3c 26 c8 e0 00     00:01:12.688  READ DMA
  25 00 00 02 80 00 00 00 3c 24 00 e0 00     00:01:12.675  READ DMA EXT
  c8 00 00 00 88 3c 16 77 3c 16 f0 e0 00     00:01:12.672  READ DMA
  c8 00 00 00 00 3c 14 77 3c 15 78 e0 00     00:01:12.664  READ DMA

Error 41 [40] occurred at disk power-on lifetime: 5634 hours (234 days + 18 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  84 -- 51 00 01 00 00 0d dd 99 93 ed 00  Error: ICRC, ABRT 1 sectors at LBA = 0x0ddd9993 = 232626579

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  c8 00 00 00 40 dc de 3f dd 98 40 ed 00     00:33:32.806  READ DMA
  c8 00 00 00 40 dc 68 bf dc de 00 ed 00     00:33:32.798  READ DMA
  c8 00 00 00 40 da 48 ff dc 68 80 ed 00     00:33:32.786  READ DMA
  c8 00 00 00 40 45 64 df da 48 c0 ed 00     00:33:32.771  READ DMA
  c8 00 00 00 50 45 64 87 45 64 90 ed 00     00:33:32.769  READ DMA

SMART Extended Self-test Log Version: 1 (1 sectors)
Num  Test_Description    Status                  Remaining  LifeTime(hours)  LBA_of_first_error
# 1  Short offline       Completed without error       00%      6492         -
# 2  Short offline       Completed without error       00%      6184         -

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Commands not supported

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11)
ID      Size     Value  Description
0x0001  4            0  Command failed due to ICRC error
0x0002  4            0  R_ERR response for data FIS
0x0003  4            0  R_ERR response for device-to-host data FIS
0x0004  4            0  R_ERR response for host-to-device data FIS
0x0005  4            0  R_ERR response for non-data FIS
0x0006  4            0  R_ERR response for device-to-host non-data FIS
0x0007  4            0  R_ERR response for host-to-device non-data FIS
0x0008  4            0  Device-to-host non-data FIS retries
0x0009  4            4  Transition from drive PhyRdy to drive PhyNRdy
0x000a  4           13  Device-to-host register FISes sent due to a COMRESET
0x000b  4            0  CRC errors within host-to-device FIS
0x000d  4            0  Non-CRC errors within host-to-device FIS
0x000f  4            0  R_ERR response for host-to-device data FIS, CRC
0x0010  4            0  R_ERR response for host-to-device data FIS, non-CRC
0x0012  4            0  R_ERR response for host-to-device non-data FIS, CRC
0x0013  4            0  R_ERR response for host-to-device non-data FIS, non-CRC

