smartctl 7.2 2020-12-30 r5155 [FreeBSD 12.1-RELEASE amd64] (local build)
Copyright (C) 2002-20, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Device Model:     SAMSUNG SP0411N
Serial Number:    --
Firmware Version: TW100-11
User Capacity:    40,059,321,856 bytes [40.0 GB]
Sector Size:      512 bytes logical/physical
Device is:        Not in smartctl database [for details use: -P showall]
ATA Version is:   ATA/ATAPI-7 T13/1532D revision 0
Local Time is:    Sat Apr 17 14:24:02 2021 UTC
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Disabled
APM feature is:   Unavailable
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, frozen [SEC2]
Wt Cache Reorder: Unavailable

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x00)	Offline data collection activity
					was never started.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(  900) seconds.
Offline data collection
capabilities: 			 (0x1b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					No Conveyance Self-test supported.
					No Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					No General Purpose Logging support.
Short self-test routine 
recommended polling time: 	 (   1) minutes.
Extended self-test routine
recommended polling time: 	 (  15) minutes.

SMART Attributes Data Structure revision number: 16
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     PO-R--   100   100   051    -    40
  3 Spin_Up_Time            POS---   074   057   000    -    4736
  4 Start_Stop_Count        -O--CK   096   096   000    -    4210
  5 Reallocated_Sector_Ct   PO--CK   253   253   010    -    0
  7 Seek_Error_Rate         PO-R--   253   253   051    -    0
  8 Seek_Time_Performance   --S--K   253   253   000    -    0
  9 Power_On_Hours          -O--CK   098   098   000    -    1459740
 10 Spin_Retry_Count        PO--C-   253   253   049    -    0
 12 Power_Cycle_Count       -O--CK   098   098   000    -    2223
194 Temperature_Celsius     -O---K   127   058   000    -    37
195 Hardware_ECC_Recovered  -O-R--   100   100   000    -    100878490
196 Reallocated_Event_Count -O--C-   099   099   000    -    4
197 Current_Pending_Sector  PO--CK   253   253   010    -    0
198 Offline_Uncorrectable   P---CK   099   099   010    -    4
199 UDMA_CRC_Error_Count    PO-R--   100   100   051    -    76
200 Multi_Zone_Error_Rate   PO-R--   100   100   051    -    0
201 Soft_Read_Error_Rate    PO-R--   100   100   051    -    3
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory not supported

SMART Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00           SL  R/O      1  Log Directory
0x01           SL  R/O      1  Summary SMART error log
0x02           SL  R/O      2  Comprehensive SMART error log
0x06           SL  R/O      2  SMART self-test log
0x80-0x9f      SL  R/W     16  Host vendor specific log

SMART Extended Comprehensive Error Log (GP Log 0x03) not supported

SMART Error Log Version: 1
Warning: ATA error count 37632 inconsistent with error log pointer 5

ATA Error Count: 37632 (device log contains only the most recent five errors)
	CR = Command Register [HEX]
	FR = Features Register [HEX]
	SC = Sector Count Register [HEX]
	SN = Sector Number Register [HEX]
	CL = Cylinder Low Register [HEX]
	CH = Cylinder High Register [HEX]
	DH = Device/Head Register [HEX]
	DC = Device Command Register [HEX]
	ER = Error register [HEX]
	ST = Status register [HEX]
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 37632 occurred at disk power-on lifetime: 12069 hours (502 days + 21 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  01 51 40 00 58 53 f1  Error: AMNF 64 sectors at LBA = 0x01535800 = 22239232

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  c8 00 40 00 58 53 f1 00  20d+23:36:49.938  READ DMA
  ca 00 08 c0 00 00 f0 00  20d+23:36:43.938  WRITE DMA
  ca 00 40 c0 ae 47 f2 00  20d+23:36:43.938  WRITE DMA
  ca 00 08 40 00 9e f0 00  20d+23:36:43.938  WRITE DMA
  c8 00 08 88 12 c3 f4 00  20d+23:36:43.438  READ DMA

Error 37631 occurred at disk power-on lifetime: 10748 hours (447 days + 20 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  84 51 00 e8 05 88 f0  Error: ICRC, ABRT at LBA = 0x008805e8 = 8914408

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  c8 00 00 e8 05 88 f0 00      00:17:40.313  READ DMA
  c8 00 00 e8 05 87 f0 00      00:17:40.313  READ DMA
  c8 00 00 e8 05 86 f0 00      00:17:40.313  READ DMA
  c8 00 00 e8 05 85 f0 00      00:17:40.313  READ DMA
  c8 00 00 e8 05 84 f0 00      00:17:40.313  READ DMA

Error 37630 occurred at disk power-on lifetime: 9893 hours (412 days + 5 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  04 51 01 01 00 00 b0

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  b1 10 01 01 00 00 b0 00      00:12:06.000  DEVICE CONFIGURATION [Reserved subcommand] [OBS-ACS-3]

Error 37629 occurred at disk power-on lifetime: 9893 hours (412 days + 5 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  04 51 01 01 00 00 b0

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  b1 10 01 01 00 00 b0 00      00:11:28.938  DEVICE CONFIGURATION [Reserved subcommand] [OBS-ACS-3]

Error 37628 occurred at disk power-on lifetime: 9893 hours (412 days + 5 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  04 51 01 01 00 00 b0

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  b1 10 01 01 00 00 b0 00      00:06:12.000  DEVICE CONFIGURATION [Reserved subcommand] [OBS-ACS-3]

SMART Extended Self-test Log (GP Log 0x07) not supported

SMART Self-test log structure revision number 1
Num  Test_Description    Status                  Remaining  LifeTime(hours)  LBA_of_first_error
# 1  Short offline       Completed without error       00%     11545         -

Selective Self-tests/Logging not supported

SCT Commands not supported

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11) not supported



