smartctl 7.2 2020-12-30 r5155 [FreeBSD 14.0-CURRENT amd64] (local build)
Copyright (C) 2002-20, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Western Digital RE3 Serial ATA
Device Model:     WDC WD5002ABYS-18B1B0
Serial Number:    --
LU WWN Device Id: 5 0014ee ...
Add. Product Id:  DELL™
Firmware Version: 02.03B04
User Capacity:    500,107,862,016 bytes [500 GB]
Sector Size:      512 bytes logical/physical
Rotation Rate:    7200 rpm
Device is:        In smartctl database [for details use: -P show]
ATA Version is:   ATA8-ACS (minor revision not indicated)
SATA Version is:  SATA 2.5, 3.0 Gb/s
Local Time is:    Fri Feb 12 21:26:52 2021 CET
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM level is:     128 (quiet), recommended: 128
APM feature is:   Unavailable
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, frozen [SEC2]
Wt Cache Reorder: Enabled

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x82)	Offline data collection activity
					was completed without error.
					Auto Offline Data Collection: Enabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		( 9480) seconds.
Offline data collection
capabilities: 			 (0x7b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   2) minutes.
Extended self-test routine
recommended polling time: 	 ( 112) minutes.
Conveyance self-test routine
recommended polling time: 	 (   5) minutes.
SCT capabilities: 	       (0x303f)	SCT Status supported.
					SCT Error Recovery Control supported.
					SCT Feature Control supported.
					SCT Data Table supported.

SMART Attributes Data Structure revision number: 16
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     POSR-K   200   200   051    -    0
  3 Spin_Up_Time            POS--K   212   185   021    -    2358
  4 Start_Stop_Count        -O--CK   096   096   000    -    4133
  5 Reallocated_Sector_Ct   PO--CK   200   200   140    -    0
  7 Seek_Error_Rate         -OSR-K   100   253   000    -    0
  9 Power_On_Hours          -O--CK   036   036   000    -    46941
 10 Spin_Retry_Count        -O--CK   100   100   000    -    0
 11 Calibration_Retry_Count -O--CK   100   100   000    -    0
 12 Power_Cycle_Count       -O--CK   098   098   000    -    2832
192 Power-Off_Retract_Count -O--CK   199   199   000    -    1030
193 Load_Cycle_Count        -O--CK   199   199   000    -    4133
194 Temperature_Celsius     -O---K   108   095   000    -    39
196 Reallocated_Event_Count -O--CK   200   200   000    -    0
197 Current_Pending_Sector  -O--CK   200   200   000    -    0
198 Offline_Uncorrectable   ----CK   200   200   000    -    0
199 UDMA_CRC_Error_Count    -O--CK   200   200   000    -    0
200 Multi_Zone_Error_Rate   ---R--   200   200   000    -    0
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory Version 1
SMART           Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00       GPL,SL  R/O      1  Log Directory
0x01           SL  R/O      1  Summary SMART error log
0x02           SL  R/O      5  Comprehensive SMART error log
0x03       GPL     R/O      6  Ext. Comprehensive SMART error log
0x06           SL  R/O      1  SMART self-test log
0x07       GPL     R/O      1  Extended self-test log
0x09           SL  R/W      1  Selective self-test log
0x10       GPL     R/O      1  NCQ Command Error log
0x11       GPL     R/O      1  SATA Phy Event Counters log
0x80-0x9f  GPL,SL  R/W     16  Host vendor specific log
0xa0-0xa7  GPL,SL  VS      16  Device vendor specific log
0xa8-0xb5  GPL,SL  VS       1  Device vendor specific log
0xb6       GPL     VS       1  Device vendor specific log
0xb7       GPL,SL  VS       1  Device vendor specific log
0xc0       GPL,SL  VS       1  Device vendor specific log
0xc1       GPL     VS      24  Device vendor specific log
0xe0       GPL,SL  R/W      1  SCT Command/Status
0xe1       GPL,SL  R/W      1  SCT Data Transfer

SMART Extended Comprehensive Error Log Version: 1 (6 sectors)
Device Error Count: 9
	CR     = Command Register
	FEATR  = Features Register
	COUNT  = Count (was: Sector Count) Register
	LBA_48 = Upper bytes of LBA High/Mid/Low Registers ]  ATA-8
	LH     = LBA High (was: Cylinder High) Register    ]   LBA
	LM     = LBA Mid (was: Cylinder Low) Register      ] Register
	LL     = LBA Low (was: Sector Number) Register     ]
	DV     = Device (was: Device/Head) Register
	DC     = Device Control Register
	ER     = Error register
	ST     = Status register
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 9 [8] occurred at disk power-on lifetime: 43247 hours (1801 days + 23 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 1c 8c 00 04 8a 40 00  Error: UNC at LBA = 0x1c8c00048a = 122607895690

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 38 00 40 00 00 00 22 64 a0 40 00     01:47:52.009  READ FPDMA QUEUED
  60 00 10 00 38 00 00 00 22 60 a8 40 00     01:47:52.008  READ FPDMA QUEUED
  60 00 10 00 30 00 00 00 22 60 50 40 00     01:47:52.008  READ FPDMA QUEUED
  60 00 08 00 28 00 00 00 73 5b 58 40 00     01:47:52.004  READ FPDMA QUEUED
  60 00 08 00 20 00 00 00 3c e0 c6 40 00     01:47:52.004  READ FPDMA QUEUED

Error 8 [7] occurred at disk power-on lifetime: 43149 hours (1797 days + 21 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 04 ef 00 db 70 40 00  Error: UNC at LBA = 0x4ef00db70 = 21189679984

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 08 00 c0 00 00 0c 29 b5 48 40 00     00:01:56.162  READ FPDMA QUEUED
  60 00 a0 00 b8 00 00 0c 29 bc 48 40 00     00:01:56.161  READ FPDMA QUEUED
  60 01 00 00 b0 00 00 0c 29 bb 48 40 00     00:01:56.161  READ FPDMA QUEUED
  60 01 00 00 a8 00 00 0c 29 ba 48 40 00     00:01:56.161  READ FPDMA QUEUED
  60 01 00 00 a0 00 00 0c 29 b9 48 40 00     00:01:56.161  READ FPDMA QUEUED

Error 7 [6] occurred at disk power-on lifetime: 43099 hours (1795 days + 19 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 40 00 73 00 40 00  Error: UNC at LBA = 0x40007300 = 1073771264

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 78 00 70 00 00 00 73 40 00 40 00     00:19:16.232  READ FPDMA QUEUED
  60 00 50 00 68 00 00 00 73 3f a8 40 00     00:19:16.230  READ FPDMA QUEUED
  60 00 48 00 60 00 00 00 13 41 98 40 00     00:19:16.230  READ FPDMA QUEUED
  60 00 08 00 58 00 00 00 13 41 88 40 00     00:19:16.230  READ FPDMA QUEUED
  60 00 08 00 50 00 00 00 13 41 70 40 00     00:19:16.230  READ FPDMA QUEUED

Error 6 [5] occurred at disk power-on lifetime: 43053 hours (1793 days + 21 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 a2 00 24 f8 40 00  Error: UNC at LBA = 0xa20024f8 = 2717918456

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 28 00 50 00 00 00 24 a2 f8 40 00     00:00:24.637  READ FPDMA QUEUED
  60 00 08 00 48 00 00 00 24 a2 28 40 00     00:00:24.637  READ FPDMA QUEUED
  60 00 80 00 40 00 00 00 13 a6 38 40 00     00:00:24.636  READ FPDMA QUEUED
  60 00 80 00 38 00 00 00 13 a5 b8 40 00     00:00:24.636  READ FPDMA QUEUED
  60 00 80 00 30 00 00 00 13 a5 38 40 00     00:00:24.635  READ FPDMA QUEUED

Error 5 [4] occurred at disk power-on lifetime: 42930 hours (1788 days + 18 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 09 45 00 44 e0 40 00  Error: UNC at LBA = 0x9450044e0 = 39812351200

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 01 00 00 10 00 00 09 44 51 e0 40 00     00:49:46.555  READ FPDMA QUEUED
  60 01 00 00 08 00 00 09 44 50 e0 40 00     00:49:46.555  READ FPDMA QUEUED
  60 01 00 00 f8 00 00 09 44 4f e0 40 00     00:49:46.555  READ FPDMA QUEUED
  60 01 00 00 f0 00 00 09 44 4e e0 40 00     00:49:46.555  READ FPDMA QUEUED
  60 01 00 00 e8 00 00 09 44 4d e0 40 00     00:49:46.554  READ FPDMA QUEUED

Error 4 [3] occurred at disk power-on lifetime: 42927 hours (1788 days + 15 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  10 -- 51 00 80 00 02 12 00 21 90 e0 00  Error: IDNF 128 sectors at LBA = 0x212002190 = 8891933072

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  35 00 00 00 80 00 00 02 21 12 90 e0 00     00:14:46.233  WRITE DMA EXT
  35 00 00 00 80 00 00 02 21 12 10 e0 00     00:14:46.233  WRITE DMA EXT
  35 00 00 00 80 00 00 02 21 11 90 e0 00     00:14:46.232  WRITE DMA EXT
  35 00 00 00 80 00 00 02 21 11 10 e0 00     00:14:46.232  WRITE DMA EXT
  35 00 00 00 80 00 00 02 21 10 90 e0 00     00:14:46.231  WRITE DMA EXT

Error 3 [2] occurred at disk power-on lifetime: 42927 hours (1788 days + 15 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 b7 00 6f 60 40 00  Error: UNC at LBA = 0xb7006f60 = 3070259040

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 28 00 40 00 00 00 6f b7 60 40 00     03:01:09.851  READ FPDMA QUEUED
  60 00 80 00 38 00 00 00 6f b6 e0 40 00     03:01:09.851  READ FPDMA QUEUED
  60 00 40 00 30 00 00 00 6f 8b c8 40 00     03:01:09.851  READ FPDMA QUEUED
  60 00 58 00 28 00 00 00 6f 8b 70 40 00     03:01:09.846  READ FPDMA QUEUED
  60 00 80 00 20 00 00 00 6f 8a f0 40 00     03:01:09.846  READ FPDMA QUEUED

Error 2 [1] occurred at disk power-on lifetime: 42925 hours (1788 days + 13 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 41 00 13 40 40 00  Error: UNC at LBA = 0x41001340 = 1090523968

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 10 00 48 00 00 03 f3 1b f0 40 00     01:44:36.041  READ FPDMA QUEUED
  60 00 e0 00 08 00 00 00 5e 70 60 40 00     01:44:36.040  READ FPDMA QUEUED
  60 01 00 00 f8 00 00 00 5e 6f 60 40 00     01:44:36.039  READ FPDMA QUEUED
  60 01 00 00 f0 00 00 00 5e 6e 60 40 00     01:44:36.039  READ FPDMA QUEUED
  60 01 00 00 e8 00 00 00 5e 6d 60 40 00     01:44:36.036  READ FPDMA QUEUED

SMART Extended Self-test Log Version: 1 (1 sectors)
Num  Test_Description    Status                  Remaining  LifeTime(hours)  LBA_of_first_error
# 1  Short offline       Completed without error       00%     44992         -
# 2  Short offline       Completed without error       00%     42660         -
# 3  Short offline       Completed without error       00%     42647         -
# 4  Short offline       Completed without error       00%     42634         -
# 5  Short offline       Completed without error       00%     42629         -
# 6  Short offline       Completed without error       00%     42617         -
# 7  Short offline       Completed without error       00%     42603         -
# 8  Short offline       Completed without error       00%     42589         -
# 9  Short offline       Completed without error       00%     42588         -
#10  Short offline       Completed without error       00%     42583         -
#11  Short offline       Interrupted (host reset)      80%     34255         -
#12  Short offline       Interrupted (host reset)      80%     32967         -
#13  Extended offline    Completed without error       00%        93         -
#14  Short offline       Completed without error       00%        91         -

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Status Version:                  2
SCT Version (vendor specific):       258 (0x0102)
Device State:                        Active (0)
Current Temperature:                    39 Celsius
Power Cycle Min/Max Temperature:     23/39 Celsius
Lifetime    Min/Max Temperature:     23/52 Celsius
Under/Over Temperature Limit Count:   0/0

SCT Temperature History Version:     2
Temperature Sampling Period:         1 minute
Temperature Logging Interval:        1 minute
Min/Max recommended Temperature:      0/60 Celsius
Min/Max Temperature Limit:           -41/85 Celsius
Temperature History Size (Index):    478 (138)

SCT Error Recovery Control:
           Read:     80 (8.0 seconds)
          Write:     80 (8.0 seconds)

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11)
ID      Size     Value  Description
0x0001  2            0  Command failed due to ICRC error
0x0002  2            0  R_ERR response for data FIS
0x0003  2            0  R_ERR response for device-to-host data FIS
0x0004  2            0  R_ERR response for host-to-device data FIS
0x0005  2            0  R_ERR response for non-data FIS
0x0006  2            0  R_ERR response for device-to-host non-data FIS
0x0007  2            0  R_ERR response for host-to-device non-data FIS
0x000a  2            1  Device-to-host register FISes sent due to a COMRESET
0x8000  4         3499  Vendor specific



