smartctl 7.3 2022-02-28 r5338 [FreeBSD 13.1-RELEASE-p2 i386] (local build)
Copyright (C) 2002-22, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Maxtor DiamondMax Plus 8
Device Model:     Maxtor 6E030L0
Serial Number:    --
Firmware Version: NAR61590
User Capacity:    30,750,031,872 bytes [30.7 GB]
Sector Size:      512 bytes logical/physical
Device is:        In smartctl database 7.3/5319
ATA Version is:   ATA/ATAPI-7 T13/1532D revision 0
Local Time is:    Sat Oct 15 06:16:25 2022 CDT
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM level is:     254 (maximum performance), recommended: 192
APM feature is:   Disabled
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, NOT FROZEN [SEC1]
Wt Cache Reorder: Unavailable

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x82)	Offline data collection activity
					was completed without error.
					Auto Offline Data Collection: Enabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		( 1021) seconds.
Offline data collection
capabilities: 			 (0x5b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					No Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					No General Purpose Logging support.
Short self-test routine 
recommended polling time: 	 (   2) minutes.
Extended self-test routine
recommended polling time: 	 (  17) minutes.

SMART Attributes Data Structure revision number: 16
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  3 Spin_Up_Time            POS--K   224   223   063    -    8966
  4 Start_Stop_Count        -O--CK   253   253   000    -    774
  5 Reallocated_Sector_Ct   PO--CK   253   253   063    -    0
  6 Read_Channel_Margin     P-----   253   253   100    -    0
  7 Seek_Error_Rate         -O-R--   253   251   000    -    0
  8 Seek_Time_Performance   POS--K   246   244   187    -    61897
  9 Power_On_Minutes        -O--CK   211   211   000    -    544h+33m
 10 Spin_Retry_Count        PO-R-K   253   252   157    -    0
 11 Calibration_Retry_Count PO-R-K   253   252   223    -    0
 12 Power_Cycle_Count       -O--CK   251   251   000    -    1147
192 Power-Off_Retract_Count -O--CK   253   253   000    -    768
193 Load_Cycle_Count        -O--CK   253   253   000    -    1246
194 Temperature_Celsius     -O--CK   253   253   000    -    42
195 Hardware_ECC_Recovered  -O-R--   253   252   000    -    1070
196 Reallocated_Event_Count ---R--   253   253   000    -    0
197 Current_Pending_Sector  ---R--   253   253   000    -    0
198 Offline_Uncorrectable   ---R--   253   253   000    -    0
199 UDMA_CRC_Error_Count    ---R--   199   199   000    -    0
200 Multi_Zone_Error_Rate   -O-R--   253   252   000    -    0
201 Soft_Read_Error_Rate    -O-R--   253   252   000    -    10
202 Data_Address_Mark_Errs  -O-R--   253   252   000    -    0
203 Run_Out_Cancel          PO-R--   253   252   180    -    0
204 Soft_ECC_Correction     -O-R--   253   252   000    -    0
205 Thermal_Asperity_Rate   -O-R--   253   252   000    -    0
207 Spin_High_Current       -O-R-K   253   252   000    -    0
208 Spin_Buzz               -O-R-K   253   252   000    -    0
209 Offline_Seek_Performnce --S--K   189   183   000    -    0
 99 Unknown_Attribute       --S---   253   253   000    -    0
100 Unknown_Attribute       --S---   253   253   000    -    0
101 Unknown_Attribute       --S---   253   253   000    -    0
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

Read SMART Log Directory failed: Input/output error

General Purpose Log Directory not supported

SMART Extended Comprehensive Error Log (GP Log 0x03) not supported

SMART Error Log Version: 1
No Errors Logged

SMART Extended Self-test Log (GP Log 0x07) not supported

SMART Self-test log structure revision number 1
No self-tests have been logged.  [To run self-tests, use: smartctl -t]

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Commands not supported

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11) not supported

