smartctl 7.1 2019-12-30 r5022 [MidnightBSD 2.0.1 amd64] (local build)
Copyright (C) 2002-19, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Device Model:     TOSHIBA-TL100
Serial Number:    --
LU WWN Device Id: 5 00080d ...
Firmware Version: SBFZ10.1
User Capacity:    120,034,123,776 bytes [120 GB]
Sector Size:      512 bytes logical/physical
Rotation Rate:    Solid State Device
Form Factor:      2.5 inches
Device is:        Not in smartctl database [for details use: -P showall]
ATA Version is:   ACS-4 (minor revision not indicated)
SATA Version is:  SATA 3.2, 6.0 Gb/s (current: 3.0 Gb/s)
Local Time is:    Fri Jan  1 16:44:34 2021 EST
SMART support is: Available - device has SMART capability.
SMART support is: Enabled

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x00)	Offline data collection activity
					was never started.
					Auto Offline Data Collection: Disabled.
Total time to complete Offline 
data collection: 		(65535) seconds.
Offline data collection
capabilities: 			 (0x00) 	Offline data collection not supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.

SMART Attributes Data Structure revision number: 16
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAG     VALUE WORST THRESH TYPE      UPDATED  WHEN_FAILED RAW_VALUE
  9 Power_On_Hours          0x0012   100   100   000    Old_age   Always       -       733
 12 Power_Cycle_Count       0x0012   100   100   000    Old_age   Always       -       33
167 Unknown_Attribute       0x0022   100   100   000    Old_age   Always       -       0
168 Unknown_Attribute       0x0012   100   100   000    Old_age   Always       -       0
169 Unknown_Attribute       0x0003   100   100   010    Pre-fail  Always       -       0
173 Unknown_Attribute       0x0012   199   199   000    Old_age   Always       -       0
192 Power-Off_Retract_Count 0x0012   100   100   000    Old_age   Always       -       32
194 Temperature_Celsius     0x0023   073   071   020    Pre-fail  Always       -       27 (Min/Max 22/29)
241 Total_LBAs_Written      0x0032   100   100   000    Old_age   Always       -       23412

SMART Error Log Version: 1
No Errors Logged

SMART Self-test log structure revision number 1
No self-tests have been logged.  [To run self-tests, use: smartctl -t]

Selective Self-tests/Logging not supported

