PNY Solid State Drives
======================

This is a list of all tested PNY solid state drive models and their MTBFs. See
more info on reliability test in the [README](https://github.com/bsdhw/SMART).

Contents
--------

1. [ SSD by Model  ](#ssd-by-model)
2. [ SSD by Family ](#ssd-by-family)

SSD by Model
------------

Please take all columns into account when reading the table. Pay attention on the
number of tested samples and power-on days. Simultaneous high values of both MTBF
and errors are possible if only rare drives in the subset encounter errors.

Days - avg. days per sample,
Err  - avg. errors per sample,
MTBF - avg. MTBF in years per sample.

| MFG       | Model              | Size   | Samples | Days  | Err   | MTBF |
|-----------|--------------------|--------|---------|-------|-------|------|
| PNY       | CS1311 240GB SSD   | 240 GB | 4       | 985   | 0     | 2.70   |
| PNY       | CS1311 120GB SSD   | 120 GB | 4       | 794   | 1     | 1.94   |
| PNY       | CS900 120GB SSD    | 120 GB | 34      | 442   | 0     | 1.21   |
| PNY       | CS900 250GB SSD    | 250 GB | 6       | 248   | 0     | 0.68   |
| PNY       | CS900 240GB SSD    | 240 GB | 19      | 221   | 0     | 0.61   |
| PNY       | SSD2SC240G1CS17... | 240 GB | 1       | 174   | 0     | 0.48   |
| PNY       | SSD2SC240G1CS27... | 240 GB | 1       | 171   | 0     | 0.47   |
| PNY       | CS1311 480GB SSD   | 480 GB | 1       | 152   | 0     | 0.42   |
| PNY       | CS900 500GB SSD    | 500 GB | 7       | 87    | 0     | 0.24   |
| PNY       | 120GB SATA SSD     | 120 GB | 4       | 70    | 0     | 0.19   |
| PNY       | CS900 1TB SSD      | 1 TB   | 1       | 68    | 0     | 0.19   |
| PNY       | SSD2SC240G1SA75... | 240 GB | 1       | 53    | 0     | 0.15   |
| PNY       | SSD2SC240G5LC70... | 240 GB | 1       | 14    | 0     | 0.04   |
| PNY       | SSD2SC120G1CS17... | 120 GB | 2       | 6     | 0     | 0.02   |

SSD by Family
-------------

Please take all columns into account when reading the table. Pay attention on the
number of tested samples and power-on days. Simultaneous high values of both MTBF
and errors are possible if only rare drives in the subset encounter errors.

Days - avg. days per sample,
Err  - avg. errors per sample,
MTBF - avg. MTBF in years per sample.

| MFG       | Family                 | Models | Samples | Days  | Err   | MTBF |
|-----------|------------------------|--------|---------|-------|-------|------|
| PNY       | Phison Driven SSDs     | 5      | 62      | 427   | 1     | 1.16   |
| PNY       | Unknown                | 9      | 24      | 120   | 0     | 0.33   |
