smartctl 7.2 2020-12-30 r5155 [FreeBSD 12.1-RELEASE-p18-HBSD amd64] (local build)
Copyright (C) 2002-20, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     JMicron based SSDs
Device Model:     Kingston SSDNow V Series 64GB
Serial Number:    --
Firmware Version: B090522a
User Capacity:    64,023,257,088 bytes [64.0 GB]
Sector Size:      512 bytes logical/physical
Rotation Rate:    Solid State Device
TRIM Command:     Unavailable
Device is:        In smartctl database [for details use: -P show]
ATA Version is:   ATA/ATAPI-7 (minor revision not indicated)
Local Time is:    Tue Jul  6 15:00:06 2021 CST
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Unavailable
APM feature is:   Unavailable
Rd look-ahead is: Unavailable
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, frozen [SEC2]
Wt Cache Reorder: Unavailable

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x00)	Offline data collection activity
					was never started.
					Auto Offline Data Collection: Disabled.
Total time to complete Offline 
data collection: 		(    0) seconds.
Offline data collection
capabilities: 			 (0x00) 	Offline data collection not supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x00)	Error logging NOT supported.
					No General Purpose Logging support.

SMART Attributes Data Structure revision number: 1280
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
 12 Power_Cycle_Count       -O--CK   100   100   000    -    503
  9 Power_On_Hours          -O--CK   100   100   000    -    0
194 Temperature_Celsius     POS---   032   100   000    -    0
229 Halt_System/Flash_ID    -O----   100   ---   000    -    0x0098d594baf41343
232 Firmware_Version_Info   -O----   100   ---   000    -    0x3039303532320804
233 ECC_Fail_Record         -O----   100   ---   000    -    0x000000000000
234 Avg/Max_Erase_Count     -O----   100   ---   000    -    1690/1800
235 Good/Sys_Block_Count    -O----   100   ---   000    -    16336/1064
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory not supported

SMART Log Directory Version 16
Address    Access  R/W   Size  Description
0x00           SL  R/O      1  Log Directory
0x01           SL  R/O     12  Summary SMART error log
0x07           SL  R/O      9  Extended self-test log
0x0d           SL  R/O    194  LPS Mis-alignment log
0x13           SL  R/O    229  SATA NCQ Send and Receive log
0x19           SL  R/O    232  LBA Status log
0x1f           SL  -      233  Reserved
0x25           SL  R/O    234  Saved Device Internal Status Data log
0x2b           SL  -      235  Reserved

SMART Extended Comprehensive Error Log (GP Log 0x03) not supported

SMART Error Log Version: 16
No Errors Logged

SMART Extended Self-test Log (GP Log 0x07) not supported

SMART Self-test Log not supported

Selective Self-tests/Logging not supported

SCT Commands not supported

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11) not supported

