smartctl 7.2 2020-12-30 r5155 [FreeBSD 13.0-RELEASE amd64] (local build)
Copyright (C) 2002-20, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Seagate Pipeline HD 5900.2
Device Model:     ST3500414CS
Serial Number:    --
LU WWN Device Id: 5 000c50 ...
Firmware Version: SC13
User Capacity:    500,107,862,016 bytes [500 GB]
Sector Size:      512 bytes logical/physical
Rotation Rate:    5900 rpm
Device is:        In smartctl database [for details use: -P show]
ATA Version is:   ATA8-ACS T13/1699-D revision 4
SATA Version is:  SATA 2.6, 3.0 Gb/s (current: 3.0 Gb/s)
Local Time is:    Tue Nov 22 11:08:45 2022 EST
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Unavailable
APM level is:     192 (intermediate level without standby)
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, frozen [SEC2]
Wt Cache Reorder: Unknown

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x00)	Offline data collection activity
					was never started.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(  623) seconds.
Offline data collection
capabilities: 			 (0x73) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					No Offline surface scan supported.
					Self-test supported.
					Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   1) minutes.
Extended self-test routine
recommended polling time: 	 ( 108) minutes.
Conveyance self-test routine
recommended polling time: 	 (   2) minutes.
SCT capabilities: 	       (0x103b)	SCT Status supported.
					SCT Error Recovery Control supported.
					SCT Feature Control supported.
					SCT Data Table supported.

SMART Attributes Data Structure revision number: 10
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     POSR--   118   100   006    -    181366137
  3 Spin_Up_Time            PO----   097   097   000    -    0
  4 Start_Stop_Count        -O--CK   098   098   020    -    2866
  5 Reallocated_Sector_Ct   PO--CK   100   100   036    -    0
  7 Seek_Error_Rate         POSR--   063   060   030    -    2395467
  9 Power_On_Hours          -O--CK   100   100   000    -    168
 10 Spin_Retry_Count        PO--C-   100   100   097    -    0
 12 Power_Cycle_Count       -O--CK   099   099   020    -    1439
184 End-to-End_Error        -O--CK   100   100   099    -    0
187 Reported_Uncorrect      -O--CK   081   081   000    -    19
188 Command_Timeout         -O--CK   100   099   000    -    21
189 High_Fly_Writes         -O-RCK   100   100   000    -    0
190 Airflow_Temperature_Cel -O---K   076   063   045    -    24 (Min/Max 24/25)
194 Temperature_Celsius     -O---K   024   040   000    -    24 (0 5 0 0 0)
195 Hardware_ECC_Recovered  -O-RC-   052   049   000    -    181366137
197 Current_Pending_Sector  -O--C-   100   100   000    -    6
198 Offline_Uncorrectable   ----C-   100   100   000    -    6
199 UDMA_CRC_Error_Count    -OSRCK   200   200   000    -    0
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory Version 1
SMART           Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00       GPL,SL  R/O      1  Log Directory
0x01       GPL,SL  R/O      1  Summary SMART error log
0x02       GPL,SL  R/O      5  Comprehensive SMART error log
0x03       GPL,SL  R/O      5  Ext. Comprehensive SMART error log
0x06       GPL,SL  R/O      1  SMART self-test log
0x07       GPL,SL  R/O      1  Extended self-test log
0x09       GPL,SL  R/W      1  Selective self-test log
0x10       GPL,SL  R/O      1  NCQ Command Error log
0x11       GPL,SL  R/O      1  SATA Phy Event Counters log
0x21       GPL,SL  R/O      1  Write stream error log
0x22       GPL,SL  R/O      1  Read stream error log
0x80-0x9f  GPL,SL  R/W     16  Host vendor specific log
0xa1       GPL,SL  VS      20  Device vendor specific log
0xa2       GPL     VS    2248  Device vendor specific log
0xa8       GPL,SL  VS     129  Device vendor specific log
0xa9       GPL,SL  VS       1  Device vendor specific log
0xb0       GPL     VS    2928  Device vendor specific log
0xbd       GPL,SL  VS     252  Device vendor specific log
0xbe-0xbf  GPL     VS   65535  Device vendor specific log
0xe0       GPL,SL  R/W      1  SCT Command/Status
0xe1       GPL,SL  R/W      1  SCT Data Transfer

SMART Extended Comprehensive Error Log Version: 1 (5 sectors)
Device Error Count: 19
	CR     = Command Register
	FEATR  = Features Register
	COUNT  = Count (was: Sector Count) Register
	LBA_48 = Upper bytes of LBA High/Mid/Low Registers ]  ATA-8
	LH     = LBA High (was: Cylinder High) Register    ]   LBA
	LM     = LBA Mid (was: Cylinder Low) Register      ] Register
	LL     = LBA Low (was: Sector Number) Register     ]
	DV     = Device (was: Device/Head) Register
	DC     = Device Control Register
	ER     = Error register
	ST     = Status register
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 19 [18] occurred at disk power-on lifetime: 125 hours (5 days + 5 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 18 d3 00 ea 39 00 00  Error: UNC at LBA = 0x18d300ea39 = 106619267641

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 08 00 18 d3 00 ea 38 e0 00     00:27:29.853  READ DMA EXT
  c8 00 00 00 48 00 0c 96 00 53 28 ec 00     00:27:29.852  READ DMA
  25 00 00 00 08 00 18 d4 00 ea 50 e0 00     00:27:29.852  READ DMA EXT
  25 00 00 00 08 00 18 d4 00 ea 48 e0 00     00:27:29.852  READ DMA EXT
  25 00 00 00 08 00 18 d4 00 ea 40 e0 00     00:27:29.852  READ DMA EXT

Error 18 [17] occurred at disk power-on lifetime: 125 hours (5 days + 5 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 18 d3 00 ea 39 00 00  Error: UNC at LBA = 0x18d300ea39 = 106619267641

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 08 00 18 d3 00 ea 38 e0 00     00:27:28.229  READ DMA EXT
  25 00 00 00 08 00 19 7b 00 7a 40 e0 00     00:27:28.212  READ DMA EXT
  35 00 00 04 00 00 1a e8 00 13 80 e0 00     00:27:28.200  WRITE DMA EXT
  c8 00 00 00 08 00 0c 9c 00 56 a0 ec 00     00:27:28.182  READ DMA
  c8 00 00 00 08 00 0c 1c 00 a4 c8 ec 00     00:27:28.133  READ DMA

Error 17 [16] occurred at disk power-on lifetime: 125 hours (5 days + 5 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 18 d3 00 ea 39 00 00  Error: UNC at LBA = 0x18d300ea39 = 106619267641

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 08 00 18 d3 00 ea 38 e0 00     00:27:26.645  READ DMA EXT
  35 00 00 04 00 00 1a e4 00 13 80 e0 00     00:27:26.643  WRITE DMA EXT
  35 00 00 00 18 00 1a 6b 00 52 e8 e0 00     00:27:26.642  WRITE DMA EXT
  35 00 00 04 00 00 1a e0 00 13 80 e0 00     00:27:26.640  WRITE DMA EXT
  c8 00 00 00 18 00 0c 9a 00 53 88 ec 00     00:27:26.632  READ DMA

Error 16 [15] occurred at disk power-on lifetime: 125 hours (5 days + 5 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 18 d3 00 ea 39 00 00  Error: UNC at LBA = 0x18d300ea39 = 106619267641

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 08 00 18 d3 00 ea 38 e0 00     00:27:25.181  READ DMA EXT
  35 00 00 04 00 00 1a dc 00 13 80 e0 00     00:27:25.168  WRITE DMA EXT
  c8 00 00 00 58 00 0c 9a 00 53 28 ec 00     00:27:25.135  READ DMA
  35 00 00 00 20 00 1a 6c 00 52 00 e0 00     00:27:25.134  WRITE DMA EXT
  25 00 00 00 40 00 18 d3 00 ea 78 e0 00     00:27:25.109  READ DMA EXT

Error 15 [14] occurred at disk power-on lifetime: 125 hours (5 days + 5 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 18 d3 00 ea 39 00 00  Error: UNC at LBA = 0x18d300ea39 = 106619267641

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 80 00 18 d3 00 ea 38 e0 00     00:27:23.508  READ DMA EXT
  35 00 00 02 f8 00 1a 68 00 52 b0 e0 00     00:27:23.497  WRITE DMA EXT
  25 00 00 00 40 00 18 d2 00 ea f8 e0 00     00:27:23.486  READ DMA EXT
  25 00 00 00 80 00 18 d2 00 ea 78 e0 00     00:27:23.485  READ DMA EXT
  35 00 00 00 18 00 1a 67 00 52 c8 e0 00     00:27:23.484  WRITE DMA EXT

Error 14 [13] occurred at disk power-on lifetime: 125 hours (5 days + 5 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 18 b6 00 cb 72 00 00  Error: UNC at LBA = 0x18b600cb72 = 106132720498

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 08 00 18 b6 00 cb 70 e0 00     00:26:04.316  READ DMA EXT
  c8 00 00 00 08 00 0c a2 00 53 40 ec 00     00:26:04.315  READ DMA
  25 00 00 00 08 00 18 b6 00 cb 68 e0 00     00:26:04.315  READ DMA EXT
  c8 00 00 00 08 00 0c a1 00 53 d8 ec 00     00:26:04.315  READ DMA
  25 00 00 00 08 00 18 b6 00 cb 60 e0 00     00:26:04.315  READ DMA EXT

Error 13 [12] occurred at disk power-on lifetime: 125 hours (5 days + 5 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 18 b6 00 cb 72 00 00  Error: UNC at LBA = 0x18b600cb72 = 106132720498

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 01 00 00 18 25 00 ca 78 e0 00     00:26:02.177  READ DMA EXT
  25 00 00 02 00 00 18 23 00 ca 78 e0 00     00:26:02.157  READ DMA EXT
  25 00 00 01 00 00 18 22 00 ca 78 e0 00     00:26:02.156  READ DMA EXT
  25 00 00 01 00 00 18 21 00 ca 78 e0 00     00:26:02.155  READ DMA EXT
  25 00 00 01 00 00 18 20 00 ca 78 e0 00     00:26:02.155  READ DMA EXT

Error 12 [11] occurred at disk power-on lifetime: 12 hours (0 days + 12 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 16 6e 00 a6 bd 00 00  Error: UNC at LBA = 0x166e00a6bd = 96334816957

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 08 00 16 6e 00 a6 b8 e0 00     00:17:52.583  READ DMA EXT
  c8 00 00 00 08 00 00 49 00 83 40 e0 00     00:17:52.582  READ DMA
  ca 00 00 00 08 00 01 54 00 82 28 e1 00     00:17:52.582  WRITE DMA
  ca 00 00 00 48 00 00 6b 00 0a 30 e0 00     00:17:52.574  WRITE DMA
  ca 00 00 00 10 00 01 53 00 82 70 e1 00     00:17:52.573  WRITE DMA

SMART Extended Self-test Log Version: 1 (1 sectors)
No self-tests have been logged.  [To run self-tests, use: smartctl -t]

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Status Version:                  3
SCT Version (vendor specific):       522 (0x020a)
Device State:                        Active (0)
Current Temperature:                    24 Celsius
Power Cycle Min/Max Temperature:     24/25 Celsius
Lifetime    Min/Max Temperature:      5/37 Celsius
Under/Over Temperature Limit Count:   0/0

SCT Temperature History Version:     2
Temperature Sampling Period:         2 minutes
Temperature Logging Interval:        94 minutes
Min/Max recommended Temperature:      1/61 Celsius
Min/Max Temperature Limit:            2/60 Celsius
Temperature History Size (Index):    128 (123)

SCT Error Recovery Control:
           Read: Disabled
          Write: Disabled

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11)
ID      Size     Value  Description
0x000a  2            3  Device-to-host register FISes sent due to a COMRESET
0x0001  2            0  Command failed due to ICRC error
0x0003  2            0  R_ERR response for device-to-host data FIS
0x0004  2            0  R_ERR response for host-to-device data FIS
0x0006  2            0  R_ERR response for device-to-host non-data FIS
0x0007  2            0  R_ERR response for host-to-device non-data FIS

