smartctl 7.2 2020-12-30 r5155 [FreeBSD 13.0-RELEASE amd64] (local build)
Copyright (C) 2002-20, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Device Model:     MAXTOR STM3160815AS
Serial Number:    --
Firmware Version: 4.AAB
User Capacity:    160,041,885,696 bytes [160 GB]
Sector Size:      512 bytes logical/physical
Device is:        Not in smartctl database [for details use: -P showall]
ATA Version is:   ATA/ATAPI-7 (minor revision not indicated)
Local Time is:    Sun Jun 13 16:54:01 2021 +07
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Unavailable
APM feature is:   Unavailable
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, NOT FROZEN [SEC1]
Wt Cache Reorder: Unavailable

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x82)	Offline data collection activity
					was completed without error.
					Auto Offline Data Collection: Enabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(  430) seconds.
Offline data collection
capabilities: 			 (0x5b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					No Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   1) minutes.
Extended self-test routine
recommended polling time: 	 (  54) minutes.

SMART Attributes Data Structure revision number: 10
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     POSR--   100   253   006    -    0
  3 Spin_Up_Time            PO----   097   097   000    -    0
  4 Start_Stop_Count        -O--CK   097   097   020    -    3223
  5 Reallocated_Sector_Ct   PO--CK   100   100   036    -    2
  7 Seek_Error_Rate         POSR--   087   060   030    -    548604482
  9 Power_On_Hours          -O--CK   084   084   000    -    14489
 10 Spin_Retry_Count        PO--C-   100   100   097    -    0
 12 Power_Cycle_Count       -O--CK   098   098   020    -    2854
187 Reported_Uncorrect      -O--CK   001   001   000    -    957
189 High_Fly_Writes         -O-RCK   098   098   000    -    2
190 Airflow_Temperature_Cel -O---K   062   048   045    -    38 (Min/Max 26/38)
194 Temperature_Celsius     -O---K   038   052   000    -    38 (0 19 0 0 0)
195 Hardware_ECC_Recovered  -O-RC-   077   072   000    -    166539402
197 Current_Pending_Sector  -O--C-   100   100   000    -    0
198 Offline_Uncorrectable   ----C-   100   100   000    -    0
199 UDMA_CRC_Error_Count    -OSRCK   200   200   000    -    0
200 Multi_Zone_Error_Rate   ------   100   253   000    -    0
202 Data_Address_Mark_Errs  -O--CK   100   253   000    -    0
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory Version 1
SMART           Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00       GPL,SL  R/O      1  Log Directory
0x01       GPL,SL  R/O      1  Summary SMART error log
0x02       GPL,SL  R/O      5  Comprehensive SMART error log
0x03       GPL,SL  R/O      5  Ext. Comprehensive SMART error log
0x06       GPL,SL  R/O      1  SMART self-test log
0x07       GPL,SL  R/O      1  Extended self-test log
0x09       GPL,SL  R/W      1  Selective self-test log
0x10       GPL,SL  R/O      1  NCQ Command Error log
0x11       GPL,SL  R/O      1  SATA Phy Event Counters log
0x20       GPL,SL  R/O      1  Streaming performance log [OBS-8]
0x21       GPL,SL  R/O      1  Write stream error log
0x22       GPL,SL  R/O      1  Read stream error log
0x23       GPL,SL  R/O      1  Delayed sector log [OBS-8]
0x80-0x9f  GPL,SL  R/W     16  Host vendor specific log
0xa0       GPL,SL  VS       1  Device vendor specific log
0xa1       GPL,SL  VS      20  Device vendor specific log
0xa2       GPL,SL  VS     101  Device vendor specific log
0xa8       GPL,SL  VS      20  Device vendor specific log
0xa9       GPL,SL  VS       1  Device vendor specific log
0xe0       GPL,SL  R/W      1  SCT Command/Status
0xe1       GPL,SL  R/W      1  SCT Data Transfer
0xff       GPL     -    23040  Reserved

SMART Extended Comprehensive Error Log Version: 1 (5 sectors)
Device Error Count: 959 (device log contains only the most recent 20 errors)
	CR     = Command Register
	FEATR  = Features Register
	COUNT  = Count (was: Sector Count) Register
	LBA_48 = Upper bytes of LBA High/Mid/Low Registers ]  ATA-8
	LH     = LBA High (was: Cylinder High) Register    ]   LBA
	LM     = LBA Mid (was: Cylinder Low) Register      ] Register
	LL     = LBA Low (was: Sector Number) Register     ]
	DV     = Device (was: Device/Head) Register
	DC     = Device Control Register
	ER     = Error register
	ST     = Status register
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 959 [18] occurred at disk power-on lifetime: 13813 hours (575 days + 13 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 89 00 ec 70 e0 00  Error: UNC at LBA = 0x8900ec70 = 2298539120

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 20 00 00 89 00 ec 60 e0 00     05:21:54.861  READ DMA EXT
  35 00 00 00 30 00 00 56 00 f8 90 e0 00     05:21:54.861  WRITE DMA EXT
  25 00 00 00 30 00 05 91 00 01 10 e0 00     05:21:54.860  READ DMA EXT
  35 00 00 00 10 00 00 56 00 f8 80 e0 00     05:21:54.857  WRITE DMA EXT
  25 00 00 00 10 00 01 a1 00 5c 00 e0 00     05:21:54.849  READ DMA EXT

Error 958 [17] occurred at disk power-on lifetime: 13741 hours (572 days + 13 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 89 00 ec 70 e0 00  Error: UNC at LBA = 0x8900ec70 = 2298539120

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 08 00 00 89 00 ec 70 e0 00     05:21:15.014  READ DMA EXT
  25 00 00 00 08 00 00 89 00 ec 68 e0 00     05:21:14.982  READ DMA EXT
  25 00 00 00 08 00 00 89 00 ec 60 e0 00     05:21:14.982  READ DMA EXT
  35 00 00 00 08 00 00 02 00 5f b8 e0 00     05:21:14.981  WRITE DMA EXT
  35 00 00 00 08 00 00 02 00 5f c0 e0 00     05:21:14.981  WRITE DMA EXT

Error 957 [16] occurred at disk power-on lifetime: 13741 hours (572 days + 13 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 89 00 ec 70 e0 00  Error: UNC at LBA = 0x8900ec70 = 2298539120

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 20 00 00 89 00 ec 60 e0 00     05:21:10.746  READ DMA EXT
  35 00 00 00 20 00 09 8b 00 a7 a0 e0 00     05:21:10.746  WRITE DMA EXT
  35 00 00 00 20 00 09 85 00 a8 e0 e0 00     05:21:10.735  WRITE DMA EXT
  25 00 00 00 20 00 00 56 00 e9 c0 e0 00     05:21:10.734  READ DMA EXT
  25 00 00 00 08 00 00 83 00 4a 10 e0 00     05:21:10.733  READ DMA EXT

Error 956 [15] occurred at disk power-on lifetime: 13813 hours (575 days + 13 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 89 00 ec 70 e0 00  Error: UNC at LBA = 0x8900ec70 = 2298539120

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 08 00 00 89 00 ec 70 e0 00     05:21:58.538  READ DMA EXT
  25 00 00 00 08 00 00 89 00 ec 68 e0 00     05:21:58.608  READ DMA EXT
  25 00 00 00 08 00 00 89 00 ec 60 e0 00     05:21:58.608  READ DMA EXT
  35 00 00 00 08 00 07 1f 00 1e 50 e0 00     05:21:58.590  WRITE DMA EXT
  35 00 00 00 08 00 07 1f 00 1e 30 e0 00     05:21:58.541  WRITE DMA EXT

Error 955 [14] occurred at disk power-on lifetime: 13813 hours (575 days + 13 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 89 00 ec 70 e0 00  Error: UNC at LBA = 0x8900ec70 = 2298539120

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 20 00 00 89 00 ec 60 e0 00     05:21:54.861  READ DMA EXT
  35 00 00 00 30 00 00 56 00 f8 90 e0 00     05:21:54.861  WRITE DMA EXT
  25 00 00 00 30 00 05 91 00 01 10 e0 00     05:21:54.860  READ DMA EXT
  35 00 00 00 10 00 00 56 00 f8 80 e0 00     05:21:54.857  WRITE DMA EXT
  25 00 00 00 10 00 01 a1 00 5c 00 e0 00     05:21:54.849  READ DMA EXT

Error 954 [13] occurred at disk power-on lifetime: 13741 hours (572 days + 13 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 89 00 ec 70 e0 00  Error: UNC at LBA = 0x8900ec70 = 2298539120

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 08 00 00 89 00 ec 70 e0 00     05:21:15.014  READ DMA EXT
  25 00 00 00 08 00 00 89 00 ec 68 e0 00     05:21:14.982  READ DMA EXT
  25 00 00 00 08 00 00 89 00 ec 60 e0 00     05:21:14.982  READ DMA EXT
  35 00 00 00 08 00 00 02 00 5f b8 e0 00     05:21:14.981  WRITE DMA EXT
  35 00 00 00 08 00 00 02 00 5f c0 e0 00     05:21:14.981  WRITE DMA EXT

Error 953 [12] occurred at disk power-on lifetime: 13741 hours (572 days + 13 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 89 00 ec 70 e0 00  Error: UNC at LBA = 0x8900ec70 = 2298539120

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 20 00 00 89 00 ec 60 e0 00     05:21:10.746  READ DMA EXT
  35 00 00 00 20 00 09 8b 00 a7 a0 e0 00     05:21:10.746  WRITE DMA EXT
  35 00 00 00 20 00 09 85 00 a8 e0 e0 00     05:21:10.735  WRITE DMA EXT
  25 00 00 00 20 00 00 56 00 e9 c0 e0 00     05:21:10.734  READ DMA EXT
  25 00 00 00 08 00 00 83 00 4a 10 e0 00     05:21:10.733  READ DMA EXT

Error 952 [11] occurred at disk power-on lifetime: 13813 hours (575 days + 13 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 89 00 ec 70 e0 00  Error: UNC at LBA = 0x8900ec70 = 2298539120

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 08 00 00 89 00 ec 70 e0 00     05:21:58.538  READ DMA EXT
  25 00 00 00 08 00 00 89 00 ec 68 e0 00     05:21:58.608  READ DMA EXT
  25 00 00 00 08 00 00 89 00 ec 60 e0 00     05:21:58.608  READ DMA EXT
  35 00 00 00 08 00 07 1f 00 1e 50 e0 00     05:21:58.590  WRITE DMA EXT
  35 00 00 00 08 00 07 1f 00 1e 30 e0 00     05:21:58.541  WRITE DMA EXT

SMART Extended Self-test Log Version: 1 (1 sectors)

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Commands not supported

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11)
ID      Size     Value  Description
0x000a  2            8  Device-to-host register FISes sent due to a COMRESET
0x0001  2            0  Command failed due to ICRC error
0x0003  2            0  R_ERR response for device-to-host data FIS
0x0004  2            0  R_ERR response for host-to-device data FIS
0x0006  2            0  R_ERR response for device-to-host non-data FIS
0x0007  2            0  R_ERR response for host-to-device non-data FIS

