smartctl 7.3 2022-02-28 r5338 [FreeBSD 13.1-RELEASE-p5 amd64] (local build)
Copyright (C) 2002-22, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Indilinx Barefoot based SSDs
Device Model:     OCZ-AGILITY
Serial Number:    --
Firmware Version: 1.5
User Capacity:    32,017,047,552 bytes [32.0 GB]
Sector Size:      512 bytes logical/physical
Rotation Rate:    Solid State Device
TRIM Command:     Available, deterministic
Device is:        In smartctl database 7.3/5319
ATA Version is:   ATA8-ACS (minor revision not indicated)
Local Time is:    Thu Jan 26 00:24:11 2023 CET
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Unavailable
APM feature is:   Unavailable
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, NOT FROZEN [SEC1]
Wt Cache Reorder: Unavailable

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x00)	Offline data collection activity
					was never started.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(    0) seconds.
Offline data collection
capabilities: 			 (0x1d) SMART execute Offline immediate.
					No Auto Offline data collection support.
					Abort Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					No Conveyance Self-test supported.
					No Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x00)	Error logging NOT supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   0) minutes.
Extended self-test routine
recommended polling time: 	 (   0) minutes.

SMART Attributes Data Structure revision number: 16
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     ------   ---   ---   ---    -    7
  9 Power_On_Hours          ------   ---   ---   ---    -    48574
 12 Power_Cycle_Count       ------   ---   ---   ---    -    459
184 Initial_Bad_Block_Count ------   ---   ---   ---    -    0
195 Program_Failure_Blk_Ct  ------   ---   ---   ---    -    0
196 Erase_Failure_Blk_Ct    ------   ---   ---   ---    -    0
197 Read_Failure_Blk_Ct     ------   ---   ---   ---    -    0
198 Read_Sectors_Tot_Ct     ------   ---   ---   ---    -    4311488490
199 Write_Sectors_Tot_Ct    ------   ---   ---   ---    -    6177692963
200 Read_Commands_Tot_Ct    ------   ---   ---   ---    -    157178875
201 Write_Commands_Tot_Ct   ------   ---   ---   ---    -    186049789
202 Error_Bits_Flash_Tot_Ct ------   ---   ---   ---    -    333872
203 Corr_Read_Errors_Tot_Ct ------   ---   ---   ---    -    302493
204 Bad_Block_Full_Flag     ------   ---   ---   ---    -    0
205 Max_PE_Count_Spec       ------   ---   ---   ---    -    10000
206 Min_Erase_Count         ------   ---   ---   ---    -    9913
207 Max_Erase_Count         ------   ---   ---   ---    -    17281
208 Average_Erase_Count     ------   ---   ---   ---    -    11047
209 Remaining_Lifetime_Perc ------   ---   ---   ---    -    100
211 SATA_Error_Ct_CRC       ------   ---   ---   ---    -    0
212 SATA_Error_Ct_Handshake ------   ---   ---   ---    -    4458
213 Indilinx_Internal       ------   ---   ---   ---    -    0
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory Version 1
SMART           Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00       GPL,SL  R/O      1  Log Directory
0x01       GPL,SL  R/O      1  Summary SMART error log
0x02       GPL,SL  R/O     51  Comprehensive SMART error log
0x03       GPL,SL  R/O     77  Ext. Comprehensive SMART error log
0x06       GPL,SL  R/O      1  SMART self-test log
0x07       GPL,SL  R/O      1  Extended self-test log
0x09       GPL,SL  R/W      1  Selective self-test log
0x10       GPL,SL  R/O      1  NCQ Command Error log
0x11       GPL,SL  R/O      1  SATA Phy Event Counters log
0xa0       GPL     VS    4096  Device vendor specific log

Warning! SMART Extended Comprehensive Error Log Structure error: invalid SMART checksum.
SMART Extended Comprehensive Error Log Version: 49 (77 sectors)
No Errors Logged

Warning! SMART Extended Self-test Log Structure error: invalid SMART checksum.
SMART Extended Self-test Log Version: 1 (1 sectors)
No self-tests have been logged.  [To run self-tests, use: smartctl -t]

Selective Self-tests/Logging not supported

SCT Commands not supported

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11)
[Reserved: 0x15 0x00 0x41 0x84]
ID      Size     Value  Description
0x8b08  10: Invalid entry

