smartctl 7.1 2019-12-30 r5022 [FreeBSD 12.1-STABLE i386] (local build)
Copyright (C) 2002-19, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Western Digital Caviar
Device Model:     WDC WD400BB-00GFA0
Serial Number:    --
Firmware Version: 09.01B09
User Capacity:    40,020,664,320 bytes [40.0 GB]
Sector Size:      512 bytes logical/physical
Device is:        In smartctl database [for details use: -P show]
ATA Version is:   ATA/ATAPI-5 (minor revision not indicated)
Local Time is:    Sun Oct  4 21:30:12 2020 EEST
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM level is:     254 (maximum performance), recommended: 128
APM feature is:   Unavailable
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, NOT FROZEN [SEC1]
Wt Cache Reorder: Unavailable

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x82)	Offline data collection activity
					was completed without error.
					Auto Offline Data Collection: Enabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		( 1506) seconds.
Offline data collection
capabilities: 			 (0x3b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					Conveyance Self-test supported.
					No Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					No General Purpose Logging support.
Short self-test routine 
recommended polling time: 	 (   2) minutes.
Extended self-test routine
recommended polling time: 	 (  28) minutes.
Conveyance self-test routine
recommended polling time: 	 (   5) minutes.

SMART Attributes Data Structure revision number: 16
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     PO-R--   200   200   051    -    0
  3 Spin_Up_Time            POS---   105   093   021    -    2125
  4 Start_Stop_Count        -O--CK   100   100   040    -    817
  5 Reallocated_Sector_Ct   PO--CK   200   200   140    -    0
  7 Seek_Error_Rate         PO-R--   200   200   051    -    0
  9 Power_On_Hours          -O--CK   008   008   000    -    67399
 10 Spin_Retry_Count        PO--C-   100   100   051    -    0
 11 Calibration_Retry_Count PO--C-   100   100   051    -    0
 12 Power_Cycle_Count       -O--CK   100   100   000    -    767
196 Reallocated_Event_Count -O--CK   200   200   000    -    0
197 Current_Pending_Sector  -O--C-   200   200   000    -    0
198 Offline_Uncorrectable   -O--C-   200   200   000    -    0
199 UDMA_CRC_Error_Count    -O-R--   200   253   000    -    0
200 Multi_Zone_Error_Rate   P--R--   200   200   051    -    0
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

Read SMART Log Directory failed: Input/output error

General Purpose Log Directory not supported

SMART Extended Comprehensive Error Log (GP Log 0x03) not supported

SMART Error Log Version: 1
No Errors Logged

SMART Extended Self-test Log (GP Log 0x07) not supported

SMART Self-test log structure revision number 1
Num  Test_Description    Status                  Remaining  LifeTime(hours)  LBA_of_first_error
# 1  Short offline       Completed without error       00%       614         -
# 2  Short offline       Completed without error       00%       446         -
# 3  Short offline       Completed without error       00%       348         -
# 4  Short offline       Completed without error       00%       180         -
# 5  Short offline       Completed without error       00%        12         -
# 6  Short offline       Completed without error       00%       936         -
# 7  Short offline       Completed without error       00%       768         -
# 8  Short offline       Completed without error       00%       600         -
# 9  Short offline       Completed without error       00%       432         -
#10  Short offline       Completed without error       00%       264         -
#11  Short offline       Completed without error       00%        96         -
#12  Short offline       Completed without error       00%      1022         -
#13  Short offline       Completed without error       00%       855         -
#14  Short offline       Completed without error       00%       689         -
#15  Short offline       Completed without error       00%       521         -
#16  Short offline       Completed without error       00%       353         -
#17  Short offline       Completed without error       00%       184         -
#18  Short offline       Completed without error       00%        16         -
#19  Short offline       Completed without error       00%       942         -
#20  Short offline       Completed without error       00%       774         -
#21  Short offline       Completed without error       00%       606         -

Selective Self-tests/Logging not supported

SCT Commands not supported

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11) not supported



