smartctl 7.2 2021-09-14 r5236 [FreeBSD 13.0-STABLE amd64] (local build)
Copyright (C) 2002-20, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Device Model:     ST240HM000-1G5152
Serial Number:    --
LU WWN Device Id: 5 000c50 ...
Firmware Version: C675
User Capacity:    240,057,409,536 bytes [240 GB]
Sector Sizes:     512 bytes logical, 4096 bytes physical
Rotation Rate:    Solid State Device
Form Factor:      2.5 inches
TRIM Command:     Available
Device is:        Not in smartctl database [for details use: -P showall]
ATA Version is:   ATA8-ACS T13/1699-D revision 4
SATA Version is:  SATA 3.0, 6.0 Gb/s (current: 6.0 Gb/s)
Local Time is:    Tue Feb 15 14:39:22 2022 MST
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Unavailable
APM feature is:   Unavailable
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, NOT FROZEN [SEC1]
Wt Cache Reorder: Unavailable

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x02)	Offline data collection activity
					was completed without error.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(    3) seconds.
Offline data collection
capabilities: 			 (0x19) SMART execute Offline immediate.
					No Auto Offline data collection support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					No Conveyance Self-test supported.
					No Selective Self-test supported.
SMART capabilities:            (0x0002)	Does not save SMART data before
					entering power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   1) minutes.
Extended self-test routine
recommended polling time: 	 (  38) minutes.

SMART Attributes Data Structure revision number: 0
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     -OSR--   166   166   006    -    2333
  5 Reallocated_Sector_Ct   PO--CK   100   100   036    -    0
  9 Power_On_Hours          -O--CK   074   074   000    -    23211
 12 Power_Cycle_Count       -O--CK   100   100   020    -    712
171 Unknown_Attribute       -O--CK   100   100   000    -    0
172 Unknown_Attribute       -O--CK   100   100   000    -    0
181 Program_Fail_Cnt_Total  -O--CK   100   100   000    -    0
182 Erase_Fail_Count_Total  -O--CK   100   100   000    -    0
194 Temperature_Celsius     -O---K   032   000   000    -    32 (Min/Max 14/58)
201 Unknown_SSD_Attribute   -O--CK   100   100   000    -    0
204 Soft_ECC_Correction     -O--CK   100   094   000    -    41
231 Unknown_SSD_Attribute   PO--C-   088   088   010    -    13
234 Unknown_Attribute       -O--CK   100   100   000    -    184211
241 Total_LBAs_Written      -O--CK   100   100   000    -    73573
242 Total_LBAs_Read         -O--CK   100   100   000    -    315616
250 Read_Error_Retry_Rate   -O--CK   100   100   000    -    20905
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory Version 1
SMART           Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00       GPL,SL  R/O      1  Log Directory
0x03       GPL,SL  R/O      5  Ext. Comprehensive SMART error log
0x04       GPL,SL  R/O      8  Device Statistics log
0x07       GPL,SL  R/O      2  Extended self-test log
0x10       GPL     R/O      1  NCQ Command Error log
0x11       GPL     R/O      1  SATA Phy Event Counters log
0x80-0x9f  GPL,SL  R/W     16  Host vendor specific log
0xa8       GPL     VS    1041  Device vendor specific log
0xa8       SL      VS     255  Device vendor specific log
0xb7       GPL,SL  VS       4  Device vendor specific log

SMART Extended Comprehensive Error Log Version: 1 (5 sectors)
Device Error Count: 45789 (device log contains only the most recent 20 errors)
	CR     = Command Register
	FEATR  = Features Register
	COUNT  = Count (was: Sector Count) Register
	LBA_48 = Upper bytes of LBA High/Mid/Low Registers ]  ATA-8
	LH     = LBA High (was: Cylinder High) Register    ]   LBA
	LM     = LBA Mid (was: Cylinder Low) Register      ] Register
	LL     = LBA Low (was: Sector Number) Register     ]
	DV     = Device (was: Device/Head) Register
	DC     = Device Control Register
	ER     = Error register
	ST     = Status register
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 45789 [8] occurred at disk power-on lifetime: 23210 hours (967 days + 2 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  04 -- 51 00 00 00 00 00 00 00 00 00 00  Error: ABRT

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  00 00 00 00 00 00 00 00 00 00 00 00 00     00:00:00.040  NOP [Abort queued commands]
  e5 00 00 00 00 00 00 00 00 00 00 00 00     00:00:00.040  CHECK POWER MODE
  ef 00 02 00 00 00 00 00 00 00 00 00 00     00:00:00.040  SET FEATURES [Enable write cache]
  c6 00 00 00 01 00 00 00 00 00 00 00 00     00:00:00.040  SET MULTIPLE MODE
  ef 00 85 00 00 00 00 00 00 00 00 00 00     00:00:00.030  SET FEATURES [Disable APM]

Error 45788 [7] occurred at disk power-on lifetime: 23210 hours (967 days + 2 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  04 -- 51 00 00 00 00 00 00 00 00 00 00  Error: ABRT

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  ef 00 85 00 00 00 00 00 00 00 00 00 00     00:00:00.030  SET FEATURES [Disable APM]
  ef 00 03 00 46 00 00 00 00 00 00 00 00     00:00:00.030  SET FEATURES [Set transfer mode]
  ef 00 03 00 0c 00 00 00 00 00 00 00 00     00:00:00.030  SET FEATURES [Set transfer mode]
  ec 00 00 00 00 00 00 00 00 00 00 00 00     00:00:00.030  IDENTIFY DEVICE
  00 00 00 00 00 00 00 00 00 00 00 00 00     00:00:00.020  NOP [Abort queued commands]

Error 45787 [6] occurred at disk power-on lifetime: 23209 hours (967 days + 1 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  04 -- 51 00 01 00 00 00 00 00 e0 40 00  Error: ABRT

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  2f 00 00 00 01 00 00 00 00 00 e0 40 00     00:01:13.380  READ LOG EXT
  ec 00 00 00 00 00 00 00 00 00 00 00 00     00:01:13.370  IDENTIFY DEVICE
  b0 00 d0 00 00 00 00 00 c2 4f 00 00 00     00:01:13.360  SMART READ DATA
  ec 00 00 00 00 00 00 00 00 00 00 00 00     00:01:13.360  IDENTIFY DEVICE
  b0 00 d0 00 00 00 00 00 c2 4f 00 00 00     00:01:12.780  SMART READ DATA

Error 45786 [5] occurred at disk power-on lifetime: 23209 hours (967 days + 1 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  04 -- 51 00 01 00 00 00 00 03 30 00 00  Error: ABRT

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  2f 00 00 00 01 00 00 00 00 03 30 00 00     00:01:11.770  READ LOG EXT

Error 45785 [4] occurred at disk power-on lifetime: 23183 hours (965 days + 23 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  04 -- 51 00 01 00 00 00 00 00 e0 40 00  Error: ABRT

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  2f 00 00 00 01 00 00 00 00 00 e0 40 00     00:48:08.600  READ LOG EXT
  ec 00 00 00 00 00 00 00 00 00 00 00 00     00:48:08.600  IDENTIFY DEVICE
  b0 00 d0 00 00 00 00 00 c2 4f 00 00 00     00:48:08.590  SMART READ DATA
  ec 00 00 00 00 00 00 00 00 00 00 00 00     00:48:08.590  IDENTIFY DEVICE
  b0 00 d0 00 00 00 00 00 c2 4f 00 00 00     00:48:08.590  SMART READ DATA

Error 45784 [3] occurred at disk power-on lifetime: 23183 hours (965 days + 23 hours)
  When the command that caused the error occurred, the device was in standby mode.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  04 -- 51 00 01 00 00 00 00 03 30 00 00  Error: ABRT

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  2f 00 00 00 01 00 00 00 00 03 30 00 00     00:48:07.600  READ LOG EXT
  e0 00 00 00 00 00 00 00 00 00 00 00 00     00:47:28.830  STANDBY IMMEDIATE
  ea 00 00 00 00 00 00 00 00 00 00 00 00     00:47:28.830  FLUSH CACHE EXT
  ea 00 00 00 00 00 00 00 00 00 00 00 00     00:47:28.800  FLUSH CACHE EXT
  ea 00 00 00 00 00 00 00 00 00 00 00 00     00:47:26.630  FLUSH CACHE EXT

Error 45783 [2] occurred at disk power-on lifetime: 23182 hours (965 days + 22 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  04 -- 51 00 01 00 00 00 00 00 e0 40 00  Error: ABRT

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  2f 00 00 00 01 00 00 00 00 00 e0 40 00     00:01:12.620  READ LOG EXT
  ec 00 00 00 00 00 00 00 00 00 00 00 00     00:01:12.610  IDENTIFY DEVICE
  b0 00 d0 00 00 00 00 00 c2 4f 00 00 00     00:01:12.600  SMART READ DATA
  ec 00 00 00 00 00 00 00 00 00 00 00 00     00:01:12.600  IDENTIFY DEVICE
  b0 00 d0 00 00 00 00 00 c2 4f 00 00 00     00:01:12.600  SMART READ DATA

Error 45782 [1] occurred at disk power-on lifetime: 23182 hours (965 days + 22 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  04 -- 51 00 01 00 00 00 00 03 30 00 00  Error: ABRT

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  2f 00 00 00 01 00 00 00 00 03 30 00 00     00:01:11.580  READ LOG EXT

SMART Extended Self-test Log Version: 1 (2 sectors)
Num  Test_Description    Status                  Remaining  LifeTime(hours)  LBA_of_first_error
# 1  Short offline       Completed without error       00%     23165         -
# 2  Short offline       Completed without error       00%     23164         -
# 3  Short offline       Completed without error       00%     23142         -

Selective Self-tests/Logging not supported

SCT Commands not supported

Device Statistics (GP Log 0x04)
Page  Offset Size        Value Flags Description
0x01  =====  =               =  ===  == General Statistics (rev 2) ==
0x01  0x008  4             712  ---  Lifetime Power-On Resets
                                |||_ C monitored condition met
                                ||__ D supports DSN
                                |___ N normalized value

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11)
ID      Size     Value  Description
0x0001  2            0  Command failed due to ICRC error
0x0002  2            0  R_ERR response for data FIS
0x0003  2            0  R_ERR response for device-to-host data FIS
0x0004  2            0  R_ERR response for host-to-device data FIS
0x0005  2            0  R_ERR response for non-data FIS
0x0006  2            0  R_ERR response for device-to-host non-data FIS
0x0007  2            0  R_ERR response for host-to-device non-data FIS
0x0008  2            0  Device-to-host non-data FIS retries
0x0009  2            0  Transition from drive PhyRdy to drive PhyNRdy
0x000a  2           12  Device-to-host register FISes sent due to a COMRESET
0x000b  2            0  CRC errors within host-to-device FIS
0x000d  2            0  Non-CRC errors within host-to-device FIS
0x000f  2            0  R_ERR response for host-to-device data FIS, CRC
0x0010  2            0  R_ERR response for host-to-device data FIS, non-CRC
0x0012  2            0  R_ERR response for host-to-device non-data FIS, CRC
0x0013  2            0  R_ERR response for host-to-device non-data FIS, non-CRC

