smartctl 7.2 2020-12-30 r5155 [FreeBSD 12.2-RELEASE amd64] (local build)
Copyright (C) 2002-20, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Device Model:     SAMSUNG HD161HJ
Serial Number:    --
LU WWN Device Id: 5 0000f0 ...
Firmware Version: GF100-07
User Capacity:    160,040,803,840 bytes [160 GB]
Sector Size:      512 bytes logical/physical
Device is:        Not in smartctl database [for details use: -P showall]
ATA Version is:   ATA8-ACS T13/1699-D revision 3b
SATA Version is:  SATA 2.5, 3.0 Gb/s
Local Time is:    Mon Jun 14 20:47:15 2021 EDT
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Disabled
APM feature is:   Disabled
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, frozen [SEC2]
Wt Cache Reorder: Enabled

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x00)	Offline data collection activity
					was never started.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (  39)	The self-test routine was interrupted
					by the host with a hard or soft reset.
Total time to complete Offline 
data collection: 		( 2640) seconds.
Offline data collection
capabilities: 			 (0x5b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					No Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   2) minutes.
Extended self-test routine
recommended polling time: 	 (  44) minutes.
SCT capabilities: 	       (0x003f)	SCT Status supported.
					SCT Error Recovery Control supported.
					SCT Feature Control supported.
					SCT Data Table supported.

SMART Attributes Data Structure revision number: 18
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     POSR--   252   100   051    -    0
  3 Spin_Up_Time            POS---   073   073   011    -    4000
  4 Start_Stop_Count        -O--CK   092   092   000    -    8077
  5 Reallocated_Sector_Ct   PO--CK   252   252   010    -    0
  7 Seek_Error_Rate         POSR--   252   252   051    -    0
  8 Seek_Time_Performance   P-S--K   252   252   015    -    0
  9 Power_On_Hours          -O--CK   095   095   000    -    2613913
 10 Spin_Retry_Count        PO--CK   252   252   051    -    0
 11 Calibration_Retry_Count -O--C-   099   099   000    -    4
 12 Power_Cycle_Count       -O--CK   095   095   000    -    4436
184 End-to-End_Error        -O--CK   252   252   000    -    0
187 Reported_Uncorrect      -O--CK   001   001   000    -    1742
188 Command_Timeout         -O--CK   252   252   000    -    0
190 Airflow_Temperature_Cel -O---K   157   085   000    -    32
194 Temperature_Celsius     -O---K   157   085   000    -    32
195 Hardware_ECC_Recovered  -O-RC-   100   100   000    -    0
196 Reallocated_Event_Count -O--CK   252   252   000    -    0
197 Current_Pending_Sector  -O--C-   252   099   000    -    0
198 Offline_Uncorrectable   ----CK   252   252   000    -    0
199 UDMA_CRC_Error_Count    -OS-CK   200   199   000    -    0
200 Multi_Zone_Error_Rate   -O-R--   252   100   000    -    0
201 Soft_Read_Error_Rate    -O-R--   252   252   000    -    0
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory Version 1
SMART           Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00       GPL,SL  R/O      1  Log Directory
0x01           SL  R/O      1  Summary SMART error log
0x02           SL  R/O      2  Comprehensive SMART error log
0x03       GPL     R/O      2  Ext. Comprehensive SMART error log
0x06           SL  R/O      1  SMART self-test log
0x07       GPL     R/O      1  Extended self-test log
0x09           SL  R/W      1  Selective self-test log
0x10       GPL     R/O      1  NCQ Command Error log
0x11       GPL     R/O      1  SATA Phy Event Counters log
0x80-0x9f  GPL,SL  R/W     16  Host vendor specific log
0xe0       GPL,SL  R/W      1  SCT Command/Status
0xe1       GPL,SL  R/W      1  SCT Data Transfer

SMART Extended Comprehensive Error Log Version: 1 (2 sectors)
Device Error Count: 2163 (device log contains only the most recent 8 errors)
	CR     = Command Register
	FEATR  = Features Register
	COUNT  = Count (was: Sector Count) Register
	LBA_48 = Upper bytes of LBA High/Mid/Low Registers ]  ATA-8
	LH     = LBA High (was: Cylinder High) Register    ]   LBA
	LM     = LBA Mid (was: Cylinder Low) Register      ] Register
	LL     = LBA Low (was: Sector Number) Register     ]
	DV     = Device (was: Device/Head) Register
	DC     = Device Control Register
	ER     = Error register
	ST     = Status register
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 2163 [2] occurred at disk power-on lifetime: 21731 hours (905 days + 11 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  04 -- 51 00 01 00 00 00 00 00 25 e0 00  Error: ABRT

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  2f 00 00 00 01 00 00 00 00 00 25 e0 00     00:01:11.000  READ LOG EXT
  ef 00 02 00 00 00 00 00 00 00 00 a0 00     00:01:11.000  SET FEATURES [Enable write cache]
  ef 00 66 00 00 00 00 00 00 00 00 a0 00     00:01:11.000  SET FEATURES [Disable revert defaults]
  f5 00 00 00 00 00 00 00 00 00 00 a0 04     00:01:11.000  SECURITY FREEZE LOCK
  c6 00 00 00 10 00 00 00 00 00 00 a0 00     00:00:56.000  SET MULTIPLE MODE

Error 2162 [1] occurred at disk power-on lifetime: 21728 hours (905 days + 8 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  04 -- 51 00 01 00 00 00 00 00 25 e0 00  Error: ABRT

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  2f 02 00 00 01 00 00 00 00 00 25 e0 04     00:00:26.000  READ LOG EXT
  ef 00 02 00 00 00 00 00 00 00 00 a0 04     00:00:26.000  SET FEATURES [Enable write cache]
  f5 00 00 00 00 00 00 00 00 00 00 a0 04     00:00:26.000  SECURITY FREEZE LOCK
  ef 00 66 00 00 00 00 00 00 00 00 a0 ff     00:00:26.000  SET FEATURES [Disable revert defaults]
  f5 00 00 00 00 00 00 00 00 00 00 a0 00     00:00:26.000  SECURITY FREEZE LOCK

Error 2161 [0] occurred at disk power-on lifetime: 21711 hours (904 days + 15 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  04 -- 51 00 01 00 00 00 00 00 25 e0 00  Error: ABRT

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  2f 02 00 00 01 00 00 00 00 00 25 e0 04     00:00:20.000  READ LOG EXT
  ef 00 02 00 00 00 00 00 00 00 00 a0 04     00:00:20.000  SET FEATURES [Enable write cache]
  f5 00 00 00 00 00 00 00 00 00 00 a0 00     00:00:20.000  SECURITY FREEZE LOCK
  ef 00 66 00 00 00 00 00 00 00 00 a0 00     00:00:20.000  SET FEATURES [Disable revert defaults]
  f5 00 00 00 00 00 00 00 00 00 00 a0 04     00:00:20.000  SECURITY FREEZE LOCK

Error 2160 [7] occurred at disk power-on lifetime: 21684 hours (903 days + 12 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  04 -- 51 00 01 00 00 00 00 00 25 e0 00  Error: ABRT

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  2f 02 00 00 01 00 00 00 00 00 25 e0 04     00:00:20.000  READ LOG EXT
  ef 00 02 00 00 00 00 00 00 00 00 a0 04     00:00:20.000  SET FEATURES [Enable write cache]
  f5 00 00 00 00 00 00 00 00 00 00 a0 04     00:00:20.000  SECURITY FREEZE LOCK
  ef 00 66 00 00 00 00 00 00 00 00 a0 00     00:00:20.000  SET FEATURES [Disable revert defaults]
  f5 00 00 00 00 00 00 00 00 00 00 a0 00     00:00:20.000  SECURITY FREEZE LOCK

Error 2159 [6] occurred at disk power-on lifetime: 21731 hours (905 days + 11 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  04 -- 51 00 01 00 00 00 00 00 25 e0 00  Error: ABRT

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  2f 00 00 00 01 00 00 00 00 00 25 e0 00     00:01:11.000  READ LOG EXT
  ef 00 02 00 00 00 00 00 00 00 00 a0 00     00:01:11.000  SET FEATURES [Enable write cache]
  ef 00 66 00 00 00 00 00 00 00 00 a0 00     00:01:11.000  SET FEATURES [Disable revert defaults]
  f5 00 00 00 00 00 00 00 00 00 00 a0 04     00:01:11.000  SECURITY FREEZE LOCK
  c6 00 00 00 10 00 00 00 00 00 00 a0 00     00:00:56.000  SET MULTIPLE MODE

Error 2158 [5] occurred at disk power-on lifetime: 21728 hours (905 days + 8 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  04 -- 51 00 01 00 00 00 00 00 25 e0 00  Error: ABRT

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  2f 02 00 00 01 00 00 00 00 00 25 e0 04     00:00:26.000  READ LOG EXT
  ef 00 02 00 00 00 00 00 00 00 00 a0 04     00:00:26.000  SET FEATURES [Enable write cache]
  f5 00 00 00 00 00 00 00 00 00 00 a0 04     00:00:26.000  SECURITY FREEZE LOCK
  ef 00 66 00 00 00 00 00 00 00 00 a0 ff     00:00:26.000  SET FEATURES [Disable revert defaults]
  f5 00 00 00 00 00 00 00 00 00 00 a0 00     00:00:26.000  SECURITY FREEZE LOCK

Error 2157 [4] occurred at disk power-on lifetime: 21711 hours (904 days + 15 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  04 -- 51 00 01 00 00 00 00 00 25 e0 00  Error: ABRT

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  2f 02 00 00 01 00 00 00 00 00 25 e0 04     00:00:20.000  READ LOG EXT
  ef 00 02 00 00 00 00 00 00 00 00 a0 04     00:00:20.000  SET FEATURES [Enable write cache]
  f5 00 00 00 00 00 00 00 00 00 00 a0 00     00:00:20.000  SECURITY FREEZE LOCK
  ef 00 66 00 00 00 00 00 00 00 00 a0 00     00:00:20.000  SET FEATURES [Disable revert defaults]
  f5 00 00 00 00 00 00 00 00 00 00 a0 04     00:00:20.000  SECURITY FREEZE LOCK

Error 2156 [3] occurred at disk power-on lifetime: 21684 hours (903 days + 12 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  04 -- 51 00 01 00 00 00 00 00 25 e0 00  Error: ABRT

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  2f 02 00 00 01 00 00 00 00 00 25 e0 04     00:00:20.000  READ LOG EXT
  ef 00 02 00 00 00 00 00 00 00 00 a0 04     00:00:20.000  SET FEATURES [Enable write cache]
  f5 00 00 00 00 00 00 00 00 00 00 a0 04     00:00:20.000  SECURITY FREEZE LOCK
  ef 00 66 00 00 00 00 00 00 00 00 a0 00     00:00:20.000  SET FEATURES [Disable revert defaults]
  f5 00 00 00 00 00 00 00 00 00 00 a0 00     00:00:20.000  SECURITY FREEZE LOCK

Warning! SMART Extended Self-test Log Structure error: invalid SMART checksum.
SMART Extended Self-test Log Version: 0 (1 sectors)
Invalid Self-test Log index = 0x2801 (reserved = 0x00)
SMART Selective self-test log data structure revision number 0
Note: revision number not 1 implies that no selective self-test has ever been run
 SPAN       MIN_LBA       MAX_LBA  CURRENT_TEST_STATUS
    1  545460846592    4294967296  Not_testing
    2             0  545460846592  Not_testing
    3    4294967296             0  Not_testing
    4  545460846592    4294967296  Not_testing
    5             0  545460846592  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Status Version:                  2
SCT Version (vendor specific):       256 (0x0100)
Device State:                        Active (0)
Current Temperature:                    32 Celsius
Power Cycle Min/Max Temperature:     --/33 Celsius
Lifetime    Min/Max Temperature:     --/33 Celsius

SCT Temperature History Version:     2
Temperature Sampling Period:         1 minute
Temperature Logging Interval:        1 minute
Min/Max recommended Temperature:     10/105 Celsius
Min/Max Temperature Limit:            5/110 Celsius
Temperature History Size (Index):    128 (23)

SCT Error Recovery Control:
           Read: Disabled
          Write: Disabled

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11)
ID      Size     Value  Description
0x0001  2            0  Command failed due to ICRC error
0x0002  2            0  R_ERR response for data FIS
0x0003  2            0  R_ERR response for device-to-host data FIS
0x0004  2            0  R_ERR response for host-to-device data FIS
0x0005  2            0  R_ERR response for non-data FIS
0x0006  2            0  R_ERR response for device-to-host non-data FIS
0x0007  2            0  R_ERR response for host-to-device non-data FIS
0x0008  2            0  Device-to-host non-data FIS retries
0x0009  2            3  Transition from drive PhyRdy to drive PhyNRdy
0x000a  2            2  Device-to-host register FISes sent due to a COMRESET
0x000b  2            0  CRC errors within host-to-device FIS
0x000d  2            0  Non-CRC errors within host-to-device FIS
0x000f  2            0  R_ERR response for host-to-device data FIS, CRC
0x0010  2            0  R_ERR response for host-to-device data FIS, non-CRC
0x0012  2            0  R_ERR response for host-to-device non-data FIS, CRC
0x0013  2            0  R_ERR response for host-to-device non-data FIS, non-CRC

