smartctl 7.3 2022-02-28 r5338 [FreeBSD 13.0-STABLE amd64] (local build)
Copyright (C) 2002-22, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Number:                       SAMSUNG MZVLW512HMJP-000H1
Serial Number:                      --
Firmware Version:                   CXY70H1Q
PCI Vendor/Subsystem ID:            0x144d
IEEE OUI Identifier:                0x002538
Total NVM Capacity:                 512,110,190,592 [512 GB]
Unallocated NVM Capacity:           0
Controller ID:                      2
NVMe Version:                       1.2
Number of Namespaces:               1
Namespace 1 Size/Capacity:          512,110,190,592 [512 GB]
Namespace 1 Utilization:            91,303,088,128 [91.3 GB]
Namespace 1 Formatted LBA Size:     512
Namespace 1 IEEE EUI-64:            002538 ...
Local Time is:                      Sun May  8 10:45:20 2022 CDT
Firmware Updates (0x16):            3 Slots, no Reset required
Optional Admin Commands (0x0007):   Security Format Frmw_DL
Optional NVM Commands (0x001f):     Comp Wr_Unc DS_Mngmt Wr_Zero Sav/Sel_Feat
Log Page Attributes (0x03):         S/H_per_NS Cmd_Eff_Lg
Warning  Comp. Temp. Threshold:     77 Celsius
Critical Comp. Temp. Threshold:     80 Celsius

Supported Power States
St Op     Max   Active     Idle   RL RT WL WT  Ent_Lat  Ex_Lat
 0 +     7.60W       -        -    0  0  0  0        0       0
 1 +     6.00W       -        -    1  1  1  1        0       0
 2 +     5.10W       -        -    2  2  2  2        0       0
 3 -   0.0400W       -        -    3  3  3  3      210    1500
 4 -   0.0050W       -        -    4  4  4  4     2200    6000

Supported LBA Sizes (NSID 0x1)
Id Fmt  Data  Metadt  Rel_Perf
 0 +     512       0         0

=== START OF SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

SMART/Health Information (NVMe Log 0x02)
Critical Warning:                   0x00
Temperature:                        43 Celsius
Available Spare:                    100%
Available Spare Threshold:          5%
Percentage Used:                    2%
Data Units Read:                    8,998,612 [4.60 TB]
Data Units Written:                 97,798,292 [50.0 TB]
Host Read Commands:                 121,339,956
Host Write Commands:                1,587,572,033
Controller Busy Time:               1,102
Power Cycles:                       332
Power On Hours:                     20,563
Unsafe Shutdowns:                   46
Media and Data Integrity Errors:    0
Error Information Log Entries:      139
Warning  Comp. Temperature Time:    0
Critical Comp. Temperature Time:    0
Temperature Sensor 1:               43 Celsius

Error Information (NVMe Log 0x01, 16 of 64 entries)
Num   ErrCount  SQId   CmdId  Status  PELoc          LBA  NSID    VS
  0        139     0  0x0018  0x4004  0x02c            0     0     -
  1        138     0  0x0017  0x4004  0x02c            0     0     -
  2        137     0  0x0015  0x4212  0x028            0     -     -
  3        136     0  0x001a  0x4004  0x02c            0     0     -
  4        135     0  0x0019  0x4004  0x02c            0     0     -
  5        134     0  0x0015  0x4212  0x028            0     -     -
  6        133     0  0x0012  0x4212  0x028            0     -     -
  7        132     0  0x0012  0x4212  0x028            0     -     -
  8        131     0  0x0018  0x4004  0x02c            0     0     -
  9        130     0  0x0017  0x4004  0x02c            0     0     -
 10        129     0  0x0015  0x4212  0x028            0     -     -
 11        128     0  0x0018  0x4004  0x02c            0     0     -
 12        127     0  0x0017  0x4004  0x02c            0     0     -
 13        126     0  0x0015  0x4212  0x028            0     -     -
 14        125     0  0x0018  0x4004  0x02c            0     0     -
 15        124     0  0x0017  0x4004  0x02c            0     0     -
... (48 entries not read)

