smartctl 7.1 2019-12-30 r5022 [FreeBSD 12.1-STABLE amd64] (local build)
Copyright (C) 2002-19, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Number:                       PM961 NVMe SAMSUNG 512GB
Serial Number:                      --
Firmware Version:                   CXY74D1Q
PCI Vendor/Subsystem ID:            0x144d
IEEE OUI Identifier:                0x002538
Total NVM Capacity:                 512,110,190,592 [512 GB]
Unallocated NVM Capacity:           0
Controller ID:                      2
Number of Namespaces:               1
Namespace 1 Size/Capacity:          512,110,190,592 [512 GB]
Namespace 1 Utilization:            429,107,023,872 [429 GB]
Namespace 1 Formatted LBA Size:     512
Namespace 1 IEEE EUI-64:            002538 ...
Local Time is:                      Sat Jul  4 19:43:12 2020 EEST
Firmware Updates (0x16):            3 Slots, no Reset required
Optional Admin Commands (0x0017):   Security Format Frmw_DL Self_Test
Optional NVM Commands (0x001f):     Comp Wr_Unc DS_Mngmt Wr_Zero Sav/Sel_Feat
Warning  Comp. Temp. Threshold:     68 Celsius
Critical Comp. Temp. Threshold:     71 Celsius

Supported Power States
St Op     Max   Active     Idle   RL RT WL WT  Ent_Lat  Ex_Lat
 0 +     7.60W       -        -    0  0  0  0        0       0
 1 +     5.00W       -        -    1  1  1  1        0       0
 2 +     3.60W       -        -    2  2  2  2        0       0
 3 -   0.0400W       -        -    3  3  3  3      210    1500
 4 -   0.0050W       -        -    4  4  4  4     2200    6000

Supported LBA Sizes (NSID 0x1)
Id Fmt  Data  Metadt  Rel_Perf
 0 +     512       0         0

=== START OF SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

SMART/Health Information (NVMe Log 0x02)
Critical Warning:                   0x00
Temperature:                        42 Celsius
Available Spare:                    100%
Available Spare Threshold:          50%
Percentage Used:                    2%
Data Units Read:                    33,864,021 [17.3 TB]
Data Units Written:                 37,459,559 [19.1 TB]
Host Read Commands:                 561,827,159
Host Write Commands:                1,261,251,634
Controller Busy Time:               2,260
Power Cycles:                       1,341
Power On Hours:                     2,787
Unsafe Shutdowns:                   453
Media and Data Integrity Errors:    0
Error Information Log Entries:      2,956
Warning  Comp. Temperature Time:    0
Critical Comp. Temperature Time:    0
Temperature Sensor 1:               42 Celsius
Temperature Sensor 2:               55 Celsius

Error Information (NVMe Log 0x01, max 64 entries)
Num   ErrCount  SQId   CmdId  Status  PELoc          LBA  NSID    VS
  0       2956     0  0x0006  0x4016  0x004            0     1     -
  1       2955     0  0x0054  0x4212  0x028            0     -     -
  2       2954     0  0x0020  0x4004  0x02c            0     0     -
  3       2953     0  0x001f  0x4004  0x02c            0     0     -
  4       2952     0  0x0002  0x4004  0x028            0     0     -
  5       2951     0  0x0006  0x4016  0x004            0     1     -
  6       2950     0  0x0006  0x4016  0x004            0     1     -
  7       2949     0  0x007c  0x4212  0x028            0     -     -
  8       2948     0  0x0020  0x4004  0x02c            0     0     -
  9       2947     0  0x001f  0x4004  0x02c            0     0     -
 10       2946     0  0x0002  0x4004  0x028            0     0     -
 11       2945     0  0x0006  0x4016  0x004            0     1     -
 12       2944     0  0x0006  0x4016  0x004            0     1     -
 13       2943     0  0x0088  0x4212  0x028            0     -     -
 14       2942     0  0x0020  0x4004  0x02c            0     0     -
 15       2941     0  0x001f  0x4004  0x02c            0     0     -
... (48 entries not shown)

