smartctl 7.2 2020-12-30 r5155 [FreeBSD 12.1-RELEASE amd64] (local build)
Copyright (C) 2002-20, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Seagate Barracuda 7200.14 (AF)
Device Model:     ST500DM002-1BD142
Serial Number:    --
LU WWN Device Id: 5 000c50 ...
Firmware Version: KC45
User Capacity:    500,107,862,016 bytes [500 GB]
Sector Sizes:     512 bytes logical, 4096 bytes physical
Rotation Rate:    7200 rpm
Device is:        In smartctl database [for details use: -P show]
ATA Version is:   ATA8-ACS T13/1699-D revision 4
SATA Version is:  SATA 3.0, 6.0 Gb/s (current: 3.0 Gb/s)
Local Time is:    Sat Apr 17 14:24:03 2021 UTC
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM level is:     208 (intermediate), recommended: 208
APM feature is:   Unavailable
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, frozen [SEC2]
Wt Cache Reorder: Enabled

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED
See vendor-specific Attribute list for marginal Attributes.

General SMART Values:
Offline data collection status:  (0x82)	Offline data collection activity
					was completed without error.
					Auto Offline Data Collection: Enabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(  600) seconds.
Offline data collection
capabilities: 			 (0x7b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   1) minutes.
Extended self-test routine
recommended polling time: 	 (  81) minutes.
Conveyance self-test routine
recommended polling time: 	 (   2) minutes.
SCT capabilities: 	       (0x303f)	SCT Status supported.
					SCT Error Recovery Control supported.
					SCT Feature Control supported.
					SCT Data Table supported.

SMART Attributes Data Structure revision number: 10
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     POSR--   108   072   006    -    19684464
  3 Spin_Up_Time            PO----   100   097   000    -    0
  4 Start_Stop_Count        -O--CK   037   037   020    -    65535
  5 Reallocated_Sector_Ct   PO--CK   095   095   036    -    1648
  7 Seek_Error_Rate         POSR--   071   060   030    -    103435131439
  9 Power_On_Hours          -O--CK   083   083   000    -    15113
 10 Spin_Retry_Count        PO--C-   100   100   097    -    0
 12 Power_Cycle_Count       -O--CK   096   096   020    -    5027
183 Runtime_Bad_Block       -O--CK   096   096   000    -    4
184 End-to-End_Error        -O--CK   100   100   099    -    0
187 Reported_Uncorrect      -O--CK   001   001   000    -    2508
188 Command_Timeout         -O--CK   100   081   000    -    4 4 155
189 High_Fly_Writes         -O-RCK   100   100   000    -    0
190 Airflow_Temperature_Cel -O---K   062   044   045    Past 38 (Min/Max 36/41 #49)
194 Temperature_Celsius     -O---K   038   056   000    -    38 (0 17 0 0 0)
195 Hardware_ECC_Recovered  -O-RC-   026   020   000    -    19684464
197 Current_Pending_Sector  -O--C-   100   030   000    -    0
198 Offline_Uncorrectable   ----C-   100   030   000    -    0
199 UDMA_CRC_Error_Count    -OSRCK   200   177   000    -    995
240 Head_Flying_Hours       ------   100   253   000    -    15085h+40m+33.395s
241 Total_LBAs_Written      ------   100   253   000    -    723767495
242 Total_LBAs_Read         ------   100   253   000    -    1405066294
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory Version 1
SMART           Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00       GPL,SL  R/O      1  Log Directory
0x01           SL  R/O      1  Summary SMART error log
0x02           SL  R/O      5  Comprehensive SMART error log
0x03       GPL     R/O      5  Ext. Comprehensive SMART error log
0x06           SL  R/O      1  SMART self-test log
0x07       GPL     R/O      1  Extended self-test log
0x09           SL  R/W      1  Selective self-test log
0x10       GPL     R/O      1  NCQ Command Error log
0x11       GPL     R/O      1  SATA Phy Event Counters log
0x21       GPL     R/O      1  Write stream error log
0x22       GPL     R/O      1  Read stream error log
0x80-0x9f  GPL,SL  R/W     16  Host vendor specific log
0xa1       GPL,SL  VS      20  Device vendor specific log
0xa2       GPL     VS    2248  Device vendor specific log
0xa8       GPL,SL  VS     129  Device vendor specific log
0xa9       GPL,SL  VS       1  Device vendor specific log
0xab       GPL     VS       1  Device vendor specific log
0xb0       GPL     VS    2928  Device vendor specific log
0xbd       GPL     VS     252  Device vendor specific log
0xbe-0xbf  GPL     VS   65535  Device vendor specific log
0xc0       GPL,SL  VS       1  Device vendor specific log
0xe0       GPL,SL  R/W      1  SCT Command/Status
0xe1       GPL,SL  R/W      1  SCT Data Transfer

SMART Extended Comprehensive Error Log Version: 1 (5 sectors)
Device Error Count: 2534 (device log contains only the most recent 20 errors)
	CR     = Command Register
	FEATR  = Features Register
	COUNT  = Count (was: Sector Count) Register
	LBA_48 = Upper bytes of LBA High/Mid/Low Registers ]  ATA-8
	LH     = LBA High (was: Cylinder High) Register    ]   LBA
	LM     = LBA Mid (was: Cylinder Low) Register      ] Register
	LL     = LBA Low (was: Sector Number) Register     ]
	DV     = Device (was: Device/Head) Register
	DC     = Device Control Register
	ER     = Error register
	ST     = Status register
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 2534 [13] occurred at disk power-on lifetime: 10941 hours (455 days + 21 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 00 a3 19 98 00 00  Error: WP at LBA = 0x00a31998 = 10688920

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 00 00 00 08 00 00 06 0a 7f f0 40 00     03:07:50.981  WRITE FPDMA QUEUED
  60 00 00 00 08 00 00 15 0d 84 38 40 00     03:07:50.981  READ FPDMA QUEUED
  61 00 00 00 08 00 00 06 0a 7f c0 40 00     03:07:50.980  WRITE FPDMA QUEUED
  61 00 00 00 d0 00 00 1c 94 22 58 40 00     03:07:50.979  WRITE FPDMA QUEUED
  60 00 00 00 08 00 00 17 ce 4b d0 40 00     03:07:50.979  READ FPDMA QUEUED

Error 2533 [12] occurred at disk power-on lifetime: 10941 hours (455 days + 21 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 00 a3 19 98 00 00  Error: WP at LBA = 0x00a31998 = 10688920

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 00 00 00 10 00 00 06 21 79 70 40 00     03:07:47.125  WRITE FPDMA QUEUED
  60 00 00 00 08 00 00 00 a3 19 98 40 00     03:07:47.124  READ FPDMA QUEUED
  61 00 00 00 08 00 00 1c 94 22 50 40 00     03:07:47.124  WRITE FPDMA QUEUED
  ea 00 00 00 00 00 00 00 00 00 00 a0 00     03:07:47.051  FLUSH CACHE EXT
  61 00 00 00 10 00 00 06 21 78 b0 40 00     03:07:47.025  WRITE FPDMA QUEUED

Error 2532 [11] occurred at disk power-on lifetime: 10941 hours (455 days + 21 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 00 a3 19 98 00 00  Error: WP at LBA = 0x00a31998 = 10688920

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 00 00 05 78 00 00 06 2a 61 60 40 00     03:07:43.096  WRITE FPDMA QUEUED
  61 00 00 00 b8 00 00 06 21 a1 e0 40 00     03:07:43.095  WRITE FPDMA QUEUED
  61 00 00 02 f8 00 00 06 29 9f 78 40 00     03:07:43.093  WRITE FPDMA QUEUED
  61 00 00 00 90 00 00 06 21 9c 38 40 00     03:07:43.093  WRITE FPDMA QUEUED
  61 00 00 00 10 00 00 06 21 77 50 40 00     03:07:43.092  WRITE FPDMA QUEUED

Error 2531 [10] occurred at disk power-on lifetime: 10941 hours (455 days + 21 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 00 a3 19 98 00 00  Error: UNC at LBA = 0x00a31998 = 10688920

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 00 08 00 00 00 a3 19 98 40 00     03:07:39.371  READ FPDMA QUEUED
  60 00 00 00 08 00 00 00 a3 19 90 40 00     03:07:39.371  READ FPDMA QUEUED
  60 00 00 00 08 00 00 00 a3 19 88 40 00     03:07:39.370  READ FPDMA QUEUED
  60 00 00 00 08 00 00 00 a3 19 80 40 00     03:07:39.370  READ FPDMA QUEUED
  60 00 00 00 08 00 00 00 a3 19 78 40 00     03:07:39.370  READ FPDMA QUEUED

Error 2530 [9] occurred at disk power-on lifetime: 10941 hours (455 days + 21 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 00 a3 19 98 00 00  Error: UNC at LBA = 0x00a31998 = 10688920

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 00 e0 00 00 1c 14 2f 20 40 00     03:07:35.444  READ FPDMA QUEUED
  60 00 00 04 00 00 00 00 a3 18 c0 40 00     03:07:35.418  READ FPDMA QUEUED
  60 00 00 04 00 00 00 1c 14 2b 20 40 00     03:07:34.990  READ FPDMA QUEUED
  60 00 00 04 00 00 00 1c 14 27 20 40 00     03:07:34.426  READ FPDMA QUEUED
  ea 00 00 00 00 00 00 00 00 00 00 a0 00     03:07:34.276  FLUSH CACHE EXT

Error 2529 [8] occurred at disk power-on lifetime: 10822 hours (450 days + 22 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 00 b2 be 28 00 00  Error: WP at LBA = 0x00b2be28 = 11714088

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 00 00 00 10 00 00 00 0b 81 30 40 00     02:18:55.040  WRITE FPDMA QUEUED
  61 00 00 00 08 00 00 00 0b 81 08 40 00     02:18:55.040  WRITE FPDMA QUEUED
  61 00 00 00 08 00 00 00 0b 80 f0 40 00     02:18:55.040  WRITE FPDMA QUEUED
  61 00 00 00 08 00 00 00 0b 80 a8 40 00     02:18:55.039  WRITE FPDMA QUEUED
  61 00 00 00 10 00 00 00 0b 80 80 40 00     02:18:55.039  WRITE FPDMA QUEUED

Error 2528 [7] occurred at disk power-on lifetime: 10822 hours (450 days + 22 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 00 b2 be 28 00 00  Error: WP at LBA = 0x00b2be28 = 11714088

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 00 00 00 08 00 00 2d 14 2f f8 40 00     02:18:51.249  WRITE FPDMA QUEUED
  61 00 00 00 30 00 00 2d 14 5e e0 40 00     02:18:51.248  WRITE FPDMA QUEUED
  61 00 00 00 70 00 00 1c 92 78 40 40 00     02:18:51.243  WRITE FPDMA QUEUED
  61 00 00 00 20 00 00 2d 14 5e c0 40 00     02:18:51.243  WRITE FPDMA QUEUED
  60 00 00 00 18 00 00 23 2c ab 00 40 00     02:18:51.199  READ FPDMA QUEUED

Error 2527 [6] occurred at disk power-on lifetime: 10822 hours (450 days + 22 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 00 b2 be 28 00 00  Error: UNC at LBA = 0x00b2be28 = 11714088

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 00 08 00 00 00 9d 08 c0 40 00     02:18:47.423  READ FPDMA QUEUED
  60 00 00 00 08 00 00 00 df 01 a0 40 00     02:18:47.423  READ FPDMA QUEUED
  60 00 00 00 08 00 00 00 9d 08 b8 40 00     02:18:47.422  READ FPDMA QUEUED
  60 00 00 00 08 00 00 00 df 01 98 40 00     02:18:47.422  READ FPDMA QUEUED
  60 00 00 00 08 00 00 00 9d 08 b0 40 00     02:18:47.421  READ FPDMA QUEUED

SMART Extended Self-test Log Version: 1 (1 sectors)
Num  Test_Description    Status                  Remaining  LifeTime(hours)  LBA_of_first_error
# 1  Short offline       Completed without error       00%     14454         -
# 2  Short offline       Completed without error       00%     10586         -
# 3  Short offline       Completed without error       00%     10572         -
# 4  Short offline       Completed without error       00%     10558         -
# 5  Short offline       Completed without error       00%     10546         -

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Status Version:                  3
SCT Version (vendor specific):       522 (0x020a)
Device State:                        Active (0)
Current Temperature:                    38 Celsius
Power Cycle Min/Max Temperature:     36/41 Celsius
Lifetime    Min/Max Temperature:     17/56 Celsius
Under/Over Temperature Limit Count:   0/0

SCT Temperature History Version:     2
Temperature Sampling Period:         1 minute
Temperature Logging Interval:        59 minutes
Min/Max recommended Temperature:     14/55 Celsius
Min/Max Temperature Limit:           10/60 Celsius
Temperature History Size (Index):    128 (114)

SCT Error Recovery Control:
           Read: Disabled
          Write: Disabled

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11)
ID      Size     Value  Description
0x000a  2           14  Device-to-host register FISes sent due to a COMRESET
0x0001  2            0  Command failed due to ICRC error
0x0003  2            0  R_ERR response for device-to-host data FIS
0x0004  2            0  R_ERR response for host-to-device data FIS
0x0006  2            0  R_ERR response for device-to-host non-data FIS
0x0007  2            0  R_ERR response for host-to-device non-data FIS

