smartctl 7.2 2020-12-30 r5155 [FreeBSD 12.1-RELEASE-p12-HBSD amd64] (local build)
Copyright (C) 2002-20, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Device Model:     Innodisk Corp. mSATA 3SE DEMSR- 02GB
Serial Number:    --
Firmware Version: S130604
User Capacity:    1,987,051,520 bytes [1.98 GB]
Sector Size:      512 bytes logical/physical
Rotation Rate:    Solid State Device
Form Factor:      2.5 inches
TRIM Command:     Unavailable
Device is:        Not in smartctl database [for details use: -P showall]
ATA Version is:   ACS-2 (minor revision not indicated)
SATA Version is:  SATA 3.0, 6.0 Gb/s (current: 6.0 Gb/s)
Local Time is:    Sun Feb 28 15:15:31 2021 UTC
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Unavailable
APM feature is:   Unavailable
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, frozen [SEC2]
Read SCT Status failed: Input/output error
Wt Cache Reorder: Unknown (SCT Feature Control command failed)

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x00)	Offline data collection activity
					was never started.
					Auto Offline Data Collection: Disabled.
Total time to complete Offline 
data collection: 		(   32) seconds.
Offline data collection
capabilities: 			 (0x00) 	Offline data collection not supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x00)	Error logging NOT supported.
					General Purpose Logging supported.
SCT capabilities: 	       (0x0039)	SCT Status supported.
					SCT Error Recovery Control supported.
					SCT Feature Control supported.
					SCT Data Table supported.

SMART Attributes Data Structure revision number: 16
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     ------   000   000   000    -    0
  2 Throughput_Performance  ------   000   000   000    -    0
  3 Spin_Up_Time            ------   000   000   000    -    0
  5 Reallocated_Sector_Ct   ------   000   000   000    -    0
  7 Unknown_SSD_Attribute   ------   000   000   000    -    0
  8 Unknown_SSD_Attribute   ------   000   000   000    -    0
  9 Power_On_Hours          ------   000   000   000    -    14819
 10 Unknown_SSD_Attribute   ------   000   000   000    -    0
 12 Power_Cycle_Count       ------   000   000   000    -    789
  1 Raw_Read_Error_Rate     ------   000   000   000    -    0
168 Unknown_Attribute       ------   000   000   000    -    0
169 Unknown_Attribute       ------   000   000   000    -    0
  1 Raw_Read_Error_Rate     ------   000   000   000    -    0
175 Program_Fail_Count_Chip ------   100   000   000    -    0
192 Power-Off_Retract_Count ------   000   000   000    -    0
  1 Raw_Read_Error_Rate     ------   000   000   000    -    2199023255552
197 Current_Pending_Sector  ------   000   000   000    -    0
240 Unknown_SSD_Attribute   ------   000   000   000    -    0
170 Unknown_Attribute       PO----   100   100   ---    -    262144
173 Unknown_Attribute       -O--C-   100   100   ---    -    4718637
229 Unknown_Attribute       -O----   100   100   ---    -    23597197349784
236 Unknown_Attribute       -O----   100   100   ---    -    0
235 Unknown_Attribute       -O----   100   000   ---    -    0
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

Read SMART Log Directory failed: Input/output error

ATA_READ_LOG_EXT (addr=0x00:0x00, page=0, n=1) failed: Input/output error
Read GP Log Directory failed

SMART Extended Comprehensive Error Log (GP Log 0x03) not supported

SMART Error Log not supported

SMART Extended Self-test Log (GP Log 0x07) not supported

SMART Self-test Log not supported

Selective Self-tests/Logging not supported

Read SCT Status failed: Input/output error

Read SCT Status failed: Input/output error
SCT (Get) Error Recovery Control command failed

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

ATA_READ_LOG_EXT (addr=0x11:0x00, page=0, n=1) failed: Input/output error
Read SATA Phy Event Counters failed

