smartctl 7.3 2022-02-28 r5338 [OpenBSD 7.2 amd64] (local build)
Copyright (C) 2002-22, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Toshiba 2.5" HDD MK..75GSX
Device Model:     TOSHIBA MK6475GSX
Serial Number:    --
LU WWN Device Id: 5 000039 ...
Firmware Version: GT001M
User Capacity:    640,135,028,736 bytes [640 GB]
Sector Size:      512 bytes logical/physical
Rotation Rate:    5400 rpm
Form Factor:      2.5 inches
Device is:        In smartctl database 7.3/5319
ATA Version is:   ATA8-ACS (minor revision not indicated)
SATA Version is:  SATA 2.6, 3.0 Gb/s (current: 3.0 Gb/s)
Local Time is:    Fri Dec 23 22:21:13 2022 EET
SMART support is: Available - device has SMART capability.
SMART support is: Enabled

=== START OF READ SMART DATA SECTION ===
SMART Status not supported: Incomplete response, ATA output registers missing
SMART overall-health self-assessment test result: PASSED
Warning: This result is based on an Attribute check.

General SMART Values:
Offline data collection status:  (0x00)	Offline data collection activity
					was never started.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(  120) seconds.
Offline data collection
capabilities: 			 (0x5b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					No Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   2) minutes.
Extended self-test routine
recommended polling time: 	 ( 207) minutes.
SCT capabilities: 	       (0x003d)	SCT Status supported.
					SCT Error Recovery Control supported.
					SCT Feature Control supported.
					SCT Data Table supported.

SMART Attributes Data Structure revision number: 16
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAG     VALUE WORST THRESH TYPE      UPDATED  WHEN_FAILED RAW_VALUE
  1 Raw_Read_Error_Rate     0x000b   100   100   050    Pre-fail  Always       -       0
  2 Throughput_Performance  0x0005   100   100   050    Pre-fail  Offline      -       0
  3 Spin_Up_Time            0x0027   100   100   001    Pre-fail  Always       -       1337
  4 Start_Stop_Count        0x0032   100   100   000    Old_age   Always       -       8126
  5 Reallocated_Sector_Ct   0x0033   100   100   050    Pre-fail  Always       -       8
  7 Seek_Error_Rate         0x000b   100   100   050    Pre-fail  Always       -       0
  8 Seek_Time_Performance   0x0005   100   100   050    Pre-fail  Offline      -       0
  9 Power_On_Hours          0x0032   071   071   000    Old_age   Always       -       11864
 10 Spin_Retry_Count        0x0033   253   100   030    Pre-fail  Always       -       0
 12 Power_Cycle_Count       0x0032   100   100   000    Old_age   Always       -       7882
191 G-Sense_Error_Rate      0x0032   100   100   000    Old_age   Always       -       3900
192 Power-Off_Retract_Count 0x0032   099   099   000    Old_age   Always       -       745
193 Load_Cycle_Count        0x0032   096   096   000    Old_age   Always       -       44267
194 Temperature_Celsius     0x0022   100   100   000    Old_age   Always       -       41 (Min/Max 9/65)
196 Reallocated_Event_Count 0x0032   100   100   000    Old_age   Always       -       1
197 Current_Pending_Sector  0x0032   100   100   000    Old_age   Always       -       0
198 Offline_Uncorrectable   0x0030   100   100   000    Old_age   Offline      -       0
199 UDMA_CRC_Error_Count    0x0032   200   200   000    Old_age   Always       -       0
220 Disk_Shift              0x0002   100   100   000    Old_age   Always       -       86
222 Loaded_Hours            0x0032   074   074   000    Old_age   Always       -       10749
223 Load_Retry_Count        0x0032   100   100   000    Old_age   Always       -       0
224 Load_Friction           0x0022   100   100   000    Old_age   Always       -       0
226 Load-in_Time            0x0026   100   100   000    Old_age   Always       -       237
240 Head_Flying_Hours       0x0001   100   100   001    Pre-fail  Offline      -       0

SMART Error Log Version: 1
ATA Error Count: 114 (device log contains only the most recent five errors)
	CR = Command Register [HEX]
	FR = Features Register [HEX]
	SC = Sector Count Register [HEX]
	SN = Sector Number Register [HEX]
	CL = Cylinder Low Register [HEX]
	CH = Cylinder High Register [HEX]
	DH = Device/Head Register [HEX]
	DC = Device Command Register [HEX]
	ER = Error register [HEX]
	ST = Status register [HEX]
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 114 occurred at disk power-on lifetime: 7890 hours (328 days + 18 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  40 41 7a d0 b1 c4 66  Error: UNC at LBA = 0x06c4b1d0 = 113553872

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  60 80 88 d8 3b 01 40 00      02:06:37.514  READ FPDMA QUEUED
  60 30 80 58 b1 f9 40 00      02:06:37.514  READ FPDMA QUEUED
  60 40 78 c8 b1 c4 40 00      02:06:37.514  READ FPDMA QUEUED
  60 40 70 ca e6 31 40 00      02:06:37.514  READ FPDMA QUEUED
  60 28 60 f0 c2 88 40 00      02:06:37.514  READ FPDMA QUEUED

Error 113 occurred at disk power-on lifetime: 7890 hours (328 days + 18 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  40 41 22 d0 b1 c4 66  Error: UNC at LBA = 0x06c4b1d0 = 113553872

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  60 68 18 50 77 31 40 00      02:06:26.061  READ FPDMA QUEUED
  60 08 08 30 60 03 40 00      02:06:26.056  READ FPDMA QUEUED
  60 40 10 f2 2a d4 40 00      02:06:26.049  READ FPDMA QUEUED
  60 20 18 8b a4 ff 40 00      02:06:26.045  READ FPDMA QUEUED
  60 08 30 20 66 bc 40 00      02:06:26.045  READ FPDMA QUEUED

Error 112 occurred at disk power-on lifetime: 7890 hours (328 days + 18 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  40 41 6a d0 b1 c4 66  Error: UNC at LBA = 0x06c4b1d0 = 113553872

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  60 18 70 28 54 e1 40 00      02:05:26.484  READ FPDMA QUEUED
  60 20 18 da b0 ff 40 00      02:05:26.480  READ FPDMA QUEUED
  60 08 68 d0 b1 c4 40 00      02:05:26.474  READ FPDMA QUEUED
  60 08 60 20 66 bc 40 00      02:05:26.473  READ FPDMA QUEUED
  60 40 50 f2 2a d4 40 00      02:05:26.473  READ FPDMA QUEUED

Error 111 occurred at disk power-on lifetime: 7890 hours (328 days + 18 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  40 41 0a d0 b1 c4 66  Error: UNC at LBA = 0x06c4b1d0 = 113553872

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  60 08 58 20 f4 11 40 00      02:04:25.891  READ FPDMA QUEUED
  60 20 50 da 44 67 40 00      02:04:25.891  READ FPDMA QUEUED
  60 10 48 f8 e8 01 40 00      02:04:25.891  READ FPDMA QUEUED
  61 08 68 00 10 fb 40 00      02:04:25.891  WRITE FPDMA QUEUED
  60 08 40 40 59 f5 40 00      02:04:25.891  READ FPDMA QUEUED

Error 110 occurred at disk power-on lifetime: 7890 hours (328 days + 18 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  40 41 6a d0 b1 c4 66  Error: WP at LBA = 0x06c4b1d0 = 113553872

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  61 08 70 e0 ef db 40 00      02:03:24.996  WRITE FPDMA QUEUED
  60 08 68 d0 b1 c4 40 00      02:03:24.996  READ FPDMA QUEUED
  61 08 68 60 13 d9 40 00      02:03:24.996  WRITE FPDMA QUEUED
  60 08 60 20 66 bc 40 00      02:03:24.996  READ FPDMA QUEUED
  61 08 60 e8 81 67 40 00      02:03:24.995  WRITE FPDMA QUEUED

SMART Self-test log structure revision number 1
No self-tests have been logged.  [To run self-tests, use: smartctl -t]

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.



