smartctl 6.6 2017-11-05 r4594 [FreeBSD 11.4-RELEASE-p5 i386] (local build)
Copyright (C) 2002-17, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Western Digital Caviar SE
Device Model:     WDC WD2000JB-00GVC0
Serial Number:    --
Firmware Version: 08.02D08
User Capacity:    200,049,647,616 bytes [200 GB]
Sector Size:      512 bytes logical/physical
Device is:        In smartctl database [for details use: -P show]
ATA Version is:   ATA/ATAPI-6 (minor revision not indicated)
Local Time is:    Sun Dec  6 00:35:06 2020 +04
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Disabled
APM feature is:   Unavailable
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, NOT FROZEN [SEC1]
Write SCT (Get) Feature Control Command failed: Read of ATA output registers not implemented [JMicron]
Wt Cache Reorder: Unknown (SCT Feature Control command failed)

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x84)	Offline data collection activity
					was suspended by an interrupting command from host.
					Auto Offline Data Collection: Enabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		( 5778) seconds.
Offline data collection
capabilities: 			 (0x7b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					No General Purpose Logging support.
Short self-test routine 
recommended polling time: 	 (   2) minutes.
Extended self-test routine
recommended polling time: 	 (  75) minutes.
Conveyance self-test routine
recommended polling time: 	 (   5) minutes.
SCT capabilities: 	       (0x003f)	SCT Status supported.
					SCT Error Recovery Control supported.
					SCT Feature Control supported.
					SCT Data Table supported.

SMART Attributes Data Structure revision number: 16
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     PO-R--   200   200   051    -    0
  3 Spin_Up_Time            POS---   115   101   021    -    6791
  4 Start_Stop_Count        -O--CK   092   092   040    -    8715
  5 Reallocated_Sector_Ct   PO--CK   200   200   140    -    0
  7 Seek_Error_Rate         PO-R--   200   200   051    -    0
  9 Power_On_Hours          -O--CK   001   001   000    -    84955
 10 Spin_Retry_Count        PO--C-   100   100   051    -    0
 11 Calibration_Retry_Count PO--C-   100   100   051    -    0
 12 Power_Cycle_Count       -O--CK   096   096   000    -    4140
194 Temperature_Celsius     -O---K   117   090   000    -    33
196 Reallocated_Event_Count -O--CK   200   200   000    -    0
197 Current_Pending_Sector  -O--C-   200   200   000    -    0
198 Offline_Uncorrectable   -O--C-   200   200   000    -    0
199 UDMA_CRC_Error_Count    -O-R--   200   253   000    -    10
200 Multi_Zone_Error_Rate   P--R--   200   200   051    -    0
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory not supported

SMART Log Directory Version 0
Address    Access  R/W   Size  Description
0x00           SL  R/O      1  Log Directory

SMART Extended Comprehensive Error Log (GP Log 0x03) not supported

SMART Error Log Version: 1
ATA Error Count: 14 (device log contains only the most recent five errors)
	CR = Command Register [HEX]
	FR = Features Register [HEX]
	SC = Sector Count Register [HEX]
	SN = Sector Number Register [HEX]
	CL = Cylinder Low Register [HEX]
	CH = Cylinder High Register [HEX]
	DH = Device/Head Register [HEX]
	DC = Device Command Register [HEX]
	ER = Error register [HEX]
	ST = Status register [HEX]
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 14 occurred at disk power-on lifetime: 10847 hours (451 days + 23 hours)
  When the command that caused the error occurred, the device was doing SMART Offline or Self-test.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  40 51 20 07 73 54 e0  Error: UNC 32 sectors at LBA = 0x00547307 = 5534471

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  25 d5 20 ff 72 54 02 00      12:10:19.750  READ DMA EXT
  25 d5 04 db 62 59 02 00      12:10:19.750  READ DMA EXT
  25 d5 04 8b b2 8a 01 00      12:10:19.750  READ DMA EXT
  25 d5 04 1f b4 8a 01 00      12:10:19.750  READ DMA EXT
  25 d5 04 2b b2 8a 01 00      12:10:19.750  READ DMA EXT

Error 13 occurred at disk power-on lifetime: 10835 hours (451 days + 11 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  40 51 20 07 73 54 e0  Error: UNC 32 sectors at LBA = 0x00547307 = 5534471

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  25 d5 20 ff 72 54 02 00      00:05:36.750  READ DMA EXT
  25 d5 20 df 72 54 02 00      00:05:36.750  READ DMA EXT
  25 d5 20 bf 72 54 02 00      00:05:36.750  READ DMA EXT
  25 d5 20 9f 72 54 02 00      00:05:36.750  READ DMA EXT
  25 d5 20 9f 9d 53 02 00      00:05:36.750  READ DMA EXT

Error 12 occurred at disk power-on lifetime: 2829 hours (117 days + 21 hours)
  When the command that caused the error occurred, the device was doing SMART Offline or Self-test.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  40 51 f0 7f 46 ab e0  Error: UNC 240 sectors at LBA = 0x00ab467f = 11224703

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  25 00 f0 00 46 ab 06 00      03:58:03.050  READ DMA EXT
  25 00 f0 00 46 ab 06 00      03:58:03.050  READ DMA EXT
  25 00 f0 00 46 ab 06 00      03:58:03.050  READ DMA EXT
  25 00 f0 00 46 ab 06 00      03:58:03.050  READ DMA EXT
  25 00 f0 00 46 ab 06 00      03:58:03.050  READ DMA EXT

Error 11 occurred at disk power-on lifetime: 2829 hours (117 days + 21 hours)
  When the command that caused the error occurred, the device was doing SMART Offline or Self-test.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  40 51 f0 7f 46 ab e0  Error: UNC 240 sectors at LBA = 0x00ab467f = 11224703

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  25 00 f0 00 46 ab 06 00      03:58:00.950  READ DMA EXT
  25 00 f0 00 46 ab 06 00      03:58:00.950  READ DMA EXT
  25 00 f0 00 46 ab 06 00      03:58:00.950  READ DMA EXT
  25 00 f0 00 46 ab 06 00      03:58:00.950  READ DMA EXT
  25 00 f0 00 46 ab 06 00      03:58:00.950  READ DMA EXT

Error 10 occurred at disk power-on lifetime: 2829 hours (117 days + 21 hours)
  When the command that caused the error occurred, the device was doing SMART Offline or Self-test.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  40 51 f0 7f 46 ab e0  Error: UNC 240 sectors at LBA = 0x00ab467f = 11224703

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  25 00 f0 00 46 ab 06 00      03:57:58.900  READ DMA EXT
  25 00 f0 00 46 ab 06 00      03:57:58.900  READ DMA EXT
  25 00 f0 00 46 ab 06 00      03:57:58.900  READ DMA EXT
  25 00 f0 00 46 ab 06 00      03:57:58.900  READ DMA EXT
  25 00 10 f0 46 ab 06 00      03:57:58.900  READ DMA EXT

SMART Extended Self-test Log (GP Log 0x07) not supported

SMART Self-test log structure revision number 1
Num  Test_Description    Status                  Remaining  LifeTime(hours)  LBA_of_first_error
# 1  Conveyance offline  Completed without error       00%      5688         -
# 2  Conveyance offline  Completed without error       00%      2757         -

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Status Version:                  2
SCT Version (vendor specific):       258 (0x0102)
SCT Support Level:                   1
Device State:                        SMART Off-line Data Collection executing in background (4)
Current Temperature:                 33 Celsius
Power Cycle Max Temperature:         42 Celsius
Lifetime    Max Temperature:         60 Celsius

SCT Temperature History Version:     2
Temperature Sampling Period:         1 minute
Temperature Logging Interval:        1 minute
Min/Max recommended Temperature:      5/55 Celsius
Min/Max Temperature Limit:            1/60 Celsius
Temperature History Size (Index):    128 (116)

Write SCT (Get) Error Recovery Control Command failed: Read of ATA output registers not implemented [JMicron]
SCT (Get) Error Recovery Control command failed

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11) not supported



