smartctl 7.2 2020-12-30 r5155 [FreeBSD 13.0-RELEASE-p5 amd64] (local build)
Copyright (C) 2002-20, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Seagate Barracuda 7200.7 and 7200.7 Plus
Device Model:     ST3200822AS
Serial Number:    --
Firmware Version: 3.02
User Capacity:    200,049,647,616 bytes [200 GB]
Sector Size:      512 bytes logical/physical
Device is:        In smartctl database [for details use: -P show]
ATA Version is:   ATA/ATAPI-6 T13/1410D revision 2
Local Time is:    Sat Jan  1 11:14:16 2022 MST
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Unavailable
APM feature is:   Unavailable
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Unavailable
Wt Cache Reorder: Unavailable

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x82)	Offline data collection activity
					was completed without error.
					Auto Offline Data Collection: Enabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(  430) seconds.
Offline data collection
capabilities: 			 (0x5b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					No Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					No General Purpose Logging support.
Short self-test routine 
recommended polling time: 	 (   1) minutes.
Extended self-test routine
recommended polling time: 	 ( 111) minutes.

SMART Attributes Data Structure revision number: 10
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     POSR--   055   046   006    -    93503769
  3 Spin_Up_Time            PO----   096   096   000    -    0
  4 Start_Stop_Count        -O--CK   099   099   020    -    2001
  5 Reallocated_Sector_Ct   PO--CK   070   070   036    -    1222
  7 Seek_Error_Rate         POSR--   089   060   030    -    939346016
  9 Power_On_Hours          -O--CK   012   012   000    -    77296
 10 Spin_Retry_Count        PO--C-   100   100   097    -    0
 12 Power_Cycle_Count       -O--CK   099   099   020    -    1994
194 Temperature_Celsius     -O---K   038   052   000    -    38
195 Hardware_ECC_Recovered  -O-RC-   055   046   000    -    93503769
197 Current_Pending_Sector  -O--C-   100   100   000    -    35
198 Offline_Uncorrectable   ----C-   100   100   000    -    35
199 UDMA_CRC_Error_Count    -OSRCK   200   199   000    -    1
200 Multi_Zone_Error_Rate   ------   100   253   000    -    0
202 Data_Address_Mark_Errs  -O--CK   030   183   000    -    70
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory not supported

SMART Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00           SL  R/O      1  Log Directory
0x01           SL  R/O      1  Summary SMART error log
0x02           SL  R/O      5  Comprehensive SMART error log
0x03           SL  R/O      5  Ext. Comprehensive SMART error log
0x06           SL  R/O      1  SMART self-test log
0x07           SL  R/O      1  Extended self-test log
0x09           SL  R/W      1  Selective self-test log
0x20           SL  R/O      1  Streaming performance log [OBS-8]
0x21           SL  R/O      1  Write stream error log
0x22           SL  R/O      1  Read stream error log
0x23           SL  R/O      1  Delayed sector log [OBS-8]
0x80-0x9f      SL  R/W     16  Host vendor specific log
0xa0           SL  VS       1  Device vendor specific log
0xa1           SL  VS      20  Device vendor specific log
0xa2           SL  VS     101  Device vendor specific log
0xa8           SL  VS      20  Device vendor specific log
0xa9           SL  VS       1  Device vendor specific log
0xb0           SL  VS       1  Device vendor specific log
0xb4           SL  VS       4  Device vendor specific log
0xbe-0xbf      SL  VS       1  Device vendor specific log

SMART Extended Comprehensive Error Log (GP Log 0x03) not supported

SMART Error Log Version: 1
ATA Error Count: 1447 (device log contains only the most recent five errors)
	CR = Command Register [HEX]
	FR = Features Register [HEX]
	SC = Sector Count Register [HEX]
	SN = Sector Number Register [HEX]
	CL = Cylinder Low Register [HEX]
	CH = Cylinder High Register [HEX]
	DH = Device/Head Register [HEX]
	DC = Device Command Register [HEX]
	ER = Error register [HEX]
	ST = Status register [HEX]
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 1447 occurred at disk power-on lifetime: 11713 hours (488 days + 1 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  40 51 97 be c6 13 40  Error: UNC 151 sectors at LBA = 0x0013c6be = 1296062

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  25 00 00 27 c4 13 40 00      17:59:17.983  READ DMA EXT
  25 00 00 27 c4 13 40 00      17:59:17.967  READ DMA EXT
  25 00 00 27 bc 13 40 00      17:59:25.827  READ DMA EXT
  25 00 00 27 b4 13 40 00      17:59:20.812  READ DMA EXT
  25 00 00 27 ac 13 40 00      17:59:19.512  READ DMA EXT

Error 1446 occurred at disk power-on lifetime: 11713 hours (488 days + 1 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  40 51 97 be c6 13 40  Error: UNC 151 sectors at LBA = 0x0013c6be = 1296062

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  25 00 00 27 c4 13 40 00      17:59:17.983  READ DMA EXT
  25 00 00 27 bc 13 40 00      17:59:17.967  READ DMA EXT
  25 00 00 27 b4 13 40 00      17:59:17.944  READ DMA EXT
  25 00 00 27 ac 13 40 00      17:59:20.812  READ DMA EXT
  25 00 00 27 a4 13 40 00      17:59:19.512  READ DMA EXT

Error 1445 occurred at disk power-on lifetime: 10788 hours (449 days + 12 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  40 51 6f fe 5e 1b 40  Error: UNC 111 sectors at LBA = 0x001b5efe = 1793790

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  25 00 00 8f 57 1b 40 00      13:39:13.972  READ DMA EXT
  25 00 00 8f 57 1b 40 00      13:39:13.972  READ DMA EXT
  25 00 00 8f 57 1b 40 00      13:39:13.897  READ DMA EXT
  25 00 00 8f 57 1b 40 00      13:39:35.598  READ DMA EXT
  25 00 00 8f 57 1b 40 00      13:39:31.119  READ DMA EXT

Error 1444 occurred at disk power-on lifetime: 10788 hours (449 days + 12 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  40 51 6f fe 5e 1b 40  Error: UNC 111 sectors at LBA = 0x001b5efe = 1793790

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  25 00 00 8f 57 1b 40 00      13:39:13.972  READ DMA EXT
  25 00 00 8f 57 1b 40 00      13:39:13.972  READ DMA EXT
  25 00 00 8f 57 1b 40 00      13:39:13.897  READ DMA EXT
  25 00 00 8f 57 1b 40 00      13:39:13.727  READ DMA EXT
  25 00 00 8f 4f 1b 40 00      13:39:31.119  READ DMA EXT

Error 1443 occurred at disk power-on lifetime: 10788 hours (449 days + 12 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  40 51 6f fe 5e 1b 40  Error: UNC 111 sectors at LBA = 0x001b5efe = 1793790

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  25 00 00 8f 57 1b 40 00      13:39:13.972  READ DMA EXT
  25 00 00 8f 57 1b 40 00      13:39:13.972  READ DMA EXT
  25 00 00 8f 57 1b 40 00      13:39:13.897  READ DMA EXT
  25 00 00 8f 4f 1b 40 00      13:39:13.727  READ DMA EXT
  25 00 00 8f 47 1b 40 00      13:39:13.696  READ DMA EXT

SMART Extended Self-test Log (GP Log 0x07) not supported

SMART Self-test log structure revision number 1
Num  Test_Description    Status                  Remaining  LifeTime(hours)  LBA_of_first_error
# 1  Short offline       Completed without error       00%      6682         -
# 2  Short offline       Completed without error       00%      6554         -
# 3  Extended offline    Completed without error       00%      4043         -
# 4  Short offline       Completed without error       00%      4042         -
# 5  Short offline       Completed without error       00%      4041         -
# 6  Short offline       Completed without error       00%     35552         -
# 7  Short offline       Completed without error       00%     33649         -
# 8  Short captive       Completed: read failure       90%     33627         182741979
# 9  Extended captive    Completed: read failure       90%     33627         182741979
#10  Extended captive    Completed: read failure       90%     33627         182741979
#11  Short offline       Completed without error       00%         0         -
3 of 3 failed self-tests are outdated by newer successful extended offline self-test # 3

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Commands not supported

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11) not supported



