smartctl 7.3 2022-02-28 r5338 [FreeBSD 12.3-RELEASE-p3 amd64] (local build)
Copyright (C) 2002-22, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Seagate Barracuda 7200.12
Device Model:     ST3500413AS
Serial Number:    --
LU WWN Device Id: 5 000c50 ...
Firmware Version: JC45
User Capacity:    500,107,862,016 bytes [500 GB]
Sector Size:      512 bytes logical/physical
Rotation Rate:    7200 rpm
Device is:        In smartctl database 7.3/5319
ATA Version is:   ATA8-ACS T13/1699-D revision 4
SATA Version is:  SATA 2.6, 6.0 Gb/s (current: 6.0 Gb/s)
Local Time is:    Mon Apr 25 09:09:28 2022 MSK
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM level is:     208 (intermediate), recommended: 208
APM feature is:   Unavailable
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, frozen [SEC2]
Wt Cache Reorder: Unknown

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x82)	Offline data collection activity
					was completed without error.
					Auto Offline Data Collection: Enabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(  600) seconds.
Offline data collection
capabilities: 			 (0x7b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   1) minutes.
Extended self-test routine
recommended polling time: 	 (  83) minutes.
Conveyance self-test routine
recommended polling time: 	 (   2) minutes.
SCT capabilities: 	       (0x103f)	SCT Status supported.
					SCT Error Recovery Control supported.
					SCT Feature Control supported.
					SCT Data Table supported.

SMART Attributes Data Structure revision number: 10
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     POSR--   093   092   006    -    169187332
  3 Spin_Up_Time            PO----   100   100   000    -    0
  4 Start_Stop_Count        -O--CK   100   100   020    -    77
  5 Reallocated_Sector_Ct   PO--CK   091   091   036    -    400
  7 Seek_Error_Rate         POSR--   088   060   030    -    759232387
  9 Power_On_Hours          -O--CK   095   011   000    -    4618
 10 Spin_Retry_Count        PO--C-   100   100   097    -    0
 12 Power_Cycle_Count       -O--CK   100   100   020    -    77
183 Runtime_Bad_Block       -O--CK   100   100   000    -    0
184 End-to-End_Error        -O--CK   100   100   099    -    0
187 Reported_Uncorrect      -O--CK   001   001   000    -    355
188 Command_Timeout         -O--CK   100   097   000    -    506813874591
189 High_Fly_Writes         -O-RCK   095   095   000    -    5
190 Airflow_Temperature_Cel -O---K   078   057   045    -    22 (Min/Max 20/43)
194 Temperature_Celsius     -O---K   022   043   000    -    22 (0 13 0 0 0)
195 Hardware_ECC_Recovered  -O-RC-   022   011   000    -    169187332
197 Current_Pending_Sector  -O--C-   081   081   000    -    803
198 Offline_Uncorrectable   ----C-   081   081   000    -    803
199 UDMA_CRC_Error_Count    -OSRCK   200   199   000    -    16406
240 Head_Flying_Hours       ------   100   253   000    -    82969 (122 85 0)
241 Total_LBAs_Written      ------   100   253   000    -    312636200
242 Total_LBAs_Read         ------   100   253   000    -    3689038254
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory Version 1
SMART           Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00       GPL,SL  R/O      1  Log Directory
0x01       GPL,SL  R/O      1  Summary SMART error log
0x02       GPL,SL  R/O      5  Comprehensive SMART error log
0x03       GPL     R/O      5  Ext. Comprehensive SMART error log
0x06       GPL,SL  R/O      1  SMART self-test log
0x07       GPL     R/O      1  Extended self-test log
0x09       GPL,SL  R/W      1  Selective self-test log
0x10       GPL     R/O      1  NCQ Command Error log
0x11       GPL     R/O      1  SATA Phy Event Counters log
0x21       GPL     R/O      1  Write stream error log
0x22       GPL     R/O      1  Read stream error log
0x80-0x9f  GPL,SL  R/W     16  Host vendor specific log
0xa1       GPL,SL  VS      20  Device vendor specific log
0xa2       GPL     VS    2248  Device vendor specific log
0xa8       GPL,SL  VS     129  Device vendor specific log
0xa9       GPL,SL  VS       1  Device vendor specific log
0xb0       GPL     VS    2928  Device vendor specific log
0xbd       GPL     VS     252  Device vendor specific log
0xbe-0xbf  GPL     VS   65535  Device vendor specific log
0xc0       GPL,SL  VS       1  Device vendor specific log
0xe0       GPL,SL  R/W      1  SCT Command/Status
0xe1       GPL,SL  R/W      1  SCT Data Transfer

SMART Extended Comprehensive Error Log Version: 1 (5 sectors)
Device Error Count: 7
	CR     = Command Register
	FEATR  = Features Register
	COUNT  = Count (was: Sector Count) Register
	LBA_48 = Upper bytes of LBA High/Mid/Low Registers ]  ATA-8
	LH     = LBA High (was: Cylinder High) Register    ]   LBA
	LM     = LBA Mid (was: Cylinder Low) Register      ] Register
	LL     = LBA Low (was: Sector Number) Register     ]
	DV     = Device (was: Device/Head) Register
	DC     = Device Control Register
	ER     = Error register
	ST     = Status register
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 7 [6] occurred at disk power-on lifetime: 8994 hours (374 days + 18 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 39 60 f1 4a 00 00  Error: UNC at LBA = 0x3960f14a = 962654538

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 00 40 00 00 39 60 f1 22 40 00 20d+10:01:35.988  READ FPDMA QUEUED
  2f 00 00 00 01 00 00 00 00 00 10 00 00 20d+10:01:35.852  READ LOG EXT
  61 00 00 00 40 00 00 1c 81 e9 a2 40 00 20d+10:01:33.213  WRITE FPDMA QUEUED
  61 00 00 00 38 00 00 1c 83 84 22 40 00 20d+10:01:33.212  WRITE FPDMA QUEUED
  60 00 00 00 40 00 00 39 60 f1 22 40 00 20d+10:01:33.207  READ FPDMA QUEUED

Error 6 [5] occurred at disk power-on lifetime: 8994 hours (374 days + 18 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 39 60 f1 4a 00 00  Error: WP at LBA = 0x3960f14a = 962654538

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 00 00 00 40 00 00 1c 81 e9 a2 40 00 20d+10:01:33.213  WRITE FPDMA QUEUED
  61 00 00 00 38 00 00 1c 83 84 22 40 00 20d+10:01:33.212  WRITE FPDMA QUEUED
  60 00 00 00 40 00 00 39 60 f1 22 40 00 20d+10:01:33.207  READ FPDMA QUEUED
  2f 00 00 00 01 00 00 00 00 00 10 00 00 20d+10:01:33.054  READ LOG EXT
  61 00 00 00 40 00 00 1c 81 e9 a2 40 00 20d+10:01:30.360  WRITE FPDMA QUEUED

Error 5 [4] occurred at disk power-on lifetime: 8994 hours (374 days + 18 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 39 60 f1 4a 00 00  Error: WP at LBA = 0x3960f14a = 962654538

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 00 00 00 40 00 00 1c 81 e9 a2 40 00 20d+10:01:30.360  WRITE FPDMA QUEUED
  61 00 00 00 38 00 00 1c 83 84 22 40 00 20d+10:01:30.359  WRITE FPDMA QUEUED
  61 00 00 01 00 00 00 02 ba b8 62 40 00 20d+10:01:30.358  WRITE FPDMA QUEUED
  61 00 00 00 40 00 00 1c 81 e9 a2 40 00 20d+10:01:30.358  WRITE FPDMA QUEUED
  60 00 00 00 40 00 00 39 60 f1 22 40 00 20d+10:01:30.358  READ FPDMA QUEUED

Error 4 [3] occurred at disk power-on lifetime: 8994 hours (374 days + 18 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 39 60 f1 4a 00 00  Error: WP at LBA = 0x3960f14a = 962654538

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 00 00 00 40 00 00 1c 81 e9 a2 40 00 20d+10:01:27.416  WRITE FPDMA QUEUED
  61 00 00 00 38 00 00 1c 83 84 22 40 00 20d+10:01:27.415  WRITE FPDMA QUEUED
  61 00 00 00 40 00 00 1c 81 e9 a2 40 00 20d+10:01:27.414  WRITE FPDMA QUEUED
  61 00 00 00 40 00 00 1c 9f 60 22 40 00 20d+10:01:27.413  WRITE FPDMA QUEUED
  60 00 00 00 40 00 00 39 60 f1 22 40 00 20d+10:01:27.413  READ FPDMA QUEUED

Error 3 [2] occurred at disk power-on lifetime: 8994 hours (374 days + 18 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 39 60 f1 4a 00 00  Error: UNC at LBA = 0x3960f14a = 962654538

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 00 40 00 00 39 60 f1 22 40 00 20d+10:01:24.200  READ FPDMA QUEUED
  61 00 00 00 40 00 00 1c 81 e9 a2 40 00 20d+10:01:24.166  WRITE FPDMA QUEUED
  61 00 00 00 40 00 00 1c 9f 60 22 40 00 20d+10:01:24.166  WRITE FPDMA QUEUED
  61 00 00 00 40 00 00 1c 81 e9 a2 40 00 20d+10:01:24.165  WRITE FPDMA QUEUED
  60 00 00 00 40 00 00 38 40 c7 22 40 00 20d+10:01:24.165  READ FPDMA QUEUED

Error 2 [1] occurred at disk power-on lifetime: 55854 hours (2327 days + 6 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 38 f4 02 00 00 00  Error: WP at LBA = 0x38f40200 = 955515392

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 00 00 00 40 00 00 00 9c 89 22 40 00 44d+08:19:58.394  WRITE FPDMA QUEUED
  61 00 00 00 40 00 00 00 88 f8 22 40 00 44d+08:19:58.393  WRITE FPDMA QUEUED
  61 00 00 00 40 00 00 00 88 f7 e2 40 00 44d+08:19:58.393  WRITE FPDMA QUEUED
  61 00 00 00 40 00 00 00 61 da 22 40 00 44d+08:19:58.393  WRITE FPDMA QUEUED
  61 00 00 00 40 00 00 00 61 d9 e2 40 00 44d+08:19:58.393  WRITE FPDMA QUEUED

Error 1 [0] occurred at disk power-on lifetime: 55854 hours (2327 days + 6 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 00 00 00 00 38 f4 01 f9 00 00  Error: UNC at LBA = 0x38f401f9 = 955515385

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 00 01 00 00 00 01 b3 e8 22 40 00 44d+08:19:22.794  READ FPDMA QUEUED
  60 00 00 00 c0 00 00 01 b3 e2 22 40 00 44d+08:19:22.793  READ FPDMA QUEUED
  60 00 00 00 40 00 00 38 f4 16 a2 40 00 44d+08:19:22.782  READ FPDMA QUEUED
  60 00 00 00 40 00 00 38 f4 05 62 40 00 44d+08:19:22.775  READ FPDMA QUEUED
  60 00 00 01 00 00 00 38 f4 01 e2 40 00 44d+08:19:22.775  READ FPDMA QUEUED

SMART Extended Self-test Log Version: 1 (1 sectors)
Num  Test_Description    Status                  Remaining  LifeTime(hours)  LBA_of_first_error
# 1  Short offline       Completed without error       00%     15123         -

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Status Version:                  3
SCT Version (vendor specific):       522 (0x020a)
Device State:                        Active (0)
Current Temperature:                    22 Celsius
Power Cycle Min/Max Temperature:     20/43 Celsius
Lifetime    Min/Max Temperature:     13/43 Celsius
Under/Over Temperature Limit Count:   0/0

SCT Temperature History Version:     2
Temperature Sampling Period:         1 minute
Temperature Logging Interval:        59 minutes
Min/Max recommended Temperature:     14/55 Celsius
Min/Max Temperature Limit:           10/60 Celsius
Temperature History Size (Index):    128 (89)

SCT Error Recovery Control:
           Read: Disabled
          Write: Disabled

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11)
ID      Size     Value  Description
0x000a  2           21  Device-to-host register FISes sent due to a COMRESET
0x0001  2            0  Command failed due to ICRC error
0x0003  2            0  R_ERR response for device-to-host data FIS
0x0004  2            0  R_ERR response for host-to-device data FIS
0x0006  2            0  R_ERR response for device-to-host non-data FIS
0x0007  2            0  R_ERR response for host-to-device non-data FIS

