smartctl 7.1 2019-12-30 r5022 [FreeBSD 12.1-RELEASE-p10 amd64] (local build)
Copyright (C) 2002-19, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Seagate Barracuda 7200.7 and 7200.7 Plus
Device Model:     ST380013AS
Serial Number:    --
Firmware Version: 3.00
User Capacity:    80,026,361,856 bytes [80.0 GB]
Sector Size:      512 bytes logical/physical
Device is:        In smartctl database [for details use: -P show]
ATA Version is:   ATA/ATAPI-6 T13/1410D revision 2
Local Time is:    Tue Nov  3 18:39:23 2020 CET
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Unavailable
APM feature is:   Unavailable
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, NOT FROZEN [SEC1]
Wt Cache Reorder: Unavailable

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x82)	Offline data collection activity
					was completed without error.
					Auto Offline Data Collection: Enabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(  430) seconds.
Offline data collection
capabilities: 			 (0x5b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					No Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					No General Purpose Logging support.
Short self-test routine 
recommended polling time: 	 (   1) minutes.
Extended self-test routine
recommended polling time: 	 (  47) minutes.

SMART Attributes Data Structure revision number: 10
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     POSR--   048   045   006    -    71105768
  3 Spin_Up_Time            PO----   098   097   000    -    0
  4 Start_Stop_Count        -O--CK   091   091   020    -    9607
  5 Reallocated_Sector_Ct   PO--CK   100   100   036    -    0
  7 Seek_Error_Rate         POSR--   085   060   030    -    4690048745
  9 Power_On_Hours          -O--CK   072   072   000    -    24660
 10 Spin_Retry_Count        PO--C-   100   100   097    -    0
 12 Power_Cycle_Count       -O--CK   098   098   020    -    3070
194 Temperature_Celsius     -O---K   026   060   000    -    26 (0 7 0 0 0)
195 Hardware_ECC_Recovered  -O-RC-   048   045   000    -    71105768
197 Current_Pending_Sector  -O--C-   100   100   000    -    0
198 Offline_Uncorrectable   ----C-   100   100   000    -    0
199 UDMA_CRC_Error_Count    -OSRCK   200   001   000    -    2018
200 Multi_Zone_Error_Rate   ------   100   253   000    -    0
202 Data_Address_Mark_Errs  -O--CK   100   253   000    -    0
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory not supported

SMART Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00           SL  R/O      1  Log Directory
0x01           SL  R/O      1  Summary SMART error log
0x02           SL  R/O      5  Comprehensive SMART error log
0x03           SL  R/O      5  Ext. Comprehensive SMART error log
0x06           SL  R/O      1  SMART self-test log
0x07           SL  R/O      1  Extended self-test log
0x09           SL  R/W      1  Selective self-test log
0x20           SL  R/O      1  Streaming performance log [OBS-8]
0x21           SL  R/O      1  Write stream error log
0x22           SL  R/O      1  Read stream error log
0x23           SL  R/O      1  Delayed sector log [OBS-8]
0x80-0x9f      SL  R/W     16  Host vendor specific log
0xa0           SL  VS       1  Device vendor specific log
0xa1           SL  VS      20  Device vendor specific log
0xa2           SL  VS     101  Device vendor specific log
0xa8           SL  VS      20  Device vendor specific log
0xa9           SL  VS       1  Device vendor specific log
0xe0           SL  R/W      1  SCT Command/Status
0xe1           SL  R/W      1  SCT Data Transfer

SMART Extended Comprehensive Error Log (GP Log 0x03) not supported

SMART Error Log Version: 1
ATA Error Count: 10 (device log contains only the most recent five errors)
	CR = Command Register [HEX]
	FR = Features Register [HEX]
	SC = Sector Count Register [HEX]
	SN = Sector Number Register [HEX]
	CL = Cylinder Low Register [HEX]
	CH = Cylinder High Register [HEX]
	DH = Device/Head Register [HEX]
	DC = Device Command Register [HEX]
	ER = Error register [HEX]
	ST = Status register [HEX]
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 10 occurred at disk power-on lifetime: 24326 hours (1013 days + 14 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  40 51 19 61 fb 5f e0  Error: UNC 25 sectors at LBA = 0x005ffb61 = 6290273

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  c8 00 00 48 fb 5f e0 00      00:00:56.016  READ DMA
  c8 00 00 48 fa 5f e0 00      00:00:56.014  READ DMA
  c8 00 00 48 f9 5f e0 00      00:00:56.012  READ DMA
  c8 00 00 48 f8 5f e0 00      00:00:56.009  READ DMA
  c8 00 00 48 f7 5f e0 00      00:00:56.007  READ DMA

Error 9 occurred at disk power-on lifetime: 24326 hours (1013 days + 14 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  40 51 01 61 fb 5f e0  Error: UNC 1 sectors at LBA = 0x005ffb61 = 6290273

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  c8 00 08 60 fb 5f e0 00      00:00:40.045  READ DMA
  c8 00 08 60 fb 5f e0 00      00:00:36.228  READ DMA
  c8 00 08 60 fb 5f e0 00      00:00:32.419  READ DMA
  c8 00 08 60 fb 5f e0 00      00:00:27.858  READ DMA
  c8 00 08 20 f9 5f e0 00      00:00:27.857  READ DMA

Error 8 occurred at disk power-on lifetime: 24326 hours (1013 days + 14 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  40 51 01 61 fb 5f e0  Error: UNC 1 sectors at LBA = 0x005ffb61 = 6290273

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  c8 00 08 60 fb 5f e0 00      00:00:27.812  READ DMA
  c8 00 08 60 fb 5f e0 00      00:00:36.228  READ DMA
  c8 00 08 60 fb 5f e0 00      00:00:32.419  READ DMA
  c8 00 08 20 f9 5f e0 00      00:00:27.858  READ DMA
  c8 00 08 f0 ff 5f e0 00      00:00:27.857  READ DMA

Error 7 occurred at disk power-on lifetime: 24326 hours (1013 days + 14 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  40 51 01 61 fb 5f e0  Error: UNC 1 sectors at LBA = 0x005ffb61 = 6290273

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  c8 00 08 60 fb 5f e0 00      00:00:27.812  READ DMA
  c8 00 08 60 fb 5f e0 00      00:00:27.811  READ DMA
  c8 00 08 20 f9 5f e0 00      00:00:32.419  READ DMA
  c8 00 08 f0 ff 5f e0 00      00:00:27.858  READ DMA
  c8 00 08 78 9f 5c e0 00      00:00:27.857  READ DMA

Error 6 occurred at disk power-on lifetime: 24326 hours (1013 days + 14 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER ST SC SN CL CH DH
  -- -- -- -- -- -- --
  40 51 01 61 fb 5f e0  Error: UNC 1 sectors at LBA = 0x005ffb61 = 6290273

  Commands leading to the command that caused the error were:
  CR FR SC SN CL CH DH DC   Powered_Up_Time  Command/Feature_Name
  -- -- -- -- -- -- -- --  ----------------  --------------------
  c8 00 08 60 fb 5f e0 00      00:00:27.812  READ DMA
  c8 00 08 20 f9 5f e0 00      00:00:27.811  READ DMA
  c8 00 08 f0 ff 5f e0 00      00:00:27.811  READ DMA
  c8 00 08 78 9f 5c e0 00      00:00:27.858  READ DMA
  c8 00 08 d8 da d4 e8 00      00:00:27.857  READ DMA

SMART Extended Self-test Log (GP Log 0x07) not supported

SMART Self-test log structure revision number 1
Num  Test_Description    Status                  Remaining  LifeTime(hours)  LBA_of_first_error
# 1  Short offline       Completed without error       00%     22024         -
# 2  Short offline       Completed without error       00%     22023         -
# 3  Extended offline    Aborted by host               90%     22023         -
# 4  Extended offline    Completed without error       00%     21828         -
# 5  Short offline       Completed without error       00%     21276         -
# 6  Short offline       Completed without error       00%     20730         -
# 7  Short offline       Completed without error       00%     20300         -
# 8  Short offline       Completed without error       00%     19856         -
# 9  Short offline       Completed without error       00%     19322         -
#10  Short offline       Completed without error       00%     18592         -
#11  Short offline       Completed without error       00%     17861         -
#12  Short offline       Completed without error       00%     17401         -
#13  Short offline       Completed without error       00%     16890         -
#14  Short offline       Completed without error       00%     16160         -
#15  Short offline       Completed without error       00%     15429         -
#16  Short offline       Completed without error       00%     14698         -
#17  Short offline       Completed without error       00%     13967         -
#18  Short offline       Completed without error       00%     13259         -
#19  Short offline       Completed without error       00%     12528         -
#20  Short offline       Completed without error       00%     11797         -
#21  Short offline       Completed without error       00%     11066         -

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Commands not supported

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11) not supported



