smartctl 5.40 2010-10-16 r3189 [FreeBSD 7.4-RELEASE amd64] (local build)
Copyright (C) 2002-10 by Bruce Allen, http://smartmontools.sourceforge.net

=== START OF INFORMATION SECTION ===
Device Model:     OCZ-AGILITY3
Serial Number:    --
Firmware Version: 2.25
User Capacity:    120,034,123,776 bytes
Device is:        Not in smartctl database [for details use: -P showall]
ATA Version is:   8
ATA Standard is:  Not recognized. Minor revision code: 0x0110
Local Time is:    Thu May 14 20:23:07 2020 CET
SMART support is: Available - device has SMART capability.
SMART support is: Enabled

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x00)	Offline data collection activity
					was never started.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		 (   0) seconds.
Offline data collection
capabilities: 			 (0x7b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   1) minutes.
Extended self-test routine
recommended polling time: 	 (  48) minutes.
Conveyance self-test routine
recommended polling time: 	 (   2) minutes.
SCT capabilities: 	       (0x0021)	SCT Status supported.
					SCT Data Table supported.

SMART Attributes Data Structure revision number: 10
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAG     VALUE WORST THRESH TYPE      UPDATED  WHEN_FAILED RAW_VALUE
  1 Raw_Read_Error_Rate     0x000f   120   120   050    Pre-fail  Always       -       0
  5 Reallocated_Sector_Ct   0x0033   100   100   003    Pre-fail  Always       -       0
  9 Power_On_Hours          0x0032   042   042   000    Old_age   Always       -       210058260563646
 12 Power_Cycle_Count       0x0032   100   100   000    Old_age   Always       -       676
171 Unknown_Attribute       0x0032   000   000   000    Old_age   Always       -       0
172 Unknown_Attribute       0x0032   000   000   000    Old_age   Always       -       0
174 Unknown_Attribute       0x0030   000   000   000    Old_age   Offline      -       143
177 Wear_Leveling_Count     0x0000   000   000   000    Old_age   Offline      -       0
181 Program_Fail_Cnt_Total  0x0032   000   000   000    Old_age   Always       -       0
182 Erase_Fail_Count_Total  0x0032   000   000   000    Old_age   Always       -       0
187 Reported_Uncorrect      0x0032   100   100   000    Old_age   Always       -       0
194 Temperature_Celsius     0x0022   128   129   000    Old_age   Always       -       128 (Min/Max 127/129)
195 Hardware_ECC_Recovered  0x001c   100   100   000    Old_age   Offline      -       0
196 Reallocated_Event_Count 0x0033   100   100   003    Pre-fail  Always       -       0
201 Soft_Read_Error_Rate    0x001c   100   100   000    Old_age   Offline      -       0
204 Soft_ECC_Correction     0x001c   100   100   000    Old_age   Offline      -       0
230 Head_Amplitude          0x0013   100   100   000    Pre-fail  Always       -       100
231 Temperature_Celsius     0x0013   100   100   010    Pre-fail  Always       -       0
233 Media_Wearout_Indicator 0x0000   000   000   000    Old_age   Offline      -       987
234 Unknown_Attribute       0x0032   000   000   000    Old_age   Always       -       1249
241 Total_LBAs_Written      0x0032   000   000   000    Old_age   Always       -       1249
242 Total_LBAs_Read         0x0032   000   000   000    Old_age   Always       -       1383

General Purpose Logging (GPL) feature set supported
ATA_READ_LOG_EXT (addr=0x00:0x00, page=0, n=1) failed: 48-bit ATA commands not supported
Read GP Log Directory failed.

SMART Log Directory Version 1 [multi-sector log support]
SMART Log at address 0x00 has    1 sectors [Log Directory]
SMART Log at address 0x09 has    1 sectors [Selective self-test log]
SMART Log at address 0x11 has    1 sectors [SATA Phy Event Counters]
SMART Log at address 0x80 has   16 sectors [Host vendor specific log]
SMART Log at address 0x81 has   16 sectors [Host vendor specific log]
SMART Log at address 0x82 has   16 sectors [Host vendor specific log]
SMART Log at address 0x83 has   16 sectors [Host vendor specific log]
SMART Log at address 0x84 has   16 sectors [Host vendor specific log]
SMART Log at address 0x85 has   16 sectors [Host vendor specific log]
SMART Log at address 0x86 has   16 sectors [Host vendor specific log]
SMART Log at address 0x87 has   16 sectors [Host vendor specific log]
SMART Log at address 0x88 has   16 sectors [Host vendor specific log]
SMART Log at address 0x89 has   16 sectors [Host vendor specific log]
SMART Log at address 0x8a has   16 sectors [Host vendor specific log]
SMART Log at address 0x8b has   16 sectors [Host vendor specific log]
SMART Log at address 0x8c has   16 sectors [Host vendor specific log]
SMART Log at address 0x8d has   16 sectors [Host vendor specific log]
SMART Log at address 0x8e has   16 sectors [Host vendor specific log]
SMART Log at address 0x8f has   16 sectors [Host vendor specific log]
SMART Log at address 0x90 has   16 sectors [Host vendor specific log]
SMART Log at address 0x91 has   16 sectors [Host vendor specific log]
SMART Log at address 0x92 has   16 sectors [Host vendor specific log]
SMART Log at address 0x93 has   16 sectors [Host vendor specific log]
SMART Log at address 0x94 has   16 sectors [Host vendor specific log]
SMART Log at address 0x95 has   16 sectors [Host vendor specific log]
SMART Log at address 0x96 has   16 sectors [Host vendor specific log]
SMART Log at address 0x97 has   16 sectors [Host vendor specific log]
SMART Log at address 0x98 has   16 sectors [Host vendor specific log]
SMART Log at address 0x99 has   16 sectors [Host vendor specific log]
SMART Log at address 0x9a has   16 sectors [Host vendor specific log]
SMART Log at address 0x9b has   16 sectors [Host vendor specific log]
SMART Log at address 0x9c has   16 sectors [Host vendor specific log]
SMART Log at address 0x9d has   16 sectors [Host vendor specific log]
SMART Log at address 0x9e has   16 sectors [Host vendor specific log]
SMART Log at address 0x9f has   16 sectors [Host vendor specific log]
SMART Log at address 0xb7 has   16 sectors [Device vendor specific log]
SMART Log at address 0xe0 has    1 sectors [SCT Command/Status]
SMART Log at address 0xe1 has    1 sectors [SCT Data Transfer]

SMART Extended Comprehensive Error Log (GP Log 0x03) not supported
SMART Error Log Version: 0
No Errors Logged

SMART Extended Self-test Log (GP Log 0x07) not supported
SMART Self-test log structure revision number 0
Warning: ATA Specification requires self-test log structure revision number = 1
No self-tests have been logged.  [To run self-tests, use: smartctl -t]


SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

Error unknown SCT Temperature History Format Version (10), should be 2.
Warning: device does not support SCT Error Recovery Control command
SATA Phy Event Counters (GP Log 0x11) not supported

