smartctl 7.1 2019-12-30 r5022 [FreeBSD 12.1-RELEASE-p2 amd64] (local build)
Copyright (C) 2002-19, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     SAMSUNG SpinPoint T166
Device Model:     SAMSUNG HD501LJ
Serial Number:    --
LU WWN Device Id: 5 0000f0 ...
Firmware Version: CR100-12
User Capacity:    500,107,862,016 bytes [500 GB]
Sector Size:      512 bytes logical/physical
Device is:        In smartctl database [for details use: -P show]
ATA Version is:   ATA8-ACS T13/1699-D revision 3b
SATA Version is:  SATA 2.5, 3.0 Gb/s
Local Time is:    Mon May 25 14:01:49 2020 MSK
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM level is:     254 (maximum performance), recommended: 254
APM feature is:   Unavailable
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, frozen [SEC2]
Wt Cache Reorder: Enabled

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x00)	Offline data collection activity
					was never started.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		( 9033) seconds.
Offline data collection
capabilities: 			 (0x5b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					No Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   2) minutes.
Extended self-test routine
recommended polling time: 	 ( 154) minutes.
SCT capabilities: 	       (0x003f)	SCT Status supported.
					SCT Error Recovery Control supported.
					SCT Feature Control supported.
					SCT Data Table supported.

SMART Attributes Data Structure revision number: 16
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     POSR--   100   100   051    -    1
  3 Spin_Up_Time            POS---   100   100   015    -    7360
  4 Start_Stop_Count        -O--CK   100   100   000    -    787
  5 Reallocated_Sector_Ct   PO--CK   253   253   010    -    0
  7 Seek_Error_Rate         POSR--   253   253   051    -    0
  8 Seek_Time_Performance   P-S--K   253   253   015    -    0
  9 Power_On_Hours          -O--CK   100   100   000    -    90221
 10 Spin_Retry_Count        PO--CK   253   253   051    -    0
 11 Calibration_Retry_Count -O--C-   253   253   000    -    0
 12 Power_Cycle_Count       -O--CK   100   100   000    -    586
 13 Read_Soft_Error_Rate    -OSR--   100   100   000    -    253323093
187 Reported_Uncorrect      -O--CK   253   253   000    -    0
188 Command_Timeout         -O--CK   100   100   000    -    2
190 Airflow_Temperature_Cel -O---K   067   051   000    -    33
194 Temperature_Celsius     -O---K   139   091   000    -    33
195 Hardware_ECC_Recovered  -O-RC-   100   100   000    -    253323093
196 Reallocated_Event_Count -O--CK   253   253   000    -    0
197 Total_Pending_Sectors   -O--C-   253   100   000    -    0
198 Offline_Uncorrectable   ----CK   253   253   000    -    0
199 UDMA_CRC_Error_Count    -OSRCK   200   200   000    -    0
200 Multi_Zone_Error_Rate   -O-R--   100   100   000    -    0
201 Soft_Read_Error_Rate    -O-R--   100   100   000    -    0
202 Data_Address_Mark_Errs  -O--CK   253   253   000    -    0
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory Version 1
SMART           Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00       GPL,SL  R/O      1  Log Directory
0x01           SL  R/O      1  Summary SMART error log
0x02           SL  R/O      2  Comprehensive SMART error log
0x03       GPL     R/O      2  Ext. Comprehensive SMART error log
0x06           SL  R/O      1  SMART self-test log
0x09       GPL,SL  R/W      1  Selective self-test log
0x10       GPL     R/O      1  NCQ Command Error log
0x11       GPL     R/O      1  SATA Phy Event Counters log
0x80-0x9f  GPL,SL  R/W     16  Host vendor specific log
0xe0       GPL,SL  R/W      1  SCT Command/Status
0xe1       GPL,SL  R/W      1  SCT Data Transfer

SMART Extended Comprehensive Error Log Version: 1 (2 sectors)
Invalid Error Log index = 0x0000, trying reserved byte (0x08) instead
Device Error Count: 56 (device log contains only the most recent 8 errors)
	CR     = Command Register
	FEATR  = Features Register
	COUNT  = Count (was: Sector Count) Register
	LBA_48 = Upper bytes of LBA High/Mid/Low Registers ]  ATA-8
	LH     = LBA High (was: Cylinder High) Register    ]   LBA
	LM     = LBA Mid (was: Cylinder Low) Register      ] Register
	LL     = LBA Low (was: Sector Number) Register     ]
	DV     = Device (was: Device/Head) Register
	DC     = Device Control Register
	ER     = Error register
	ST     = Status register
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 56 [7] occurred at disk power-on lifetime: 30381 hours (1265 days + 21 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 0a 58 00 00 27 ea ed 19 40 00  Error: WP at LBA = 0x27eaed19 = 669707545

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 01 02 0a 58 00 00 27 ea ed 19 40 00  1d+06:25:56.688  WRITE FPDMA QUEUED
  2f 01 00 00 01 00 00 00 00 00 10 40 00  1d+06:25:51.813  READ LOG EXT

Error 55 [6] occurred at disk power-on lifetime: 30381 hours (1265 days + 21 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 06 38 00 00 27 ea ed 19 40 00  Error: WP at LBA = 0x27eaed19 = 669707545

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 01 02 06 38 00 00 27 ea ed 19 40 00  1d+06:25:51.688  WRITE FPDMA QUEUED
  2f 01 00 00 01 00 00 00 00 00 10 40 00  1d+06:25:46.563  READ LOG EXT

Error 54 [5] occurred at disk power-on lifetime: 30381 hours (1265 days + 21 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 02 18 00 00 27 ea ed 19 40 00  Error: WP at LBA = 0x27eaed19 = 669707545

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 01 02 02 18 00 00 27 ea ed 19 40 00  1d+06:25:46.438  WRITE FPDMA QUEUED
  2f 01 00 00 01 00 00 00 00 00 10 40 00  1d+06:25:40.563  READ LOG EXT

Error 53 [4] occurred at disk power-on lifetime: 30381 hours (1265 days + 21 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 1e f8 00 00 27 ea ed 19 40 00  Error: WP at LBA = 0x27eaed19 = 669707545

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 01 02 1e f8 00 00 27 ea ed 19 40 00  1d+06:25:40.438  WRITE FPDMA QUEUED
  2f 01 00 00 01 00 00 00 00 00 10 40 00  1d+06:25:34.313  READ LOG EXT

Error 52 [3] occurred at disk power-on lifetime: 30381 hours (1265 days + 21 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 17 b8 00 00 33 d1 6f b9 40 00  Error: UNC at LBA = 0x33d16fb9 = 869363641

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 01 17 b8 00 00 33 d1 6f b9 40 00  1d+06:25:34.188  READ FPDMA QUEUED
  ea 02 00 00 00 00 00 00 00 00 00 40 00  1d+06:25:29.438  FLUSH CACHE EXT
  61 02 02 16 b8 00 00 3a 38 5e c6 40 00  1d+06:25:29.438  WRITE FPDMA QUEUED
  61 02 02 16 b8 00 00 3a 38 5e c6 40 00  1d+06:25:29.438  WRITE FPDMA QUEUED
  61 02 02 15 b0 00 00 3a 38 5c c6 40 00  1d+06:25:29.438  WRITE FPDMA QUEUED

Error 51 [2] occurred at disk power-on lifetime: 30381 hours (1265 days + 21 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 16 b8 00 00 0a 81 07 80 40 00  Error: WP at LBA = 0x0a810780 = 176228224

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 01 08 16 b8 00 00 0a 81 07 80 40 00  1d+06:24:38.875  WRITE FPDMA QUEUED
  ec d5 00 00 01 00 00 00 00 00 00 40 00  1d+06:24:33.125  IDENTIFY DEVICE
  b0 00 d5 00 01 00 00 00 c2 4f 01 40 00  1d+06:24:33.000  SMART READ LOG
  2f 01 00 00 01 00 00 00 00 00 10 40 00  1d+06:24:33.000  READ LOG EXT

Error 50 [1] occurred at disk power-on lifetime: 30381 hours (1265 days + 21 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 15 b0 00 00 0a 81 07 80 40 00  Error: WP at LBA = 0x0a810780 = 176228224

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 01 08 15 b0 00 00 0a 81 07 80 40 00  1d+06:24:32.875  WRITE FPDMA QUEUED
  b0 00 d5 00 01 00 00 00 c2 4f 06 40 00  1d+06:24:28.063  SMART READ LOG
  2f 01 00 00 01 00 00 00 00 00 10 40 00  1d+06:24:28.000  READ LOG EXT

Error 49 [0] occurred at disk power-on lifetime: 30381 hours (1265 days + 21 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  40 -- 51 14 a8 00 00 0a 81 07 80 40 00  Error: WP at LBA = 0x0a810780 = 176228224

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  61 01 08 14 a8 00 00 0a 81 07 80 40 00  1d+06:24:27.875  WRITE FPDMA QUEUED
  b0 00 d0 00 01 00 00 00 c2 4f 00 40 00  1d+06:24:20.688  SMART READ DATA
  2f 01 00 00 01 00 00 00 00 00 10 40 00  1d+06:24:20.625  READ LOG EXT

SMART Extended Self-test Log (GP Log 0x07) not supported

SMART Self-test log structure revision number 1
Num  Test_Description    Status                  Remaining  LifeTime(hours)  LBA_of_first_error
# 1  Extended offline    Completed without error       00%     19174         -
# 2  Extended offline    Completed without error       00%      8405         -

SMART Selective self-test log data structure revision number 0
Note: revision number not 1 implies that no selective self-test has ever been run
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Status Version:                  2
SCT Version (vendor specific):       256 (0x0100)
Device State:                        Active (0)
Current Temperature:                    33 Celsius
Power Cycle Min/Max Temperature:     28/38 Celsius
Lifetime    Min/Max Temperature:     12/49 Celsius
Under/Over Temperature Limit Count:   0/0

SCT Temperature History Version:     2
Temperature Sampling Period:         1 minute
Temperature Logging Interval:        1 minute
Min/Max recommended Temperature:     -4/72 Celsius
Min/Max Temperature Limit:           -9/77 Celsius
Temperature History Size (Index):    128 (26)

SCT Error Recovery Control:
           Read: Disabled
          Write: Disabled

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11)
ID      Size     Value  Description
0x0001  2            0  Command failed due to ICRC error
0x0002  2            0  R_ERR response for data FIS
0x0003  2            0  R_ERR response for device-to-host data FIS
0x0004  2            0  R_ERR response for host-to-device data FIS
0x0005  2            0  R_ERR response for non-data FIS
0x0006  2            0  R_ERR response for device-to-host non-data FIS
0x0007  2            0  R_ERR response for host-to-device non-data FIS
0x0008  2            0  Device-to-host non-data FIS retries
0x0009  2            2  Transition from drive PhyRdy to drive PhyNRdy
0x000a  2           66  Device-to-host register FISes sent due to a COMRESET
0x000b  2            0  CRC errors within host-to-device FIS
0x000d  2            0  Non-CRC errors within host-to-device FIS
0x000f  2            0  R_ERR response for host-to-device data FIS, CRC
0x0010  2            0  R_ERR response for host-to-device data FIS, non-CRC
0x0012  2            0  R_ERR response for host-to-device non-data FIS, CRC
0x0013  2            0  R_ERR response for host-to-device non-data FIS, non-CRC
0x8001  2            0  Vendor specific



