smartctl 7.2 2020-12-30 r5155 [FreeBSD 13.0-RELEASE-p13 amd64] (local build)
Copyright (C) 2002-20, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Device Model:     Smartbuy SSD 256GB
Serial Number:    --
LU WWN Device Id: 5 000000 ...
Firmware Version: H190117D
User Capacity:    256,060,514,304 bytes [256 GB]
Sector Size:      512 bytes logical/physical
Rotation Rate:    Solid State Device
Form Factor:      2.5 inches
TRIM Command:     Available, deterministic, zeroed
Device is:        Not in smartctl database [for details use: -P showall]
ATA Version is:   ACS-2 (minor revision not indicated)
SATA Version is:  SATA 3.2, 6.0 Gb/s (current: 3.0 Gb/s)
Local Time is:    Mon Oct 10 15:32:56 2022 EDT
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Unavailable
APM feature is:   Unavailable
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, frozen [SEC2]
Wt Cache Reorder: Enabled

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x00)	Offline data collection activity
					was never started.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(   33) seconds.
Offline data collection
capabilities: 			 (0x7b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   2) minutes.
Extended self-test routine
recommended polling time: 	 (   2) minutes.
Conveyance self-test routine
recommended polling time: 	 (   2) minutes.
SCT capabilities: 	       (0x0031)	SCT Status supported.
					SCT Feature Control supported.
					SCT Data Table supported.

SMART Attributes Data Structure revision number: 16
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  5 Reallocated_Sector_Ct   PO--C-   100   100   050    -    0
  9 Power_On_Hours          -O--C-   100   100   000    -    5386
 12 Power_Cycle_Count       -O--C-   100   100   000    -    1426
167 Unknown_Attribute       -O---K   100   100   000    -    0
168 Unknown_Attribute       -O--C-   100   100   000    -    148
169 Unknown_Attribute       PO--C-   093   093   010    -    15204381
171 Unknown_Attribute       -O--CK   000   000   000    -    0
172 Unknown_Attribute       -O--CK   000   000   000    -    0
173 Unknown_Attribute       -O--C-   200   200   000    -    700093431988
175 Program_Fail_Count_Chip -O---K   100   100   010    -    0
177 Wear_Leveling_Count     -O--C-   100   100   000    -    0
180 Unused_Rsvd_Blk_Cnt_Tot PO--CK   100   100   000    -    3168
187 Reported_Uncorrect      -O--CK   100   000   000    -    0
192 Power-Off_Retract_Count -O--C-   100   100   000    -    499
194 Temperature_Celsius     -O---K   048   048   000    -    48 (Min/Max 48/48)
199 UDMA_CRC_Error_Count    -O--C-   100   100   000    -    0
206 Unknown_SSD_Attribute   -O--CK   200   200   000    -    163
207 Unknown_SSD_Attribute   -O--CK   200   200   000    -    210
208 Unknown_SSD_Attribute   -O--CK   200   200   000    -    180
209 Unknown_SSD_Attribute   -O--CK   200   200   000    -    526
210 Unknown_Attribute       -O--CK   200   200   000    -    1198
211 Unknown_Attribute       -O--CK   200   200   000    -    943
231 Unknown_SSD_Attribute   PO---K   088   088   005    -    12
241 Total_LBAs_Written      -O--CK   100   100   000    -    31545
242 Total_LBAs_Read         -O--CK   100   100   000    -    10182
245 Unknown_Attribute       -O--CK   100   100   000    -    0
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory Version 1
SMART           Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00       GPL,SL  R/O      1  Log Directory
0x01           SL  R/O      1  Summary SMART error log
0x02           SL  R/O     51  Comprehensive SMART error log
0x03       GPL     R/O     64  Ext. Comprehensive SMART error log
0x04       GPL,SL  R/O      8  Device Statistics log
0x06           SL  R/O      1  SMART self-test log
0x07       GPL     R/O      1  Extended self-test log
0x09           SL  R/W      1  Selective self-test log
0x10       GPL     R/O      1  NCQ Command Error log
0x11       GPL     R/O      1  SATA Phy Event Counters log
0x30       GPL,SL  R/O      9  IDENTIFY DEVICE data log
0x80-0x9f  GPL,SL  R/W     16  Host vendor specific log
0xe0       GPL,SL  R/W      1  SCT Command/Status
0xe1       GPL,SL  R/W      1  SCT Data Transfer

SMART Extended Comprehensive Error Log Version: 1 (64 sectors)
Device Error Count: 148
	CR     = Command Register
	FEATR  = Features Register
	COUNT  = Count (was: Sector Count) Register
	LBA_48 = Upper bytes of LBA High/Mid/Low Registers ]  ATA-8
	LH     = LBA High (was: Cylinder High) Register    ]   LBA
	LM     = LBA Mid (was: Cylinder Low) Register      ] Register
	LL     = LBA Low (was: Sector Number) Register     ]
	DV     = Device (was: Device/Head) Register
	DC     = Device Control Register
	ER     = Error register
	ST     = Status register
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 148 [147] occurred at disk power-on lifetime: 5097 hours (212 days + 9 hours)
  When the command that caused the error occurred, the device was in an unknown state.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  10 -- 51 67 01 00 00 02 00 00 00 a0 08

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  70 00 ff 00 00 00 00 00 00 00 00 a0 80     00:01:31.300  SEEK [OBS-7]
  25 03 da 00 67 00 00 00 00 00 02 40 80     00:01:31.300  READ DMA EXT
  25 03 da 00 01 00 00 00 00 00 01 40 80     00:01:31.300  READ DMA EXT
  25 03 da 00 01 00 00 00 00 00 00 40 80     00:01:31.300  READ DMA EXT
  f5 00 da 00 01 00 00 00 c2 4f f0 a0 80     00:01:31.000  SECURITY FREEZE LOCK

Error 147 [146] occurred at disk power-on lifetime: 5097 hours (212 days + 9 hours)
  When the command that caused the error occurred, the device was in an unknown state.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  10 -- 51 67 01 00 00 02 00 00 00 a0 08

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  70 00 ff 00 00 00 00 00 00 00 00 a0 80     00:00:39.400  SEEK [OBS-7]
  25 03 da 00 67 00 00 00 00 00 02 40 80     00:00:39.400  READ DMA EXT
  25 03 da 00 01 00 00 00 00 00 01 40 80     00:00:39.400  READ DMA EXT
  25 03 da 00 01 00 00 00 00 00 00 40 80     00:00:39.400  READ DMA EXT
  f5 00 da 00 01 00 00 00 c2 4f f0 a0 80     00:00:39.100  SECURITY FREEZE LOCK

Error 146 [145] occurred at disk power-on lifetime: 5097 hours (212 days + 9 hours)
  When the command that caused the error occurred, the device was in an unknown state.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  10 -- 51 67 01 00 00 02 00 00 00 a0 08

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  70 00 ff 00 00 00 00 00 00 00 00 a0 80     00:00:04.100  SEEK [OBS-7]
  25 03 da 00 67 00 00 00 00 00 02 40 80     00:00:04.100  READ DMA EXT
  25 03 da 00 01 00 00 00 00 00 01 40 80     00:00:04.100  READ DMA EXT
  25 03 da 00 01 00 00 00 00 00 00 40 80     00:00:04.100  READ DMA EXT
  f5 00 da 00 01 00 00 00 c2 4f f0 a0 80     00:00:03.800  SECURITY FREEZE LOCK

Error 145 [144] occurred at disk power-on lifetime: 5097 hours (212 days + 9 hours)
  When the command that caused the error occurred, the device was in an unknown state.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  10 -- 51 67 01 00 00 02 00 00 00 a0 08

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  70 00 ff 00 00 00 00 00 00 00 00 a0 80     00:00:17.100  SEEK [OBS-7]
  25 03 da 00 67 00 00 00 00 00 02 40 80     00:00:17.100  READ DMA EXT
  25 03 da 00 01 00 00 00 00 00 01 40 80     00:00:17.100  READ DMA EXT
  25 03 da 00 01 00 00 00 00 00 00 40 80     00:00:17.100  READ DMA EXT
  f5 00 da 00 01 00 00 00 c2 4f f0 a0 80     00:00:16.900  SECURITY FREEZE LOCK

Error 144 [143] occurred at disk power-on lifetime: 5097 hours (212 days + 9 hours)
  When the command that caused the error occurred, the device was in an unknown state.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  10 -- 51 67 01 00 00 02 00 00 00 a0 08

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  70 00 ff 00 00 00 00 00 00 00 00 a0 80     00:00:09.500  SEEK [OBS-7]
  25 03 da 00 67 00 00 00 00 00 02 40 80     00:00:09.500  READ DMA EXT
  25 03 da 00 01 00 00 00 00 00 01 40 80     00:00:09.500  READ DMA EXT
  25 03 da 00 01 00 00 00 00 00 00 40 80     00:00:09.500  READ DMA EXT
  f5 00 da 00 01 00 00 00 c2 4f f0 a0 80     00:00:09.300  SECURITY FREEZE LOCK

Error 143 [142] occurred at disk power-on lifetime: 5097 hours (212 days + 9 hours)
  When the command that caused the error occurred, the device was in an unknown state.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  10 -- 51 67 01 00 00 02 00 00 00 a0 08

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  70 00 ff 00 00 00 00 00 00 00 00 a0 80     00:02:25.800  SEEK [OBS-7]
  25 03 da 00 67 00 00 00 00 00 02 40 80     00:02:25.800  READ DMA EXT
  25 03 da 00 01 00 00 00 00 00 01 40 80     00:02:25.800  READ DMA EXT
  25 03 da 00 01 00 00 00 00 00 00 40 80     00:02:25.800  READ DMA EXT
  f5 00 da 00 01 00 00 00 c2 4f f0 a0 80     00:02:25.500  SECURITY FREEZE LOCK

Error 142 [141] occurred at disk power-on lifetime: 5097 hours (212 days + 9 hours)
  When the command that caused the error occurred, the device was in an unknown state.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  10 -- 51 67 01 00 00 02 00 00 00 a0 08

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  70 00 ff 00 00 00 00 00 00 00 00 a0 80     00:02:07.500  SEEK [OBS-7]
  25 03 da 00 67 00 00 00 00 00 02 40 80     00:02:07.500  READ DMA EXT
  25 03 da 00 01 00 00 00 00 00 01 40 80     00:02:07.500  READ DMA EXT
  25 03 da 00 01 00 00 00 00 00 00 40 80     00:02:07.500  READ DMA EXT
  f5 00 da 00 01 00 00 00 c2 4f f0 a0 80     00:02:07.200  SECURITY FREEZE LOCK

Error 141 [140] occurred at disk power-on lifetime: 5097 hours (212 days + 9 hours)
  When the command that caused the error occurred, the device was in an unknown state.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  10 -- 51 67 01 00 00 02 00 00 00 a0 08

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  70 00 ff 00 00 00 00 00 00 00 00 a0 80     00:00:04.800  SEEK [OBS-7]
  25 03 da 00 67 00 00 00 00 00 02 40 80     00:00:04.800  READ DMA EXT
  25 03 da 00 01 00 00 00 00 00 01 40 80     00:00:04.800  READ DMA EXT
  25 03 da 00 01 00 00 00 00 00 00 40 80     00:00:04.800  READ DMA EXT
  f5 00 da 00 01 00 00 00 c2 4f f0 a0 80     00:00:04.500  SECURITY FREEZE LOCK

SMART Extended Self-test Log Version: 1 (1 sectors)
Num  Test_Description    Status                  Remaining  LifeTime(hours)  LBA_of_first_error
# 1  Short offline       Completed without error       00%      3448         -
# 2  Short offline       Completed without error       00%      3430         -
# 3  Short offline       Completed without error       00%      3423         -
# 4  Short offline       Completed without error       00%      3414         -
# 5  Short offline       Completed without error       00%      2662         -
# 6  Extended offline    Completed without error       00%      1962         -

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Status Version:                  3
SCT Version (vendor specific):       1 (0x0001)
Device State:                        Active (0)
Current Temperature:                    48 Celsius
Power Cycle Min/Max Temperature:      ?/48 Celsius
Lifetime    Min/Max Temperature:      ?/ ? Celsius
Under/Over Temperature Limit Count:   0/0

SCT Temperature History Version:     2
Temperature Sampling Period:         1 minute
Temperature Logging Interval:        1 minute
Min/Max recommended Temperature:     -127/127 Celsius
Min/Max Temperature Limit:           -127/127 Celsius
Temperature History Size (Index):    478 (237)

SCT Error Recovery Control command not supported

Device Statistics (GP Log 0x04)
Page  Offset Size        Value Flags Description
0x01  =====  =               =  ===  == General Statistics (rev 1) ==
0x01  0x008  4            1426  ---  Lifetime Power-On Resets
0x01  0x010  4            5386  ---  Power-on Hours
0x01  0x018  6     66156024936  ---  Logical Sectors Written
0x01  0x020  6       178691956  ---  Number of Write Commands
0x01  0x028  6     21353520428  ---  Logical Sectors Read
0x01  0x030  6       121423124  ---  Number of Read Commands
0x01  0x038  6   4962898895796  ---  Date and Time TimeStamp
0x07  =====  =               =  ===  == Solid State Device Statistics (rev 1) ==
0x07  0x008  1              28  N--  Percentage Used Endurance Indicator
                                |||_ C monitored condition met
                                ||__ D supports DSN
                                |___ N normalized value

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11)
ID      Size     Value  Description
0x0001  2          148  Command failed due to ICRC error
0x0003  2            0  R_ERR response for device-to-host data FIS
0x0004  2            0  R_ERR response for host-to-device data FIS
0x0006  2            0  R_ERR response for device-to-host non-data FIS
0x0007  2            0  R_ERR response for host-to-device non-data FIS
0x0008  2            0  Device-to-host non-data FIS retries
0x0009  4            0  Transition from drive PhyRdy to drive PhyNRdy
0x000a  4           28  Device-to-host register FISes sent due to a COMRESET
0x000f  2            0  R_ERR response for host-to-device data FIS, CRC
0x0010  2            0  R_ERR response for host-to-device data FIS, non-CRC
0x0012  2            0  R_ERR response for host-to-device non-data FIS, CRC
0x0013  2            0  R_ERR response for host-to-device non-data FIS, non-CRC



