smartctl 7.3 2022-02-28 r5338 [FreeBSD 13.1-RELEASE-p5 amd64] (local build)
Copyright (C) 2002-22, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Innodisk 1IE3/3IE3/3ME3/3IE4/3ME4 SSDs
Device Model:     SATADOM-SH 3ME4
Serial Number:    --
LU WWN Device Id: 5 02b2a2 ...
Firmware Version: L17606
User Capacity:    16,013,942,784 bytes [16.0 GB]
Sector Size:      512 bytes logical/physical
Rotation Rate:    Solid State Device
TRIM Command:     Available, deterministic, zeroed
Device is:        In smartctl database 7.3/5319
ATA Version is:   ACS-3 T13/2161-D revision 4
SATA Version is:  SATA 3.2, 6.0 Gb/s (current: 6.0 Gb/s)
Local Time is:    Thu Jan 26 21:35:02 2023 CET
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Unavailable
APM feature is:   Unavailable
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, frozen [SEC2]
Wt Cache Reorder: Unavailable

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x02)	Offline data collection activity
					was completed without error.
					Auto Offline Data Collection: Disabled.
Total time to complete Offline 
data collection: 		(   32) seconds.
Offline data collection
capabilities: 			 (0x00) 	Offline data collection not supported.
SMART capabilities:            (0x0002)	Does not save SMART data before
					entering power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x00)	Error logging NOT supported.
					General Purpose Logging supported.

SMART Attributes Data Structure revision number: 16
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     ------   000   000   000    -    0
  2 Throughput_Performance  ------   000   000   000    -    0
  5 Later_Bad_Block         -O--C-   100   100   001    -    0
  7 Seek_Error_Rate         ------   000   000   000    -    0
  8 Seek_Time_Performance   ------   000   000   000    -    0
  9 Power_On_Hours          -O--C-   003   000   000    -    761
 10 Spin_Retry_Count        ------   000   000   000    -    0
 12 Power_Cycle_Count       -O--C-   172   000   000    -    172
163 Total_Bad_Block_Count   ------   000   000   000    -    21
168 SATA_PHY_Error_Count    ------   000   000   000    -    0
169 Remaining_Lifetime_Perc ------   100   000   000    -    100
175 Bad_Cluster_Table_Count ------   000   000   000    -    0
192 Power-Off_Retract_Count -O--C-   000   000   000    -    131
194 Temperature_Celsius     -O----   055   100   000    -    55 (3 56 0 45 0)
197 Current_Pending_Sector  ------   000   000   000    -    0
225 Data_Log_Write_Count    ------   000   000   000    -    0
240 Write_Head              ------   000   000   000    -    0
165 Max_Erase_Count         -O--C-   006   100   000    -    6
167 Average_Erase_Count     -O--C-   000   100   000    -    3
170 Spare_Block_Count       PO--C-   100   100   010    -    131
171 Program_Fail_Count      -O--C-   000   100   000    -    0
172 Erase_Fail_Count        -O--C-   000   100   000    -    0
176 RANGE_RECORD_Count      ------   000   000   000    -    0
184 End-to-End_Error        -O--C-   000   000   000    -    0
187 Reported_Uncorrect      -O--C-   000   000   000    -    0
229 Flash_ID                ------   100   100   000    -    0x517693943a98
232 Spares_Remaining_Perc   PO--C-   000   000   000    -    0
235 Later_Bad_Blk_Inf_R/W/E -O----   000   000   000    -    0 0 0
241 Host_Writes_32MiB       -O----   100   100   000    -    1645
242 Host_Reads_32MiB        -O----   100   100   000    -    49352
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory Version 1
SMART           Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00       GPL,SL  R/O      1  Log Directory
0x07       GPL,SL  R/O      1  Extended self-test log
0x09       GPL,SL  R/W      1  Selective self-test log
0x10       GPL,SL  R/O      1  NCQ Command Error log
0x30       GPL,SL  R/O      9  IDENTIFY DEVICE data log
0x80-0x9f  GPL,SL  R/W     16  Host vendor specific log
0xdf       GPL,SL  VS       1  Device vendor specific log

SMART Extended Comprehensive Error Log (GP Log 0x03) not supported

SMART Error Log not supported

SMART Extended Self-test Log Version: 1 (1 sectors)
No self-tests have been logged.  [To run self-tests, use: smartctl -t]

Selective Self-tests/Logging not supported

SCT Commands not supported

Device Statistics (GP/SMART Log 0x04) not supported

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11) not supported



