smartctl 7.1 2019-12-30 r5022 [FreeBSD 12.1-RELEASE amd64] (local build)
Copyright (C) 2002-19, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Model Family:     Toshiba HG6 Series SSD
Device Model:     TOSHIBA THNSNJ128GCSU
Serial Number:    --
LU WWN Device Id: 5 00080d ...
Firmware Version: JURA0101
User Capacity:    128,035,676,160 bytes [128 GB]
Sector Size:      512 bytes logical/physical
Rotation Rate:    Solid State Device
Form Factor:      2.5 inches
Device is:        In smartctl database [for details use: -P show]
ATA Version is:   ACS-2 (minor revision not indicated)
SATA Version is:  SATA 3.1, 6.0 Gb/s (current: 6.0 Gb/s)
Local Time is:    Fri Feb 12 23:01:32 2021 EST
SMART support is: Available - device has SMART capability.
SMART support is: Enabled
AAM feature is:   Unavailable
APM level is:     254 (maximum performance)
Rd look-ahead is: Enabled
Write cache is:   Enabled
DSN feature is:   Unavailable
ATA Security is:  Disabled, frozen [SEC2]
Wt Cache Reorder: Enabled

=== START OF READ SMART DATA SECTION ===
SMART overall-health self-assessment test result: PASSED

General SMART Values:
Offline data collection status:  (0x00)	Offline data collection activity
					was never started.
					Auto Offline Data Collection: Disabled.
Self-test execution status:      (   0)	The previous self-test routine completed
					without error or no self-test has ever 
					been run.
Total time to complete Offline 
data collection: 		(  120) seconds.
Offline data collection
capabilities: 			 (0x5b) SMART execute Offline immediate.
					Auto Offline data collection on/off support.
					Suspend Offline collection upon new
					command.
					Offline surface scan supported.
					Self-test supported.
					No Conveyance Self-test supported.
					Selective Self-test supported.
SMART capabilities:            (0x0003)	Saves SMART data before entering
					power-saving mode.
					Supports SMART auto save timer.
Error logging capability:        (0x01)	Error logging supported.
					General Purpose Logging supported.
Short self-test routine 
recommended polling time: 	 (   2) minutes.
Extended self-test routine
recommended polling time: 	 (   5) minutes.
SCT capabilities: 	       (0x003d)	SCT Status supported.
					SCT Error Recovery Control supported.
					SCT Feature Control supported.
					SCT Data Table supported.

SMART Attributes Data Structure revision number: 16
Vendor Specific SMART Attributes with Thresholds:
ID# ATTRIBUTE_NAME          FLAGS    VALUE WORST THRESH FAIL RAW_VALUE
  1 Raw_Read_Error_Rate     -O-R--   100   100   000    -    0
  2 Throughput_Performance  P-S---   100   100   050    -    0
  3 Spin_Up_Time            POS---   100   100   050    -    0
  5 Reallocated_Sector_Ct   PO--C-   100   100   050    -    0
  7 Unknown_SSD_Attribute   PO-R--   100   100   050    -    0
  8 Unknown_SSD_Attribute   P-S---   100   100   050    -    0
  9 Power_On_Hours          -O--C-   100   100   000    -    4270
 10 Unknown_SSD_Attribute   PO--C-   100   100   050    -    0
 12 Power_Cycle_Count       -O--C-   100   100   000    -    2441
167 SSD_Protect_Mode        -O---K   100   100   000    -    0
168 SATA_PHY_Error_Count    -O--C-   100   100   000    -    9
169 Bad_Block_Count         PO--C-   100   100   010    -    100
173 Erase_Count             -O--C-   194   194   000    -    0
175 Program_Fail_Count_Chip PO--C-   100   100   010    -    0
192 Power-Off_Retract_Count -O--C-   100   100   000    -    1047
194 Temperature_Celsius     PO---K   072   056   020    -    28 (Min/Max 10/44)
197 Current_Pending_Sector  -O--C-   100   100   000    -    0
240 Unknown_SSD_Attribute   PO--C-   100   100   050    -    0
                            ||||||_ K auto-keep
                            |||||__ C event count
                            ||||___ R error rate
                            |||____ S speed/performance
                            ||_____ O updated online
                            |______ P prefailure warning

General Purpose Log Directory Version 1
SMART           Log Directory Version 1 [multi-sector log support]
Address    Access  R/W   Size  Description
0x00       GPL,SL  R/O      1  Log Directory
0x01           SL  R/O      1  Summary SMART error log
0x02           SL  R/O     51  Comprehensive SMART error log
0x03       GPL     R/O     64  Ext. Comprehensive SMART error log
0x04       GPL,SL  R/O      8  Device Statistics log
0x06           SL  R/O      1  SMART self-test log
0x07       GPL     R/O      1  Extended self-test log
0x09           SL  R/W      1  Selective self-test log
0x10       GPL     R/O      1  NCQ Command Error log
0x11       GPL     R/O      1  SATA Phy Event Counters log
0x30       GPL,SL  R/O      9  IDENTIFY DEVICE data log
0x80-0x9f  GPL,SL  R/W     16  Host vendor specific log
0xe0       GPL,SL  R/W      1  SCT Command/Status
0xe1       GPL,SL  R/W      1  SCT Data Transfer

SMART Extended Comprehensive Error Log Version: 1 (64 sectors)
Device Error Count: 9
	CR     = Command Register
	FEATR  = Features Register
	COUNT  = Count (was: Sector Count) Register
	LBA_48 = Upper bytes of LBA High/Mid/Low Registers ]  ATA-8
	LH     = LBA High (was: Cylinder High) Register    ]   LBA
	LM     = LBA Mid (was: Cylinder Low) Register      ] Register
	LL     = LBA Low (was: Sector Number) Register     ]
	DV     = Device (was: Device/Head) Register
	DC     = Device Control Register
	ER     = Error register
	ST     = Status register
Powered_Up_Time is measured from power on, and printed as
DDd+hh:mm:SS.sss where DD=days, hh=hours, mm=minutes,
SS=sec, and sss=millisec. It "wraps" after 49.710 days.

Error 9 [8] occurred at disk power-on lifetime: 4263 hours (177 days + 15 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  84 -- 51 00 2e 00 00 01 35 33 12 e0 00  Error: ICRC, ABRT 46 sectors at LBA = 0x01353312 = 20263698

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  25 00 00 00 2e 00 00 01 35 33 12 e0 00     00:01:52.434  READ DMA EXT
  25 00 00 00 12 00 00 01 35 33 00 e0 00     00:01:52.433  READ DMA EXT
  25 00 00 00 2d 00 00 01 35 32 d3 e0 00     00:01:52.433  READ DMA EXT
  25 00 00 00 13 00 00 01 35 32 c0 e0 00     00:01:52.433  READ DMA EXT
  25 00 00 00 2c 00 00 01 35 32 94 e0 00     00:01:52.433  READ DMA EXT

Error 8 [7] occurred at disk power-on lifetime: 1281 hours (53 days + 9 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  84 -- 51 00 60 00 00 00 77 b5 10 40 08  Error: ICRC, ABRT at LBA = 0x0077b510 = 7845136

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 03 48 00 80 00 00 03 1e eb b0 40 08     00:27:23.998  READ FPDMA QUEUED
  60 02 58 00 78 00 00 03 1d 9d e8 40 08     00:27:23.998  READ FPDMA QUEUED
  60 04 18 00 70 00 00 03 1d 99 60 40 08     00:27:23.997  READ FPDMA QUEUED
  60 00 88 00 68 00 00 03 1d 8f 68 40 08     00:27:23.997  READ FPDMA QUEUED
  60 02 40 00 60 00 00 00 77 b5 10 40 08     00:27:23.996  READ FPDMA QUEUED

Error 7 [6] occurred at disk power-on lifetime: 1281 hours (53 days + 9 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  84 -- 51 00 d8 00 00 00 70 cd b8 40 08  Error: ICRC, ABRT at LBA = 0x0070cdb8 = 7392696

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 04 38 00 e0 00 00 00 70 d6 a8 40 08     00:27:23.658  READ FPDMA QUEUED
  60 07 08 00 d8 00 00 00 70 cd b8 40 08     00:27:23.658  READ FPDMA QUEUED
  60 00 f0 00 d0 00 00 03 94 76 80 40 08     00:27:23.658  READ FPDMA QUEUED
  60 00 08 00 c8 00 00 03 51 12 10 40 08     00:27:23.657  READ FPDMA QUEUED
  60 01 98 00 c0 00 00 03 21 13 f8 40 08     00:27:23.657  READ FPDMA QUEUED

Error 6 [5] occurred at disk power-on lifetime: 1281 hours (53 days + 9 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  84 -- 51 00 b0 00 00 03 20 ba 18 40 08  Error: ICRC, ABRT at LBA = 0x0320ba18 = 52476440

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 01 00 00 c8 00 00 00 91 8a 08 40 08     00:27:23.093  READ FPDMA QUEUED
  60 01 00 00 c0 00 00 00 91 16 88 40 08     00:27:23.093  READ FPDMA QUEUED
  60 00 20 00 b8 00 00 03 1f f1 88 40 08     00:27:23.092  READ FPDMA QUEUED
  60 06 c0 00 b0 00 00 03 20 ba 18 40 08     00:27:23.092  READ FPDMA QUEUED
  60 01 00 00 a8 00 00 00 91 89 08 40 08     00:27:23.092  READ FPDMA QUEUED

Error 5 [4] occurred at disk power-on lifetime: 1281 hours (53 days + 9 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  84 -- 51 00 98 00 00 00 92 47 e0 40 08  Error: ICRC, ABRT at LBA = 0x009247e0 = 9586656

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 00 30 00 d8 00 00 03 55 b5 10 40 08     00:27:22.336  READ FPDMA QUEUED
  60 00 08 00 d0 00 00 0c 11 20 58 40 08     00:27:22.334  READ FPDMA QUEUED
  60 00 08 00 c8 00 00 0b 14 58 00 40 08     00:27:22.325  READ FPDMA QUEUED
  60 00 08 00 c0 00 00 0c 91 20 c8 40 08     00:27:22.325  READ FPDMA QUEUED
  60 00 28 00 b8 00 00 03 16 06 d8 40 08     00:27:22.325  READ FPDMA QUEUED

Error 4 [3] occurred at disk power-on lifetime: 1281 hours (53 days + 9 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  84 -- 51 00 c0 00 00 00 84 4a e8 40 08  Error: ICRC, ABRT at LBA = 0x00844ae8 = 8669928

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 01 00 00 c0 00 00 00 84 4a e8 40 08     00:02:45.570  READ FPDMA QUEUED
  60 01 00 00 b8 00 00 00 84 49 e8 40 08     00:02:45.560  READ FPDMA QUEUED
  60 01 00 00 b0 00 00 00 84 48 e8 40 08     00:02:45.551  READ FPDMA QUEUED
  60 00 e8 00 a8 00 00 00 84 48 00 40 08     00:02:45.540  READ FPDMA QUEUED
  60 00 18 00 a0 00 00 00 84 07 e8 40 08     00:02:45.540  READ FPDMA QUEUED

Error 3 [2] occurred at disk power-on lifetime: 1281 hours (53 days + 9 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  84 -- 51 00 00 00 00 00 74 71 c8 40 08  Error: ICRC, ABRT at LBA = 0x007471c8 = 7631304

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 01 00 00 00 00 00 00 74 71 c8 40 08     00:01:40.850  READ FPDMA QUEUED
  60 00 78 00 f0 00 00 03 14 62 d0 40 08     00:01:40.850  READ FPDMA QUEUED
  60 00 88 00 e8 00 00 03 14 60 78 40 08     00:01:40.849  READ FPDMA QUEUED
  60 00 08 00 e0 00 00 0b 55 09 e0 40 08     00:01:40.849  READ FPDMA QUEUED
  60 00 08 00 d8 00 00 07 91 13 60 40 08     00:01:40.849  READ FPDMA QUEUED

Error 2 [1] occurred at disk power-on lifetime: 1281 hours (53 days + 9 hours)
  When the command that caused the error occurred, the device was active or idle.

  After command completion occurred, registers were:
  ER -- ST COUNT  LBA_48  LH LM LL DV DC
  -- -- -- == -- == == == -- -- -- -- --
  84 -- 51 00 c0 00 00 03 1f 95 d0 40 08  Error: ICRC, ABRT at LBA = 0x031f95d0 = 52401616

  Commands leading to the command that caused the error were:
  CR FEATR COUNT  LBA_48  LH LM LL DV DC  Powered_Up_Time  Command/Feature_Name
  -- == -- == -- == == == -- -- -- -- --  ---------------  --------------------
  60 01 00 00 c0 00 00 03 1f 95 d0 40 08     00:00:27.209  READ FPDMA QUEUED
  60 00 20 00 b8 00 00 03 20 07 a0 40 08     00:00:27.209  READ FPDMA QUEUED
  60 00 18 00 b0 00 00 03 1d 27 20 40 08     00:00:27.208  READ FPDMA QUEUED
  60 00 70 00 a8 00 00 03 1c f5 08 40 08     00:00:27.208  READ FPDMA QUEUED
  60 01 00 00 a0 00 00 03 1c f4 08 40 08     00:00:27.207  READ FPDMA QUEUED

SMART Extended Self-test Log Version: 1 (1 sectors)
Num  Test_Description    Status                  Remaining  LifeTime(hours)  LBA_of_first_error
# 1  Extended offline    Completed without error       00%      2045         -

SMART Selective self-test log data structure revision number 1
 SPAN  MIN_LBA  MAX_LBA  CURRENT_TEST_STATUS
    1        0        0  Not_testing
    2        0        0  Not_testing
    3        0        0  Not_testing
    4        0        0  Not_testing
    5        0        0  Not_testing
Selective self-test flags (0x0):
  After scanning selected spans, do NOT read-scan remainder of disk.
If Selective self-test is pending on power-up, resume after 0 minute delay.

SCT Status Version:                  3
SCT Version (vendor specific):       3 (0x0003)
Device State:                        Active (0)
Current Temperature:                    28 Celsius
Power Cycle Min/Max Temperature:     24/28 Celsius
Lifetime    Min/Max Temperature:     10/44 Celsius
Under/Over Temperature Limit Count:   0/0
Vendor specific:
00 00 04 00 05 01 00 05 05 00 00 00 00 00 00 00
00 02 00 00 ee 99 ea 00 02 02 00 00 00 00 00 06

SCT Temperature History Version:     2
Temperature Sampling Period:         1 minute
Temperature Logging Interval:        1 minute
Min/Max recommended Temperature:      5/40 Celsius
Min/Max Temperature Limit:            0/80 Celsius
Temperature History Size (Index):    128 (10)

SCT Error Recovery Control:
           Read:    600 (60.0 seconds)
          Write:    600 (60.0 seconds)

Device Statistics (GP Log 0x04)
Page  Offset Size        Value Flags Description
0x01  =====  =               =  ===  == General Statistics (rev 2) ==
0x01  0x008  4            2441  ---  Lifetime Power-On Resets
0x01  0x018  6     12725674345  ---  Logical Sectors Written
0x01  0x020  6       195092366  ---  Number of Write Commands
0x01  0x028  6     10895510889  ---  Logical Sectors Read
0x01  0x030  6       178680733  ---  Number of Read Commands
0x04  =====  =               =  ===  == General Errors Statistics (rev 1) ==
0x04  0x008  4               0  ---  Number of Reported Uncorrectable Errors
0x04  0x010  4               0  ---  Resets Between Cmd Acceptance and Completion
0x05  =====  =               =  ===  == Temperature Statistics (rev 1) ==
0x05  0x008  1              28  ---  Current Temperature
0x05  0x010  1              29  ---  Average Short Term Temperature
0x05  0x018  1              24  ---  Average Long Term Temperature
0x05  0x020  1              44  ---  Highest Temperature
0x05  0x028  1              12  ---  Lowest Temperature
0x05  0x030  1              37  ---  Highest Average Short Term Temperature
0x05  0x038  1              14  ---  Lowest Average Short Term Temperature
0x05  0x040  1              31  ---  Highest Average Long Term Temperature
0x05  0x048  1              18  ---  Lowest Average Long Term Temperature
0x05  0x050  4            2170  ---  Time in Over-Temperature
0x05  0x058  1              40  ---  Specified Maximum Operating Temperature
0x05  0x060  4               0  ---  Time in Under-Temperature
0x05  0x068  1               5  ---  Specified Minimum Operating Temperature
0x06  =====  =               =  ===  == Transport Statistics (rev 1) ==
0x06  0x008  4            4463  ---  Number of Hardware Resets
0x06  0x018  4               9  ---  Number of Interface CRC Errors
0x07  =====  =               =  ===  == Solid State Device Statistics (rev 1) ==
0x07  0x008  1               6  N--  Percentage Used Endurance Indicator
                                |||_ C monitored condition met
                                ||__ D supports DSN
                                |___ N normalized value

Pending Defects log (GP Log 0x0c) not supported

SATA Phy Event Counters (GP Log 0x11)
ID      Size     Value  Description
0x0001  2            0  Command failed due to ICRC error
0x0002  4            0  R_ERR response for data FIS
0x0003  2            0  R_ERR response for device-to-host data FIS
0x0004  2            0  R_ERR response for host-to-device data FIS
0x0005  4            0  R_ERR response for non-data FIS
0x0006  2            0  R_ERR response for device-to-host non-data FIS
0x0007  2            0  R_ERR response for host-to-device non-data FIS
0x0008  2            0  Device-to-host non-data FIS retries
0x0009  4            6  Transition from drive PhyRdy to drive PhyNRdy
0x000a  4            7  Device-to-host register FISes sent due to a COMRESET
0x000b  4            0  CRC errors within host-to-device FIS
0x000d  4            0  Non-CRC errors within host-to-device FIS
0x000f  2            0  R_ERR response for host-to-device data FIS, CRC
0x0010  2            0  R_ERR response for host-to-device data FIS, non-CRC
0x0012  2            0  R_ERR response for host-to-device non-data FIS, CRC
0x0013  2            0  R_ERR response for host-to-device non-data FIS, non-CRC

