OCZ Solid State Drives
======================

This is a list of all tested OCZ solid state drive models and their MTBFs. See
more info on reliability test in the [README](https://github.com/bsdhw/SMART).

Contents
--------

1. [ SSD by Model  ](#ssd-by-model)
2. [ SSD by Family ](#ssd-by-family)

SSD by Model
------------

Please take all columns into account when reading the table. Pay attention on the
number of tested samples and power-on days. Simultaneous high values of both MTBF
and errors are possible if only rare drives in the subset encounter errors.

Days - avg. days per sample,
Err  - avg. errors per sample,
MTBF - avg. MTBF in years per sample.

| MFG       | Model              | Size   | Samples | Days  | Err   | MTBF |
|-----------|--------------------|--------|---------|-------|-------|------|
| OCZ       | VERTEX2            | 64 GB  | 1       | 3103  | 0     | 8.50   |
| OCZ       | VERTEX3 MI         | 240 GB | 1       | 2552  | 0     | 6.99   |
| OCZ       | AGILITY            | 32 GB  | 2       | 2269  | 0     | 6.22   |
| OCZ       | VECTOR             | 256 GB | 1       | 2265  | 0     | 6.21   |
| OCZ       | SOLID3             | 120 GB | 1       | 2144  | 0     | 5.87   |
| OCZ       | VERTEX PLUS R2     | 64 GB  | 1       | 2045  | 0     | 5.60   |
| OCZ       | VERTEX PLUS        | 64 GB  | 1       | 1901  | 0     | 5.21   |
| OCZ       | AGILITY4           | 256 GB | 1       | 1775  | 0     | 4.87   |
| OCZ       | VERTEX4            | 256 GB | 3       | 1639  | 0     | 4.49   |
| OCZ       | VERTEX3 MI         | 120 GB | 2       | 2104  | 1     | 3.97   |
| OCZ       | AGILITY3           | 120 GB | 8       | 1466  | 151   | 3.93   |
| OCZ       | AGILITY3           | 128 GB | 1       | 1233  | 0     | 3.38   |
| OCZ       | VERTEX3            | 64 GB  | 4       | 1591  | 8     | 2.96   |
| OCZ       | VERTEX4            | 128 GB | 5       | 1130  | 1     | 2.61   |
| OCZ       | VERTEX3            | 90 GB  | 1       | 2678  | 2     | 2.45   |
| OCZ       | AGILITY3           | 64 GB  | 6       | 1028  | 1     | 2.36   |
| OCZ       | VERTEX3            | 120 GB | 8       | 1218  | 21    | 2.09   |
| OCZ       | ARC100             | 240 GB | 3       | 726   | 0     | 1.99   |
| OCZ       | VERTEX460A         | 120 GB | 2       | 634   | 0     | 1.74   |
| OCZ       | VERTEX3            | 240 GB | 2       | 1232  | 511   | 1.48   |
| OCZ       | VERTEX2 3.5        | 120 GB | 1       | 472   | 0     | 1.30   |
| OCZ       | VERTEX2            | 120 GB | 2       | 455   | 0     | 1.25   |
| OCZ       | VERTEX2 3.5        | 240 GB | 1       | 413   | 0     | 1.13   |
| OCZ       | VECTOR150          | 120 GB | 1       | 758   | 1     | 1.04   |
| OCZ       | TRION150           | 480 GB | 1       | 373   | 0     | 1.02   |
| OCZ       | TRION100           | 240 GB | 2       | 365   | 0     | 1.00   |
| OCZ       | TRION150           | 240 GB | 2       | 338   | 0     | 0.93   |
| OCZ       | AGILITY4           | 128 GB | 3       | 314   | 1     | 0.78   |
| OCZ       | ARC100             | 120 GB | 1       | 279   | 0     | 0.77   |
| OCZ       | VERTEX4            | 64 GB  | 1       | 206   | 0     | 0.57   |
| OCZ       | VERTEX3            | 128 GB | 1       | 184   | 0     | 0.50   |
| OCZ       | AGILITY3           | 240 GB | 2       | 893   | 7     | 0.45   |
| OCZ       | VERTEX             | 32 GB  | 1       | 243   | 1     | 0.33   |
| OCZ       | PETROL             | 256 GB | 1       | 100   | 0     | 0.28   |
| OCZ       | VERTEX2            | 80 GB  | 1       | 50    | 0     | 0.14   |
| OCZ       | VERTEX2            | 55 GB  | 1       | 50    | 0     | 0.14   |
| OCZ       | VERTEX-TURBO       | 32 GB  | 2       | 298   | 56    | 0.09   |
| OCZ       | VECTOR150          | 240 GB | 1       | 603   | 18    | 0.09   |
| OCZ       | AGILITY2           | 64 GB  | 1       | 1220  | 1006  | 0.00   |
| OCZ       | TRION100           | 120 GB | 1       | 1     | 0     | 0.00   |

SSD by Family
-------------

Please take all columns into account when reading the table. Pay attention on the
number of tested samples and power-on days. Simultaneous high values of both MTBF
and errors are possible if only rare drives in the subset encounter errors.

Days - avg. days per sample,
Err  - avg. errors per sample,
MTBF - avg. MTBF in years per sample.

| MFG       | Family                 | Models | Samples | Days  | Err   | MTBF |
|-----------|------------------------|--------|---------|-------|-------|------|
| OCZ       | Indilinx Barefoot_2... | 8      | 16      | 1096  | 1     | 2.84   |
| OCZ       | SandForce Driven SSDs  | 19     | 45      | 1277  | 77    | 2.64   |
| OCZ       | Indilinx Barefoot b... | 3      | 5       | 1076  | 23    | 2.59   |
| OCZ       | Indilinx Barefoot 3... | 6      | 9       | 817   | 3     | 1.95   |
| OCZ       | OCZ/Toshiba Trion SSDs | 4      | 6       | 296   | 0     | 0.81   |
