Fujitsu Hard Drives
===================

This is a list of all tested Fujitsu hard drive models and their MTBFs. See more
info on reliability test in the [README](https://github.com/bsdhw/SMART).

Contents
--------

1. [ HDD by Model  ](#hdd-by-model)
2. [ HDD by Family ](#hdd-by-family)

HDD by Model
------------

Please take all columns into account when reading the table. Pay attention on the
number of tested samples and power-on days. Simultaneous high values of both MTBF
and errors are possible if only rare drives in the subset encounter errors.

Days - avg. days per sample,
Err  - avg. errors per sample,
MTBF - avg. MTBF in years per sample.

| MFG       | Model              | Size   | Samples | Days  | Err   | MTBF |
|-----------|--------------------|--------|---------|-------|-------|------|
| Fujitsu   | MHW2120BH          | 120 GB | 2       | 945   | 0     | 2.59   |
| Fujitsu   | MHZ2250BJ FFS G2   | 250 GB | 1       | 711   | 0     | 1.95   |
| Fujitsu   | MJA2160BH FFS G1   | 160 GB | 1       | 707   | 0     | 1.94   |
| Fujitsu   | MHT2080BH          | 80 GB  | 1       | 584   | 0     | 1.60   |
| Fujitsu   | MHV2100BH PL       | 100 GB | 1       | 553   | 0     | 1.52   |
| Fujitsu   | MJA2160BH G2       | 160 GB | 2       | 537   | 0     | 1.47   |
| Fujitsu   | MHY2120BH          | 120 GB | 2       | 456   | 0     | 1.25   |
| Fujitsu   | MHT2080AH          | 80 GB  | 1       | 427   | 0     | 1.17   |
| Fujitsu   | MJA2320BH G2       | 320 GB | 2       | 416   | 0     | 1.14   |
| Fujitsu   | MHY2200BH          | 200 GB | 2       | 412   | 0     | 1.13   |
| Fujitsu   | MHZ2120BH G2       | 120 GB | 1       | 374   | 0     | 1.03   |
| Fujitsu   | MJA2250BH FFS G1   | 250 GB | 1       | 302   | 0     | 0.83   |
| Fujitsu   | MHY2250BH          | 250 GB | 1       | 253   | 0     | 0.69   |
| Fujitsu   | MHY2160BH          | 160 GB | 1       | 206   | 0     | 0.57   |
| Fujitsu   | MHZ2320BH FFS G1   | 320 GB | 1       | 203   | 0     | 0.56   |
| Fujitsu   | MJA2250BH G2       | 250 GB | 1       | 161   | 0     | 0.44   |
| Fujitsu   | MHZ2250BH G1       | 250 GB | 1       | 673   | 9     | 0.18   |
| Fujitsu   | MHZ2160BH G2       | 160 GB | 1       | 721   | 14    | 0.13   |
| Fujitsu   | MHS2040AT D        | 40 GB  | 1       | 1337  | 37    | 0.10   |
| Fujitsu   | MHZ2160BH FFS G1   | 160 GB | 1       | 380   | 200   | 0.01   |
| Fujitsu   | MHW2160BH          | 160 GB | 1       | 475   | 957   | 0.00   |
| Fujitsu   | MHZ2250BH G2       | 250 GB | 1       | 148   | 1026  | 0.00   |
| Fujitsu   | MHV2120BH PL       | 120 GB | 1       | 0     | 0     | 0.00   |

HDD by Family
-------------

Please take all columns into account when reading the table. Pay attention on the
number of tested samples and power-on days. Simultaneous high values of both MTBF
and errors are possible if only rare drives in the subset encounter errors.

Days - avg. days per sample,
Err  - avg. errors per sample,
MTBF - avg. MTBF in years per sample.

| MFG       | Family                 | Models | Samples | Days  | Err   | MTBF |
|-----------|------------------------|--------|---------|-------|-------|------|
| Fujitsu   | MHZ BJ                 | 1      | 1       | 711   | 0     | 1.95   |
| Fujitsu   | MHW BH                 | 2      | 3       | 788   | 319   | 1.73   |
| Fujitsu   | MHT                    | 2      | 2       | 506   | 0     | 1.39   |
| Fujitsu   | MJA BH                 | 5      | 7       | 439   | 0     | 1.20   |
| Fujitsu   | MHY BH                 | 4      | 6       | 366   | 0     | 1.00   |
| Fujitsu   | MHV                    | 2      | 2       | 276   | 0     | 0.76   |
| Fujitsu   | MHZ BH                 | 6      | 6       | 416   | 209   | 0.32   |
| Fujitsu   | MHS AT                 | 1      | 1       | 1337  | 37    | 0.10   |
